
                 D-Link DFE-530TX PCI Fast Ethernet Adapter

 Contents
 --------

    - Introduction
    - Getting Started
    - Revision History
    - Trouble shooting
    - Support Options
    - Copyrights and Trademarks

 Introduction
 ------------
    
    Thank you for purchasing the D-Link DFE-530TX PCI Fast Ethernet adapter.
    This CD-R driver support for the D-Link DFE-530TX PCI Fast Ethernet adapter
    (support 10M/100M PCI).
    
    This driver contains many kinds of Network Operating System 
    installation .  Please refer to the readme file or user's guide
    if any problems for installation, or please freely contact 
    our technical support.

    You can get latest releases of drivers from D-Link's Web site 
    (http://www.dlink.com). We hope our new readmes and installations
    will minimize the users effort to make our products work. Should there
    be further recommendations please contact the support manager at the
    local D-Link Office listed bellow.

 Getting Started
 ---------------

    Auto-run program assist your ease of setup.  It will configure
    driver, install appropriate network drivers for popular network
    operating systems on the DFE-530TX adapter.


    You can operate some function through the friendly button:

    1.Install Driver: It will configure driver, install appropriate 
      network drivers for popular network operating systems on the
      DFE-530TX adapter.

    2.View Quick Installation Guide: It will show Quick Installation Guide 
      for your reference.

    3.View manual: It will show detail manual for your reference.

    4.Install Adobe Acrobat Reader: The QIG and Manual are in Adobe .PDF format.
      If you do not have a .PDF viewer install on your system, install Adobe Acrobat 
      Reader to view these file. 
    
    5.Visit support.dlink.com: Please see the detail of our local branch office and
      contact our customer service window.

    6.Exit: You can exit Window by this button.
     
    If the NOS (Network Operating System) you are using is not covered
    by the auto-run program, please refer to the individual documentation
    provided in INFO directory.


 Revisions History
 -----------------

    Diskette revision: 20120217
    ---------------------------
    -- add support Macintosh driver MAC OS X 10.7.x 32bit/64bit
    -- Update Linux driver ver:5.21 (support Linux kernel 2:6.37)

    Diskette revision: 20100301
    ---------------------------
    -- Add Windows 7 X86/X64 driver
    -- Add Windows Server 2008 R2 X64 driver

    Diskette revision: 20070601
    ---------------------------
     -- Update Macintosh driver
     -- Update Packet driver
     -- Update Netware 5.x/6.x
     -- Update ODI.DOS driver
     -- Update Linux driver
     -- Update Diagnostic Program for Windows 
     -- Update Windows 2K/2003/XP Driver 
     -- Add Windows Vista x86/Vista x64/2003 x64/XP x64 Driver   

    Diskette revision: 20031001
    ---------------------------- 
    -- Support MAC Driver (Ver 10.02 and later). 

    Diskette revision: 20030701
    ---------------------------- 
    -- Support Windows Server 2003. 
    -- Support NetWare 6.5.
    -- Update all drivers.

    Diskette revision: 20030101
    ---------------------------- 
    -- Support 802.1x supplicant.
    -- Support Win Diagnostic,DOS Diagnostic.
    -- Add INFO directory.
    -- Windows 98/ME/2000/XP passed PC99 logo certification.

    Diskette revision: 20020701
    ---------------------------- 
    -- Support DFE-530TX A1/A3/B1/B2/C1 adapters. 

    -- It supports the following drivers:
      --Novell NetWare 3.x, 4.x,5.x,6.x and ODI.DOS.
      --Microsoft Windows NT3.51, NT4.0.
      --Windows 95/95OSR2, 98/98SE/Me,2000/XP.
      --Microsoft Windows for Workgroups 3.11.
      --Microsoft Client for DOS.
      --IBM LAN Support Program v1.3x.
      --FTP PC/TCP.
      --SUN PC-NFS.
      --NDIS 2.x, 3.x, 4.x, 5.x Driver.
      --Packet Driver.
      --Linux Driver. 
    -- Win Diagnostic, SCO OpenServer 5.0, and UnixWare 7.x will be support on
       D-Link Web in the Future. 

    Diskette revision: 20020201
    ---------------------------
    --Add auto-run program.

    Diskette revision: 20011015
    ---------------------------
    -- Update inf file and Windows 98/2000/NT40/ME passed PC99 logo
       certification.

    Diskette revision: 20000615
    ---------------------------
    -- Support DFE-530TX A1/A3/B1 adapters.
    -- Fixed reading of null Mac address when soft-rebooting PC after 
       Windows 98 shutdown.

    Diskette revision: 20000301
    ---------------------------
    -- Flow control function update.
    
    Diskette revision: 20000201
    ---------------------------
    -- Support DFE-530TX A1 and B1
    -- Support WOL, Flow control (DFE-530TX B1 hardware only)

    Diskette revision: 991215
    -------------------------
    -- Support Windows 2000 driver. 
    
    Diskette revision: 990615
    -------------------------
    -- Add NDIS5 drivers for Win98 root file
    -- Win95A/Osr2/Win98 use NDIS3 driver 
       and the same INF file in the root path.

    Diskette revision: 981115
    -------------------------
    --Update NDIS3 and NDIS4 drivers.
    --Update Packet driver.

    Diskette revision: 980915
    -------------------------
    --To update NetWare server driver. 
  
    Diskette revision: 980815
    -------------------------
     --Supports NetWare5.0 driver.
     --To solve "Windows Protection Error" problem.     

    Diskette revision: 980601
    --------------------------
      To solve NEC NX compatible issue under NDIS3 and  NDIS4 drivers.

    Diskette revision: 980515
    -------------------------
      To update Novell NetWare server, NDIS2 and Packet drivers.

    Diskette revision: 980501
    -------------------------
      It supports drivers as the following list.
      --Installation program.
      --Diagnostics program.
      --Novell NetWare 3.12, 4.x, ODI.DOS.
      --Microsoft Windows NT3.51, NT4.0.
      --Windows 95, 98.
      --Microsoft Windows for Workgroups 3.11.
      --IBM LAN Support Program v1.3x.
      --DECnet PathWorks v4.0.
      --Banyan VINES v4.00(2).
      --WIN/TCP PathWay Access for DOS v1.1.
      --FTP PC/TCP.
      --SUN PC-NFS.
      --SCO OpenServer 5.0.
      --NDIS 2.x, 3.x, 4.x Driver.
      --Packet Driver.

    Diskette revision : 980315
    --------------------------
      It supports drivers as the following list.
      --Novell NetWare 3.12, 4.x, ODI.DOS.
      --Microsoft Windows NT3.51, NT4.0.
      --Windows 95, 98.


 Trouble shooting
 ----------------
 During testing of the WOL feature of the DFE-530TX.B1, if you discover  
 the following phenomena:

 1) In WIN98(SE) or WIN2000, if the user turns the Stand By using the normal 
    procedure, then the card can be remote awakened successfully.

 2) If the DFE-530TX.B1 encounters either of the following power-off 
    situations: 
    (a) sudden, abnormal power-down, or (b) PC freezes suddenly, then the WOL
    function fails.
    
    For the second situation, there are two workarounds to re-enable the 
    WOL function:
  
    1. Restart the PC ->
       The PC will scan the harddisk and file system automatically ->
       After the OS is rebooted successfully, turn the Stand By using 
       the normal procedure.

    2. Restart the PC ->
       Enter DOS mode immediately ->
       Use the Setup utility ( please contact with the local D-Link's OBU )
       to re-enable the WOL function.



 Support Options
 ---------------

    For technical support, you may contact your authorized D-Link
    distributor, dealer or the following D-Link branch offices.
    

    D-Link Australia
    1 Giffnock Avenue
    North Ryde, NSW 2113
    Australia
    TEL: 61-2-8899-1800
    FAX: 61-2-8899-1868
    URL: www.dlink.com.au


    D-Link Canada
    2180 Winston Park Drive 
    Oakville, Ontario, L6H 5W1
    Canada
    TEL: 1-905-8295033
    FAX: 1-905-8295223
    URL: www.dlink.ca


    D-Link LatinAmerica
    Av. Vitacura # 2939, floor 6th
    Las Condes, Santiago. RM
    Chile
    TEL: 56-2-5838-950
    FAX: 56-2-5838-952
    URL: www.dlinkla.com


    D-Link Denmark 
    Naverland 2, DK-2600
    GGlostrup, Copenhagen
    Denmark
    TEL: 45-43-969040
    FAX: 45-43-424347
    URL: www.dlink.dk


    D-Link Middle East (Dubai)
    P.O.Box: 500376
    Office: 103, Building:3
    Dubai Internet City
    Dubai, United Arab Emirates
    TEL: +971-4-3916480
    FAX: +971-4-3908881
    URL: www.dlink-me.com


    D-Link France
    41 boulevard Vauban
    78280 Guyancourt
    France
    TEL: 33-1-30238688
    FAX: 33-1-30238689
    URL: www.dlink.fr


    D-Link Germany
    Schwalbacher Strasse 74
    D-65760 Eschborn
    Germany
    TEL: 49-6196-77990
    FAX: 49-6196-7799300
    URL: www.dlink.de


    D-Link India
    D-Link House, Plot No.5,
    Kurla-Bandra Complex Road, Off. CST Road,
    Santacruz (E), Mumbai - 400 098 India
    TEL: 91-22-26526696/30616666
    FAX: 91-22-26528914/8476
    URL: www.dlink.co.in


    D-Link Italy
    Via Nino Bonnet n. 6/b
    20154 ¡V Milano
    Italy
    TEL: 39-02-2900-0676
    FAX: 39-02-2900-1723
    URL: www.dlink.it


    D-Link Japan K.K.
    Level 6 Konan YK Building, Konan 2-4-12
    Minato-Ku Tokyo 108-0075, Japan 


    D-Link Russia 
    Grafsky per., 14, floor 6
    Moscow 
    129626 Russia
    TEL: 7-495-744-0099
    FAX: 7-495-744-0099 #350
    URL: www.dlink.ru


    D-Link Singapore
    1 International Business Park
    #03-12 The Synergy 
    Singapore 609917
    TEL: 65-6774-6233
    FAX: 65-6774-6322
    URL: www.dlink-intl.com 
    FAX: 65-774-6322
    URL: www.dlink-intl.com   


    D-Link South Africa
    Einstein Park II
    Block B
    102-106 Witch-Hazel Avenue
    First Floor Block B
    Einstein Park II
    Highveld Techno Park
    Centurion
    Gauteng
    Republic of South Africa
    TEL: 27-12-665-2165
    FAX: 27-12-665-2186
    URL: www.d-link.co.za


    D-Link Sweden
    P.O. Box 15036, S-167 15 Bromma
    Sweden
    TEL: 46-(0)8564-61900
    FAX: 46-(0)8564-61901
    URL: www.dlink.se


    D-Link Taiwan
    No. 289 , Sinhu 3rd Rd., Neihu District , 
    Taipei City 114 ,Taiwan
    TEL: 886-2-6600-0123
    FAX: 886-2-6600-1188
    URL: www.dlinktw.com.tw


    D-Link European HQ & UK & I
    D-Link House, Abbey Road,
    Park Royal, London,
    NW10 7BX, UK
    TEL: +44-20-8955-9000
    FAX: +44-20-8955-9003
    URL:www.dlink.eu
    URL: www.dlink.co.uk


    D-Link U.S.A
    17595 Mt. Herrmann Street 
    Fountain Valley, CA 92708
    U.S.A.
    TEL: 1 1-800-326-1688
    URL: www.dlink.com

                      
 
    The BBS communication setup information is as follows :

    Speed     :  2400-14400  baud                           - Germany
                 2400-9600   baud                           - Asia,Taiwan
                 14400-16800 baud                           - Canada
                 9600-14400  baud V32, V32bis, V42, V42bis  - U.S.A.
                 2400-19200  baud V24, V32, V32bis, V42bis  - U.K. & Europe
    Parity    : none
    Data bits : 8
    Stop bit  : 1

 Copyrights, Trademarks
 ======================
    All documents and software provided herewith are Copyright (c)2002
    D-Link Corporation. All rights reserved.

    Windows 95/95OSR2, 98/98SE/Me,2000/XP/Server 2003/Vista, NT 4.0 are trade 
    names of Microsoft Corporation.

    Other trademarks or trade names used herein are properties of the
    respective owners.

