



          -- Request for Comments: Draft             cisco Systems, Inc.


                                  -- cisco MIB*

                           -- Wed Apr  8 14:37:15 1992


                              -- cisco Systems, Inc.
                                 -- 1525 O'Brien
                             -- Menlo Park, CA  94025

                          -- customer-service@cisco.com



          -- 1. Introduction

          -- This memo describes the variables that are implemented for
          -- the cisco Systems, Inc.  set of products including the
          -- Gateway Server, Terminal Server, Trouter, and Protocol
          -- Translator.  The document relies upon the Structure of
          -- Management Information (SMI), RFC1155.  It is presented in
          -- a format described in RFC1212, the Concise MIB document.

          -- This  document describes the cisco local Management
          -- Information Base (MIB) variables for
          -- version 8.3 of the system software.


          -- 2. Object Definitions

               -- CISCO-MIB { iso org(3) dod(6) internet(1) private(4)
                                       -- enterprises(1) 9 }

               CISCO-MIB DEFINITIONS ::= BEGIN

               IMPORTS
                    enterprises, OBJECT-TYPE, NetworkAddress, IpAddress,
                    Counter, Gauge, TimeTicks
                    FROM RFC1155-SMI
                    ifIndex, ipAdEntAddr, ipRouteDest, tcpConnLocalAddress,
                    tcpConnLocalPort, tcpConnRemAddress, tcpConnRemPort
                    FROM RFC1213-MIB;

          
             -- *This file is machine generated. Do not edit.






          -- cisco MIB                                          [Page 1]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               cisco               OBJECT IDENTIFIER ::= { enterprises 9 }

               products            OBJECT IDENTIFIER ::= { cisco 1 }
               local               OBJECT IDENTIFIER ::= { cisco 2 }
               temporary           OBJECT IDENTIFIER ::= { cisco 3 }

               gateway-server      OBJECT IDENTIFIER ::= { products 1 }
               terminal-server     OBJECT IDENTIFIER ::= { products 2 }
               trouter             OBJECT IDENTIFIER ::= { products 3 }
               protocol-translator OBJECT IDENTIFIER ::= { products 4 }
               igs                 OBJECT IDENTIFIER ::= { products 5 }

               lsystem             OBJECT IDENTIFIER ::= { local 1 }
               linterfaces         OBJECT IDENTIFIER ::= { local 2 }
               lat                 OBJECT IDENTIFIER ::= { local 3 }
               lip                 OBJECT IDENTIFIER ::= { local 4 }
               licmp               OBJECT IDENTIFIER ::= { local 5 }
               ltcp                OBJECT IDENTIFIER ::= { local 6 }
               ludp                OBJECT IDENTIFIER ::= { local 7 }
               legp                OBJECT IDENTIFIER ::= { local 8 }
               lts                 OBJECT IDENTIFIER ::= { local 9 }

               decnet              OBJECT IDENTIFIER ::= { temporary 1 }
               xns                 OBJECT IDENTIFIER ::= { temporary 2 }
               appletalk           OBJECT IDENTIFIER ::= { temporary 3 }
               novell              OBJECT IDENTIFIER ::= { temporary 4 }
               vines               OBJECT IDENTIFIER ::= { temporary 5 }



          -- Product Section

          -- The product section contains the different product's
          -- object identifiers.  Each product has a unique object
          -- identifier allocated from this section which is referenced
          -- by the sysObjectID variable from RFC1156.

               -- gateway-server      OBJECT IDENTIFIER ::= { products 1 }
               -- terminal-server     OBJECT IDENTIFIER ::= { products 2 }
               -- trouter             OBJECT IDENTIFIER ::= { products 3 }
               -- protocol-translator OBJECT IDENTIFIER ::= { products 4 }
               -- igs                 OBJECT IDENTIFIER ::= { products 5 }

          -- New products will be added at the end of this list.






          -- cisco MIB                                          [Page 2]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


          -- Local Variable Section

          -- This section describes the local variables within the cisco
          -- product line.  Groups may or may not be present depending
          -- on the software options present in the managed device.


          -- Local System Group

          -- This group is present in all products.

               romId OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "This variable contains a printable octet
                           string which contains the System Bootstrap
                           description and version identification."
                   ::= { lsystem 1 }

               whyReload OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "This variable contains a printable octet
                           string which contains the reason why the
                           system was last restarted."
                   ::= { lsystem 2 }

               hostName OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "This variable represents the name of the
                           host."
                   ::= { lsystem 3 }

               domainName OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION





          -- cisco MIB                                          [Page 3]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           "This variable is the domain portion of the
                           domain name of the host."
                   ::= { lsystem 4 }

               authAddr OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "This variable contains the last SNMP
                           authorization failure IP address."
                   ::= { lsystem 5 }

               bootHost OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the IP address of the host that
                           supplied the currently running software."
                   ::= { lsystem 6 }

               ping OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "Supplies a way to ping a host from this
                           entity. The ping variable takes the following
                           instance identifiers: 1 - IP protocol ping.
                           IP - address to ping. integer - count of
                           packets to send. integer - size of ping
                           packet. integer - timeout delay between
                           packets."
                   ::= { lsystem 7 }

               freeMem OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Return the amount of free memory in bytes."
                   ::= { lsystem 8 }

               bufferElFree OBJECT-TYPE





          -- cisco MIB                                          [Page 4]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of free buffer
                           elements."
                   ::= { lsystem 9 }

               bufferElMax OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the maximum number of buffer
                           elements."
                   ::= { lsystem 10 }

               bufferElHit OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of buffer element hits."
                   ::= { lsystem 11 }

               bufferElMiss OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of buffer element
                           misses."
                   ::= { lsystem 12 }

               bufferElCreate OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of buffer element
                           creates."
                   ::= { lsystem 13 }

               bufferSmSize OBJECT-TYPE
                   SYNTAX  INTEGER





          -- cisco MIB                                          [Page 5]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the size of small buffers."
                   ::= { lsystem 14 }

               bufferSmTotal OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the total number of small buffers."
                   ::= { lsystem 15 }

               bufferSmFree OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of free small buffers."
                   ::= { lsystem 16 }

               bufferSmMax OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the maximum number of small
                           buffers."
                   ::= { lsystem 17 }

               bufferSmHit OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of small buffer hits."
                   ::= { lsystem 18 }

               bufferSmMiss OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of small buffer misses."





          -- cisco MIB                                          [Page 6]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ::= { lsystem 19 }

               bufferSmTrim OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of small buffer trims."
                   ::= { lsystem 20 }

               bufferSmCreate OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of small buffer
                           creates."
                   ::= { lsystem 21 }

               bufferMdSize OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the size of medium buffers."
                   ::= { lsystem 22 }

               bufferMdTotal OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the total number of medium
                           buffers."
                   ::= { lsystem 23 }

               bufferMdFree OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of free medium buffers."
                   ::= { lsystem 24 }

               bufferMdMax OBJECT-TYPE





          -- cisco MIB                                          [Page 7]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the maximum number of medium
                           buffers."
                   ::= { lsystem 25 }

               bufferMdHit OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of medium buffer hits."
                   ::= { lsystem 26 }

               bufferMdMiss OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of medium buffer
                           misses."
                   ::= { lsystem 27 }

               bufferMdTrim OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of medium buffer trims."
                   ::= { lsystem 28 }

               bufferMdCreate OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of medium buffer
                           creates."
                   ::= { lsystem 29 }

               bufferBgSize OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only





          -- cisco MIB                                          [Page 8]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the size of big buffers."
                   ::= { lsystem 30 }

               bufferBgTotal OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the total number of big buffers."
                   ::= { lsystem 31 }

               bufferBgFree OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of free big buffers."
                   ::= { lsystem 32 }

               bufferBgMax OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the maximum number of big buffers."
                   ::= { lsystem 33 }

               bufferBgHit OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of big buffer hits."
                   ::= { lsystem 34 }

               bufferBgMiss OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of big buffer misses."
                   ::= { lsystem 35 }






          -- cisco MIB                                          [Page 9]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               bufferBgTrim OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of big buffer trims."
                   ::= { lsystem 36 }

               bufferBgCreate OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of big buffer creates."
                   ::= { lsystem 37 }

               bufferLgSize OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the size of large buffers."
                   ::= { lsystem 38 }

               bufferLgTotal OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the total number of large buffers."
                   ::= { lsystem 39 }

               bufferLgFree OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of free large buffers."
                   ::= { lsystem 40 }

               bufferLgMax OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION





          -- cisco MIB                                         [Page 10]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           "Contains the maximum number of large
                           buffers."
                   ::= { lsystem 41 }

               bufferLgHit OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of large buffer hits."
                   ::= { lsystem 42 }

               bufferLgMiss OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of large buffer misses."
                   ::= { lsystem 43 }

               bufferLgTrim OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of large buffer trims."
                   ::= { lsystem 44 }

               bufferLgCreate OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of large buffer
                           creates."
                   ::= { lsystem 45 }

               bufferFail OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Count of the number of buffer allocation
                           failures."
                   ::= { lsystem 46 }





          -- cisco MIB                                         [Page 11]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               bufferNoMem OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Count of the number of buffer create
                           failures due to no free memory."
                   ::= { lsystem 47 }

               netConfigIP OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Holds the IP address of the host that
                           supplied the network-confg file."
                   ::= { lsystem 48 }

               netConfigName OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Holds the name of the network configuration
                           file."
                   ::= { lsystem 49 }

               netConfigSet OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  write-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Permit the loading of a new network-confg
                           file using TFTP."
                   ::= { lsystem 50 }

               hostConfigIP OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the IP address of the host that
                           provided the host-config file."
                   ::= { lsystem 51 }






          -- cisco MIB                                         [Page 12]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               hostConfigName OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the name of the last configured
                           host-confg file."
                   ::= { lsystem 52 }

               hostConfigSet OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  write-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Permit the loading of a new host-confg file
                           using TFTP."
                   ::= { lsystem 53 }

               writeMem OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  write-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Write configuration into non-volatile memory
                           / erase config memory if 0"
                   ::= { lsystem 54 }

               writeNet OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  write-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Write configuration to host using TFTP."
                   ::= { lsystem 55 }

               busyPer OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "CPU busy percentage in the last 5 second
                           period. Not the last 5 realtime seconds but
                           the last 5 second period in the scheduler."
                   ::= { lsystem 56 }






          -- cisco MIB                                         [Page 13]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               avgBusy1 OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "1 minute exponentially-decayed moving
                           average of the CPU busy percentage."
                   ::= { lsystem 57 }

               avgBusy5 OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "5 minute exponentially-decayed moving
                           average of the CPU busy percentage."
                   ::= { lsystem 58 }

               idleCount OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "cisco internal variable. not to be used"
                   ::= { lsystem 59 }

               idleWired OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "cisco internal variable. not to be used"
                   ::= { lsystem 60 }

               ciscoContactInfo OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "cisco's name and address"
                   ::= { lsystem 61 }

               bufferHgSize OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only





          -- cisco MIB                                         [Page 14]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the size of huge buffers."
                   ::= { lsystem 62 }

               bufferHgTotal OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the total number of huge buffers."
                   ::= { lsystem 63 }

               bufferHgFree OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of free huge buffers."
                   ::= { lsystem 64 }

               bufferHgMax OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the maximum number of huge
                           buffers."
                   ::= { lsystem 65 }

               bufferHgHit OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of huge buffer hits."
                   ::= { lsystem 66 }

               bufferHgMiss OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of huge buffer misses."
                   ::= { lsystem 67 }





          -- cisco MIB                                         [Page 15]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               bufferHgTrim OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of huge buffer trims."
                   ::= { lsystem 68 }

               bufferHgCreate OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Contains the number of huge buffer creates."
                   ::= { lsystem 69 }


               -- Local Interface Group

          -- This group is present in all products.


          -- Local Interface Table

          -- This group provides additional objects to the table
          -- defined by RFC1156.

               lifTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LIfEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A list of interface entries."
                   ::= { linterfaces 1 }

               lifEntry OBJECT-TYPE
                   SYNTAX LIfEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A collection of additional objects in the
                            cisco interface."
                   INDEX { ifIndex }
               ::= { lifTable 1 }






          -- cisco MIB                                         [Page 16]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               LIfEntry ::=
                   SEQUENCE {
                       locIfHardType
                           DisplayString,
                       locIfLineProt
                           INTEGER,
                       locIfLastIn
                           INTEGER,
                       locIfLastOut
                           INTEGER,
                       locIfLastOutHang
                           INTEGER,
                       locIfInBitsSec
                           INTEGER,
                       locIfInPktsSec
                           INTEGER,
                       locIfOutBitsSec
                           INTEGER,
                       locIfOutPktsSec
                           INTEGER,
                       locIfInRunts
                           INTEGER,
                       locIfInGiants
                           INTEGER,
                       locIfInCRC
                           INTEGER,
                       locIfInFrame
                           INTEGER,
                       locIfInOverrun
                           INTEGER,
                       locIfInIgnored
                           INTEGER,
                       locIfInAbort
                           INTEGER,
                       locIfResets
                           INTEGER,
                       locIfRestarts
                           INTEGER,
                       locIfKeep
                           INTEGER,
                       locIfReason
                           DisplayString,
                       locIfCarTrans
                           INTEGER,
                       locIfReliab





          -- cisco MIB                                         [Page 17]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           INTEGER,
                       locIfDelay
                           INTEGER,
                       locIfLoad
                           INTEGER,
                       locIfCollisions
                           INTEGER,
                       locIfInputQueueDrops
                           INTEGER,
                       locIfOutputQueueDrops
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               locIfHardType OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Returns the type of interface."
                   ::= { lifEntry 1 }

               locIfLineProt OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Boolean whether interface line protocol is
                           up or not."
                   ::= { lifEntry 2 }

               locIfLastIn OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Elapsed time in milliseconds since last
                           successful line protocol input packet was
                           received."
                   ::= { lifEntry 3 }

               locIfLastOut OBJECT-TYPE





          -- cisco MIB                                         [Page 18]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Elapsed time in milliseconds since last
                           successful line protocol output packet was
                           transmitted."
                   ::= { lifEntry 4 }

               locIfLastOutHang OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Elapsed time in milliseconds since last line
                           protocol output packet could not be
                           successfully transmitted."
                   ::= { lifEntry 5 }

               locIfInBitsSec OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Five minute average of input bits per
                           second."
                   ::= { lifEntry 6 }

               locIfInPktsSec OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Five minute average of input packets per
                           second."
                   ::= { lifEntry 7 }

               locIfOutBitsSec OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Five minute average of output bits per
                           second."
                   ::= { lifEntry 8 }





          -- cisco MIB                                         [Page 19]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               locIfOutPktsSec OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Five minute average of output packets per
                           second."
                   ::= { lifEntry 9 }

               locIfInRunts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of packets input which were smaller
                           then the allowable physical media permitted."
                   ::= { lifEntry 10 }

               locIfInGiants OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of input packets which were larger
                           then the physical media permitted."
                   ::= { lifEntry 11 }

               locIfInCRC OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of input packets which had cyclic
                           redundancy checksum errors."
                   ::= { lifEntry 12 }

               locIfInFrame OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of input packet which were
                           misaligned."
                   ::= { lifEntry 13 }






          -- cisco MIB                                         [Page 20]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               locIfInOverrun OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Count of input which arrived too quickly for
                           the to hardware receive."
                   ::= { lifEntry 14 }

               locIfInIgnored OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of input packets which were simply
                           ignored by this interface."
                   ::= { lifEntry 15 }

               locIfInAbort OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of input packets which were aborted."
                   ::= { lifEntry 16 }

               locIfResets OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of times the interface internally
                           reset."
                   ::= { lifEntry 17 }

               locIfRestarts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of times interface needed to be
                           completely restarted."
                   ::= { lifEntry 18 }

               locIfKeep OBJECT-TYPE





          -- cisco MIB                                         [Page 21]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Boolean whether keepalives are enabled on
                           this interface."
                   ::= { lifEntry 19 }

               locIfReason OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Reason for interface last status change."
                   ::= { lifEntry 20 }

               locIfCarTrans OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of times interface saw the carrier
                           signal transition."
                   ::= { lifEntry 21 }

               locIfReliab OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "The reliability of the interface. Used by
                           IGRP."
                   ::= { lifEntry 22 }

               locIfDelay OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "The amount of delay in microseconds of the
                           interface. Used by IGRP."
                   ::= { lifEntry 23 }

               locIfLoad OBJECT-TYPE
                   SYNTAX  INTEGER





          -- cisco MIB                                         [Page 22]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "The loading factor of the interface. Used by
                           IGRP."
                   ::= { lifEntry 24 }

               locIfCollisions OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "The number of output collisions detected on
                           this interface."
                   ::= { lifEntry 25 }

               locIfInputQueueDrops OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "The number of packets dropped because the
                           input queue was full."
                   ::= { lifEntry 26 }

               locIfOutputQueueDrops OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "The number of packets dropped because the
                           output queue was full."
                   ::= { lifEntry 27 }

               -- End of table



               -- Local IP Group

          -- This group is present in all products which are using the
          -- IP protocol.


          -- Local IP Address Table





          -- cisco MIB                                         [Page 23]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


          -- This group provides additional objects to the table
          -- defined by RFC1156.

               lipAddrTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LIpAddrEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A list of IP address entries."
                   ::= { lip 1 }

               lipAddrEntry OBJECT-TYPE
                   SYNTAX LIpAddrEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A collection of additional objects in the
                            cisco IP implementation."
                   INDEX { ipAdEntAddr }
               ::= { lipAddrTable 1 }

               LIpAddrEntry ::=
                   SEQUENCE {
                       locIPHow
                           DisplayString,
                       locIPWho
                           NetworkAddress,
                       locIPHelper
                           NetworkAddress,
                       locIPSecurity
                           INTEGER,
                       locIPRedirects
                           INTEGER,
                       locIPUnreach
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               locIPHow OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory





          -- cisco MIB                                         [Page 24]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                           "Method of how this interface obtained its IP
                           address."
                   ::= { lipAddrEntry 1 }

               locIPWho OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "IP address of who supplied this interface
                           its IP address."
                   ::= { lipAddrEntry 2 }

               locIPHelper OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "IP helper address for broadcast forwarding
                           support."
                   ::= { lipAddrEntry 3 }

               locIPSecurity OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "IP security level. See RFC 1038."
                   ::= { lipAddrEntry 4 }

               locIPRedirects OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Boolean whether ICMP redirects will be sent
                           or not."
                   ::= { lipAddrEntry 5 }

               locIPUnreach OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION





          -- cisco MIB                                         [Page 25]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           "Boolean whether ICMP unreachables will be
                           sent or not."
                   ::= { lipAddrEntry 6 }

               -- End of table



               -- Local IP Routing Table

          -- This group provides additional objects to the table
          -- defined by RFC1156.

               lipRoutingTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LIpRouteEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A list of IP routing entries."
                   ::= { lip 2 }

               lipRouteEntry OBJECT-TYPE
                   SYNTAX LIpRouteEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A collection of additional objects in the
                            cisco IP routing implementation."
                   INDEX { ipRouteDest }
               ::= { lipRoutingTable 1 }

               LIpRouteEntry ::=
                   SEQUENCE {
                       locRtMask
                           NetworkAddress,
                       locRtCount
                           INTEGER,
                       locRtUses
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.






          -- cisco MIB                                         [Page 26]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               locRtMask OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Routing table network mask."
                   ::= { lipRouteEntry 1 }

               locRtCount OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of parallel routes within routing
                           table."
                   ::= { lipRouteEntry 2 }

               locRtUses OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of times this route was used in a
                           forward operation."
                   ::= { lipRouteEntry 3 }

               -- End of table


               actThresh OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Threshold of IP accounting records in use
                           before IP traffic will be discarded."
                   ::= { lip 4 }

               actLostPkts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Lost IP packets due to memory limitations."
                   ::= { lip 5 }





          -- cisco MIB                                         [Page 27]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               actLostByts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total bytes of lost IP packets."
                   ::= { lip 6 }


               -- Local IP Accounting Table

          -- This group provides access to the cisco IP accounting
          -- support.

               lipAccountingTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LIpAccountEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A list of IP accounting entries."
                   ::= { lip 7 }

               lipAccountEntry OBJECT-TYPE
                   SYNTAX LIpAccountEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A collection of objects necessary for IP
                            accounting."
                   INDEX { actSrc, actDst }
               ::= { lipAccountingTable 1 }

               LIpAccountEntry ::=
                   SEQUENCE {
                       actSrc
                           NetworkAddress,
                       actDst
                           NetworkAddress,
                       actPkts
                           INTEGER,
                       actByts
                           INTEGER
                   }







          -- cisco MIB                                         [Page 28]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


          -- The following section describes the components of the
          -- table.

               actSrc OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "IP Source address for host traffic matrix."
                   ::= { lipAccountEntry 1 }

               actDst OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "IP Destination address for host traffic
                           matrix."
                   ::= { lipAccountEntry 2 }

               actPkts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of IP packets sent from source to
                           destination."
                   ::= { lipAccountEntry 3 }

               actByts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of bytes in IP packets from
                           source to destination."
                   ::= { lipAccountEntry 4 }

               -- End of table


               actAge OBJECT-TYPE
                   SYNTAX  TimeTicks
                   ACCESS  read-only
                   STATUS  mandatory





          -- cisco MIB                                         [Page 29]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                           "The age of the data in the current data
                           matrix."
                   ::= { lip 8 }


               -- Local IP Checkpoint Accounting Table

          -- This group provides access to the cisco
          -- IP checkpoint accounting support.

               lipCkAccountingTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LIpCkAccountEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A list of IP checkpoint accounting
                            entries."
                   ::= { lip 9 }

               lipCkAccountEntry OBJECT-TYPE
                   SYNTAX LIpCkAccountEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A collection of objects necessary for IP
                            checkpoint accounting."
                   INDEX { ckactSrc, ckactDst }
               ::= { lipCkAccountingTable 1 }

               LIpCkAccountEntry ::=
                   SEQUENCE {
                       ckactSrc
                           NetworkAddress,
                       ckactDst
                           NetworkAddress,
                       ckactPkts
                           INTEGER,
                       ckactByts
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.





          -- cisco MIB                                         [Page 30]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               ckactSrc OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "IP Source address for host in checkpoint
                           traffic matrix."
                   ::= { lipCkAccountEntry 1 }

               ckactDst OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "IP Destination address for host in
                           checkpoint traffic matrix."
                   ::= { lipCkAccountEntry 2 }

               ckactPkts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of IP packets sent from source to
                           destination in checkpoint matrix."
                   ::= { lipCkAccountEntry 3 }

               ckactByts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of bytes in IP packets from
                           source to destination in checkpoint matrix."
                   ::= { lipCkAccountEntry 4 }

               -- End of table


               ckactAge OBJECT-TYPE
                   SYNTAX  TimeTicks
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Age of data in the checkpoint matrix."





          -- cisco MIB                                         [Page 31]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ::= { lip 10 }

               actCheckPoint OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "Check points the accounting database. This
                           mib variable must be read and then set with
                           the same value for the check point to
                           succeed. The value read and then set will be
                           incremented after a successful set request"
                   ::= { lip 11 }

               ipNoaccess OBJECT-TYPE
                   SYNTAX  Counter
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of packets dropped due to
                           access control failure."
                   ::= { lip 12 }


               -- Local TCP Group

          -- This group is present in all products which are using the
          -- TCP protocol.


          -- Local TCP Connection Table

          -- This group provides additional objects to the table defined
          -- by RFC1156.

               ltcpConnTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LTcpConnEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A list of TCP connection entries."
                   ::= { ltcp 1 }

               ltcpConnEntry OBJECT-TYPE
                   SYNTAX LTcpConnEntry





          -- cisco MIB                                         [Page 32]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A collection of additional objects in the
                            cisco TCP implementation."
                   INDEX { tcpConnLocalAddress, tcpConnLocalPort,
                   tcpConnRemAddress, tcpConnRemPort}
               ::= { ltcpConnTable 1 }

               LTcpConnEntry ::=
                   SEQUENCE {
                       loctcpConnInBytes
                           INTEGER,
                       loctcpConnOutBytes
                           INTEGER,
                       loctcpConnInPkts
                           INTEGER,
                       loctcpConnOutPkts
                           INTEGER,
                       loctcpConnElapsed
                           TimeTicks
                   }


          -- The following section describes the components of the
          -- table.

               loctcpConnInBytes OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Bytes input for this TCP connection."
                   ::= { ltcpConnEntry 1 }

               loctcpConnOutBytes OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Bytes output for this TCP connection."
                   ::= { ltcpConnEntry 2 }

               loctcpConnInPkts OBJECT-TYPE
                   SYNTAX  INTEGER





          -- cisco MIB                                         [Page 33]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Packets input for this TCP connection."
                   ::= { ltcpConnEntry 3 }

               loctcpConnOutPkts OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Packets output for this TCP connection."
                   ::= { ltcpConnEntry 4 }

               loctcpConnElapsed OBJECT-TYPE
                   SYNTAX  TimeTicks
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "How long this TCP connection has been
                           established."
                   ::= { ltcpConnEntry 5 }

               -- End of table



               -- Local cisco Terminal Server Group

          -- This group is present in all products which contain
          -- asynchronous terminal lines.

               tsLines OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of physical lines on this device."
                   ::= { lts 1 }


               -- Local Terminal Server Line Table

          -- This group contains terminal server specific
          -- information on a per line basis.





          -- cisco MIB                                         [Page 34]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               ltsLineTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LTsLineEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A list of terminal server line entries."
                   ::= { lts 2 }

               ltsLineEntry OBJECT-TYPE
                   SYNTAX LTsLineEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A collection of per TTY objects in the
                            cisco Terminal Server implementation."
                   INDEX { INTEGER }
               ::= { ltsLineTable 1 }

               LTsLineEntry ::=
                   SEQUENCE {
                       tsLineActive
                           INTEGER,
                       tsLineType
                           INTEGER,
                       tsLineAutobaud
                           INTEGER,
                       tsLineSpeedin
                           INTEGER,
                       tsLineSpeedout
                           INTEGER,
                       tsLineFlow
                           INTEGER,
                       tsLineModem
                           INTEGER,
                       tsLineLoc
                           DisplayString,
                       tsLineTerm
                           DisplayString,
                       tsLineScrlen
                           INTEGER,
                       tsLineScrwid
                           INTEGER,
                       tsLineEsc
                           OCTET STRING,
                       tsLineTmo





          -- cisco MIB                                         [Page 35]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           INTEGER,
                       tsLineSestmo
                           INTEGER,
                       tsLineRotary
                           INTEGER,
                       tsLineUses
                           INTEGER,
                       tsLineNses
                           INTEGER,
                       tsLineUser
                           DisplayString,
                       tsLineNoise
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               tsLineActive OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Boolean whether this line is active or not."
                   ::= { ltsLineEntry 1 }

               tsLineType OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        console(2),
                        terminal(3),
                        line-printer(4),
                        virtual-terminal(5),
                        auxiliary(6)
                   }
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Type of line."
                   ::= { ltsLineEntry 2 }

               tsLineAutobaud OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only





          -- cisco MIB                                         [Page 36]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   STATUS  mandatory
                   DESCRIPTION
                           "Boolean whether line will autobaud or not."
                   ::= { ltsLineEntry 3 }

               tsLineSpeedin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "What input speed the line is running at."
                   ::= { ltsLineEntry 4 }

               tsLineSpeedout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "What output speed the line is running at."
                   ::= { ltsLineEntry 5 }

               tsLineFlow OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        none(2),
                        software-input(3),
                        software-output(4),
                        software-both(5),
                        hardware-input(6),
                        hardware-output(7),
                        hardware-both(8)
                   }
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "What kind of flow control the line is
                           using."
                   ::= { ltsLineEntry 6 }

               tsLineModem OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        none(2),
                        call-in(3),
                        call-out(4),





          -- cisco MIB                                         [Page 37]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                        cts-required(5),
                        rs-is-cd(6)
                   }
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "What kind of modem control the line is
                           using."
                   ::= { ltsLineEntry 7 }

               tsLineLoc OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Describes the line's physical location."
                   ::= { ltsLineEntry 8 }

               tsLineTerm OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Describes the line's terminal type."
                   ::= { ltsLineEntry 9 }

               tsLineScrlen OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Length in lines of the screen of terminal
                           attached to this line."
                   ::= { ltsLineEntry 10 }

               tsLineScrwid OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Width in characters of the screen of
                           terminal attached to this line."
                   ::= { ltsLineEntry 11 }

               tsLineEsc OBJECT-TYPE





          -- cisco MIB                                         [Page 38]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  OCTET STRING
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Escape character used to break out of active
                           sessions."
                   ::= { ltsLineEntry 12 }

               tsLineTmo OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Line idleness timeout in seconds."
                   ::= { ltsLineEntry 13 }

               tsLineSestmo OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Session idleness timeout in seconds."
                   ::= { ltsLineEntry 14 }

               tsLineRotary OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Rotary group number the line belongs in."
                   ::= { ltsLineEntry 15 }

               tsLineUses OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of times a connection has been made
                           to or from this line."
                   ::= { ltsLineEntry 16 }

               tsLineNses OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory





          -- cisco MIB                                         [Page 39]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                           "Current number of sessions in use on this
                           line."
                   ::= { ltsLineEntry 17 }

               tsLineUser OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "TACACS user name, if TACACS enabled, of user
                           on this line."
                   ::= { ltsLineEntry 18 }

               tsLineNoise OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Count of garbage characters received when
                           line inactive."
                   ::= { ltsLineEntry 19 }

               -- End of table



               -- Local Terminal Server Line Session Table

          -- This group contains terminal server specific
          -- information on a per line and per session basis.

               ltsLineSessionTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LTsLineSessionEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "A list of terminal server line and session
                            entries."
                   ::= { lts 3 }

               ltsLineSessionEntry OBJECT-TYPE
                   SYNTAX LTsLineSessionEntry
                   ACCESS  not-accessible
                   STATUS  mandatory





          -- cisco MIB                                         [Page 40]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                            "A collection of per session and per TTY
                            objects in the cisco Terminal Server
                            implementation."
                   INDEX { INTEGER, INTEGER }
               ::= { ltsLineSessionTable 1 }

               LTsLineSessionEntry ::=
                   SEQUENCE {
                       tslineSesType
                           INTEGER,
                       tslineSesDir
                           INTEGER,
                       tslineSesAddr
                           NetworkAddress,
                       tslineSesName
                           DisplayString,
                       tslineSesCur
                           INTEGER,
                       tslineSesIdle
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               tslineSesType OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        pad(2),
                        stream(3),
                        rlogin(4),
                        telnet(5),
                        tcp(6),
                        lat(7),
                        mop(8),
                        slip(9),
                        xremote(10)
                   }
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Type of session."
                   ::= { ltsLineSessionEntry 1 }





          -- cisco MIB                                         [Page 41]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               tslineSesDir OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        incoming(2),
                        outgoing(3)
                   }
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Direction of session."
                   ::= { ltsLineSessionEntry 2 }

               tslineSesAddr OBJECT-TYPE
                   SYNTAX  NetworkAddress
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Remote host address of session. [What about
                           PAD connections?]"
                   ::= { ltsLineSessionEntry 3 }

               tslineSesName OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Remote host name of session."
                   ::= { ltsLineSessionEntry 4 }

               tslineSesCur OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Boolean whether session is the currently
                           active one."
                   ::= { ltsLineSessionEntry 5 }

               tslineSesIdle OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Time in seconds session has been idle."
                   ::= { ltsLineSessionEntry 6 }





          -- cisco MIB                                         [Page 42]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               -- End of table


               tsMsgTtyLine OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "tty line to send the message to. -1 will
                           send it to all tty lines"
                   ::= { lts 4 }

               tsMsgIntervaltim OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "Interval between reissuing message in
                           milliseconds. Minimum non-zero setting is
                           10000. 0 will cause the routine to choose its
                           own intervals becoming more frequent as
                           MessageDuration gets close to expiring.
                           2hr, 1hr, 30min, 5min, 1min"
                   ::= { lts 5 }

               tsMsgDuration OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "Length of time to reissue message in
                           milliseconds. Minimum non-zero setting is
                           10000. A setting of 0 will not repeat the
                           message."
                   ::= { lts 6 }

               tsMsgText OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "Up to 256 characters that will make up the
                           message"
                   ::= { lts 7 }

               tsMsgTmpBanner OBJECT-TYPE





          -- cisco MIB                                         [Page 43]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  INTEGER {
                        no(1),
                        additive(2)
                   }
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "Should the message be used as a temporary
                           banner. 1 - No. 2 - In addition to the normal
                           banner"
                   ::= { lts 8 }

               tsMsgSend OBJECT-TYPE
                   SYNTAX  INTEGER {
                        nothing(1),
                        reload(2),
                        messagedone(3),
                        abort(4)
                   }
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "Sends the message. The value determines what
                           to do after the message has completed."
                   ::= { lts 9 }


               -- Temporary Variable Section

          -- This section is equivalent to the experimental
          -- space defined by the SMI. It contains variables
          -- that are useful to have but are beyond cisco's
          -- ability to control and maintain. This section can
          -- change from release to release without warning.
          -- This document controls what is contained here for
          -- this version.


          -- Temporary DECNET Section

          -- This group is present in all router based products.

               dnForward OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only





          -- cisco MIB                                         [Page 44]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of DECNET packets forwarded."
                   ::= { decnet 1 }

               dnReceived OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Count of total DECNET packets received."
                   ::= { decnet 2 }

               dnFormaterr OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of DECNET packets received with
                           header errors."
                   ::= { decnet 3 }

               dnNotgateway OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of packets received while not
                           routing."
                   ::= { decnet 4 }

               dnNotimp OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of unknown control packets
                           received."
                   ::= { decnet 5 }

               dnHellos OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION





          -- cisco MIB                                         [Page 45]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           "Total number of Hellos received."
                   ::= { decnet 6 }

               dnBadhello OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of received bad Hellos."
                   ::= { decnet 7 }

               dnNotlong OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of received packets not in long
                           format."
                   ::= { decnet 8 }

               dnDatas OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of received data packets."
                   ::= { decnet 9 }

               dnBigaddr OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of too large addresses."
                   ::= { decnet 10 }

               dnNoroute OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of packets dropped due to no
                           route present."
                   ::= { decnet 11 }






          -- cisco MIB                                         [Page 46]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               dnNoencap OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of packets dropped due to
                           output encapsulation failure."
                   ::= { decnet 12 }

               dnLevel1s OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of Level 1 routing packets
                           received."
                   ::= { decnet 13 }

               dnBadlevel1 OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of bad Level 1 routing packets
                           received."
                   ::= { decnet 14 }

               dnToomanyhops OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of packets received which
                           visited too many nodes."
                   ::= { decnet 15 }

               dnHellosent OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of Hellos output."
                   ::= { decnet 16 }

               dnLevel1sent OBJECT-TYPE





          -- cisco MIB                                         [Page 47]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of Level 1 routing packets
                           sent."
                   ::= { decnet 17 }

               dnNomemory OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of memory requests denied."
                   ::= { decnet 18 }

               dnOtherhello OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of Hellos received from another
                           area."
                   ::= { decnet 19 }

               dnOtherlevel1 OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of Level 1 routing packets
                           received from another area."
                   ::= { decnet 20 }

               dnLevel2s OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of Level 2 routing packets
                           received."
                   ::= { decnet 21 }

               dnLevel2sent OBJECT-TYPE
                   SYNTAX  INTEGER





          -- cisco MIB                                         [Page 48]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of Level 2 routing packets
                           sent."
                   ::= { decnet 22 }

               dnNovector OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of missing routing vectors."
                   ::= { decnet 23 }

               dnOtherlevel2 OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of received Level 2 routing
                           packets from another area."
                   ::= { decnet 24 }

               dnNoaccess OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of packets dropped due to
                           access control failure."
                   ::= { decnet 25 }

               dnAreaTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF DnAreaTableEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "DECNET area routing table"
                   ::= { decnet 26 }

               dnAreaTableEntry OBJECT-TYPE
                   SYNTAX DnAreaTableEntry
                   ACCESS  not-accessible
                   STATUS  mandatory





          -- cisco MIB                                         [Page 49]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                            "DECNET area routing table"
                   INDEX { dnArea }
               ::= { dnAreaTable 1 }

               DnAreaTableEntry ::=
                   SEQUENCE {
                       dnArea
                           INTEGER,
                       dnACost
                           INTEGER,
                       dnAHop
                           INTEGER,
                       dnAIfIndex
                           INTEGER,
                       dnANextHop
                           OCTET STRING,
                       dnAAge
                           INTEGER,
                       dnAPrio
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               dnArea OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "DECNet area from the area table."
                   ::= { dnAreaTableEntry 1 }

               dnACost OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Cost of area in the area table."
                   ::= { dnAreaTableEntry 2 }

               dnAHop OBJECT-TYPE
                   SYNTAX  INTEGER





          -- cisco MIB                                         [Page 50]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of hops to area in the area table."
                   ::= { dnAreaTableEntry 3 }

               dnAIfIndex OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Index of interface to the next hop address
                           to the area. 0 denotes self."
                   ::= { dnAreaTableEntry 4 }

               dnANextHop OBJECT-TYPE
                   SYNTAX  OCTET STRING
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Next hop DECNet address."
                   ::= { dnAreaTableEntry 5 }

               dnAAge OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Age in seconds of area route."
                   ::= { dnAreaTableEntry 6 }

               dnAPrio OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Priority of next hop router for area route."
                   ::= { dnAreaTableEntry 7 }

               -- End of table


               dnHostTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF DnHostTableEntry
                   ACCESS  not-accessible





          -- cisco MIB                                         [Page 51]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   STATUS  mandatory
                   DESCRIPTION
                            "DECNET routing table"
                   ::= { decnet 27 }

               dnHostTableEntry OBJECT-TYPE
                   SYNTAX DnHostTableEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "DECNET routing table"
                   INDEX { INTEGER, INTEGER }
               ::= { dnHostTable 1 }

               DnHostTableEntry ::=
                   SEQUENCE {
                       dnHost
                           INTEGER,
                       dnHCost
                           INTEGER,
                       dnHHop
                           INTEGER,
                       dnHIfIndex
                           INTEGER,
                       dnHNextHop
                           OCTET STRING,
                       dnHAge
                           INTEGER,
                       dnHPrio
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               dnHost OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "DECNet node address from the routing table."
                   ::= { dnHostTableEntry 1 }

               dnHCost OBJECT-TYPE





          -- cisco MIB                                         [Page 52]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Cost of path to node in the routing table."
                   ::= { dnHostTableEntry 2 }

               dnHHop OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Number of hops to node in the routing
                           table."
                   ::= { dnHostTableEntry 3 }

               dnHIfIndex OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Index of interface to the next hop address
                           to the node. 0 denotes self."
                   ::= { dnHostTableEntry 4 }

               dnHNextHop OBJECT-TYPE
                   SYNTAX  OCTET STRING
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Next hop DECNet address."
                   ::= { dnHostTableEntry 5 }

               dnHAge OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Age in seconds of route to node."
                   ::= { dnHostTableEntry 6 }

               dnHPrio OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory





          -- cisco MIB                                         [Page 53]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                           "Priority of next hop router for node."
                   ::= { dnHostTableEntry 7 }

               -- End of table


               dnIfTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF DnIfTableEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "DECNET interface table"
                   ::= { decnet 28 }

               dnIfTableEntry OBJECT-TYPE
                   SYNTAX DnIfTableEntry
                   ACCESS  not-accessible
                   STATUS  mandatory
                   DESCRIPTION
                            "DECNET interface table"
                   INDEX { ifIndex }
               ::= { dnIfTable 1 }

               DnIfTableEntry ::=
                   SEQUENCE {
                       dnIfCost
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               dnIfCost OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Cost of this interface."
                   ::= { dnIfTableEntry 1 }

               -- End of table







          -- cisco MIB                                         [Page 54]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               -- Temporary XNS Section

          -- This group is present in all router based products.

               xnsInput OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total input count of number of XNS packets."
                   ::= { xns 1 }

               xnsLocal OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of XNS input packets for this
                           host."
                   ::= { xns 2 }

               xnsBcastin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS input broadcast
                           packets."
                   ::= { xns 3 }

               xnsForward OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS packets
                           forwarded."
                   ::= { xns 4 }

               xnsBcastout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS output





          -- cisco MIB                                         [Page 55]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           broadcast packets."
                   ::= { xns 5 }

               xnsErrin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS Error input
                           packets."
                   ::= { xns 6 }

               xnsErrout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS Error output
                           packets."
                   ::= { xns 7 }

               xnsFormerr OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS input packets
                           with header errors."
                   ::= { xns 8 }

               xnsChksum OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS input packets
                           with checksum errors."
                   ::= { xns 9 }

               xnsNotgate OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS input packets





          -- cisco MIB                                         [Page 56]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           received while not routing."
                   ::= { xns 10 }

               xnsHopcnt OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS input packets
                           that have exceeded the maximum hop count."
                   ::= { xns 11 }

               xnsNoroute OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS packets dropped
                           due to no route."
                   ::= { xns 12 }

               xnsNoencap OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS packets dropped
                           due to output encapsulation failure."
                   ::= { xns 13 }

               xnsOutput OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS output
                           packets."
                   ::= { xns 14 }

               xnsInmult OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS input multicast





          -- cisco MIB                                         [Page 57]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           packets."
                   ::= { xns 15 }

               xnsUnknown OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of unknown XNS input
                           packets."
                   ::= { xns 16 }

               xnsFwdbrd OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS broadcast
                           packets forwarded."
                   ::= { xns 17 }

               xnsEchoreqin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS Echo request
                           packets received."
                   ::= { xns 18 }

               xnsEchoreqout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS Echo request
                           packets sent."
                   ::= { xns 19 }

               xnsEchorepin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS Echo reply





          -- cisco MIB                                         [Page 58]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           packets received."
                   ::= { xns 20 }

               xnsEchorepout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of XNS Echo reply
                           packets sent."
                   ::= { xns 21 }


               -- Temporary AppleTalk Section

          -- This group is present in all router based products.

               atInput OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total input count of number of AppleTalk
                           packets."
                   ::= { appletalk 1 }

               atLocal OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of AppleTalk input packets for
                           this host."
                   ::= { appletalk 2 }

               atBcastin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk input
                           broadcast packets."
                   ::= { appletalk 3 }

               atForward OBJECT-TYPE





          -- cisco MIB                                         [Page 59]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk packets
                           forwarded."
                   ::= { appletalk 4 }

               atBcastout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk output
                           broadcast packets."
                   ::= { appletalk 5 }

               atChksum OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk input
                           packets with checksum erors."
                   ::= { appletalk 7 }

               atNotgate OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of AppleTalk input packets
                           received while not routing."
                   ::= { appletalk 8 }

               atHopcnt OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk input
                           packets that have exceeded the maximum hop
                           count."
                   ::= { appletalk 9 }






          -- cisco MIB                                         [Page 60]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               atNoaccess OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total number of AppleTalk packets dropped
                           due to access control."
                   ::= { appletalk 10 }

               atNoroute OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk packets
                           dropped due to no route."
                   ::= { appletalk 11 }

               atNoencap OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk packets
                           dropped due to output encapsulation failure."
                   ::= { appletalk 12 }

               atOutput OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk output
                           packets."
                   ::= { appletalk 13 }

               atInmult OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk input
                           multicast packets."
                   ::= { appletalk 14 }






          -- cisco MIB                                         [Page 61]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               atRtmpin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk RTMP
                           packets received."
                   ::= { appletalk 15 }

               atRtmpout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk RTMP
                           packets sent."
                   ::= { appletalk 16 }

               atNbpin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk NBP
                           packets received."
                   ::= { appletalk 17 }

               atNbpout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk NBP
                           packets sent."
                   ::= { appletalk 18 }

               atAtp OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk ATP
                           packets received."
                   ::= { appletalk 19 }






          -- cisco MIB                                         [Page 62]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               atZipin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk ZIP
                           packets received."
                   ::= { appletalk 20 }

               atZipout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk ZIP
                           packets sent."
                   ::= { appletalk 21 }

               atEcho OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk Echo
                           packets received."
                   ::= { appletalk 22 }

               atEchoill OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of illegal AppleTalk
                           Echo packets received."
                   ::= { appletalk 23 }

               atDdpshort OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of short AppleTalk DDP
                           packets received."
                   ::= { appletalk 24 }






          -- cisco MIB                                         [Page 63]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               atDdplong OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of long AppleTalk DDP
                           packets received."
                   ::= { appletalk 25 }

               atDdpbad OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of illegal sized
                           AppleTalk DDP packets received."
                   ::= { appletalk 26 }

               atNobuffer OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk packets
                           lost due to no memory."
                   ::= { appletalk 27 }

               atArpreq OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of input AppleTalk ARP
                           request packets."
                   ::= { appletalk 28 }

               atArpreply OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of AppleTalk ARP reply
                           packets output."
                   ::= { appletalk 29 }






          -- cisco MIB                                         [Page 64]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


               atArpprobe OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of input AppleTalk ARP
                           probe packets."
                   ::= { appletalk 30 }

               atUnknown OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of unknown AppleTalk
                           input packets."
                   ::= { appletalk 31 }


               -- Temporary Novell Section

          -- This group is present in all router based products.

               novellInput OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total input count of number of NOVELL
                           packets."
                   ::= { novell 1 }

               novellBcastin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL input
                           broadcast packets."
                   ::= { novell 2 }

               novellForward OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory





          -- cisco MIB                                         [Page 65]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                           "Total count of number of NOVELL packets
                           forwarded."
                   ::= { novell 3 }

               novellBcastout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL output
                           broadcast packets."
                   ::= { novell 4 }

               novellFormerr OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL input
                           packets with header errors."
                   ::= { novell 5 }

               novellChksum OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL input
                           packets with checksum erors."
                   ::= { novell 6 }

               novellHopcnt OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL input
                           packets that have exceeded the maximum hop
                           count."
                   ::= { novell 7 }

               novellNoroute OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only





          -- cisco MIB                                         [Page 66]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL packets
                           dropped due to no route."
                   ::= { novell 8 }

               novellNoencap OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL packets
                           dropped due to output encapsulation failure."
                   ::= { novell 9 }

               novellOutput OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL output
                           packets."
                   ::= { novell 10 }

               novellInmult OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL input
                           multicast packets."
                   ::= { novell 11 }

               novellLocal OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of NOVELL input packets for this
                           host."
                   ::= { novell 12 }

               novellUnknown OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only





          -- cisco MIB                                         [Page 67]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of unknown NOVELL
                           input packets."
                   ::= { novell 13 }

               novellSapreqin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL SAP request
                           packets received."
                   ::= { novell 14 }

               novellSapresin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL SAP response
                           packets received."
                   ::= { novell 15 }

               novellSapout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL SAP request
                           packets sent."
                   ::= { novell 16 }

               novellSapreply OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of NOVELL SAP reply
                           packets sent."
                   ::= { novell 17 }


               -- Temporary Vines Section






          -- cisco MIB                                         [Page 68]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


          -- This group is present in all router based products.

               vinesInput OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total input count of number of Vines
                           packets."
                   ::= { vines 1 }

               vinesOutput OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines output
                           packets."
                   ::= { vines 2 }

               vinesLocaldest OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of Vines input packets for this
                           host."
                   ::= { vines 3 }

               vinesForwarded OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines packets
                           forwarded."
                   ::= { vines 4 }

               vinesBcastin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines input
                           broadcast packets."





          -- cisco MIB                                         [Page 69]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   ::= { vines 5 }

               vinesBcastout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines output
                           broadcast packets."
                   ::= { vines 6 }

               vinesBcastfwd OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines broadcast
                           packets forwarded."
                   ::= { vines 7 }

               vinesNotlan OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines broadcast
                           packets not forwarded to all interfaces
                           because the LAN ONLY bit was set."
                   ::= { vines 8 }

               vinesNotgt4800 OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines broadcast
                           packets not forwarded to all interfaces
                           because the OVER 4800 BPS bit was set."
                   ::= { vines 9 }

               vinesNocharges OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION





          -- cisco MIB                                         [Page 70]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                           "Total count of number of Vines broadcast
                           packets not forwarded to all interfaces
                           because the NO CHARGES only bit was set."
                   ::= { vines 10 }

               vinesFormaterror OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines input packets
                           with header errors."
                   ::= { vines 11 }

               vinesCksumerr OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines input packets
                           with checksum erors."
                   ::= { vines 12 }

               vinesHopcount OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines input packets
                           that have exceeded the maximum hop count."
                   ::= { vines 13 }

               vinesNoroute OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines packets
                           dropped due to no route."
                   ::= { vines 14 }

               vinesEncapsfailed OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory





          -- cisco MIB                                         [Page 71]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                           "Total count of number of Vines packets
                           dropped due to output encapsulation failed."
                   ::= { vines 15 }

               vinesUnknown OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of unknown Vines input
                           packets."
                   ::= { vines 16 }

               vinesIcpIn OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines ICP packets
                           received."
                   ::= { vines 17 }

               vinesIcpOut OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines ICP packets
                           generaed."
                   ::= { vines 18 }

               vinesMetricOut OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines ICP Metric
                           Notification packets generated."
                   ::= { vines 19 }

               vinesMacEchoIn OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory





          -- cisco MIB                                         [Page 72]
--





          -- Request for Comments: Draft             cisco Systems, Inc.


                   DESCRIPTION
                           "Total count of number of Vines MAC level
                           Echo packets received."
                   ::= { vines 20 }

               vinesMacEchoOut OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines MAC level
                           Echo packets generated."
                   ::= { vines 21 }

               vinesEchoIn OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines Echo packets
                           received."
                   ::= { vines 22 }

               vinesEchoOut OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "Total count of number of Vines Echo packets
                           generated."
                   ::= { vines 23 }
               END


















          -- cisco MIB                                         [Page 73]
--

