--- Log started: 01/02/09 14:46:50
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                                                   Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\LE1I3A46+slic.wph...
        
        Error code : 2(0x00000002)
        Description:
            系统找不到指定的文件。
            错误代码： 2
--- Log started: 01/02/09 14:47:20
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                                                   Skycn123汉化

Error code : -200(0xFFFFFF38)
Description:
    错误代码： -200
--- Log stopped: 01/02/09 14:47:21

--- Log stopped: 01/02/09 14:47:24

--- Log started: 01/02/09 14:47:30
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                                                   Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 019009A2
        UI or command line masks  : 00000000
        Effective flags           : 019009A2
        DMI update mode           : 3
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHNT.SYS
        Initializing driver...
        
        SFLS - Get Entry Point
        
         dwFuncNumErrorCode=00000000
         EntryPoint=b412386e
         
        SFLS - Get Capabilities (0201h)
        
        SFLS Get Capabilities Error.
    
    Get BIOS information from image file...
        BCPSYS information:
            Version    : 3.2
            Size       : 130
            Date       : 6/15/2007
            Time       : 13:47:23
            Part number: DEVELP72(P72)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 2
    
    Get BIOS information from system...
        BCPSYS information:
            Version    : 3.2
            Size       : 128
            Date       : 3/17/2006
            Time       : 9:52:10
            Part number: DEVEL3XV(3XV)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 3
        BIOS image is not Axx swapped
    Stage completed

Get BIOS information from image file...
    BCPSYS information:
        Version    : 3.2
        Size       : 130
        Date       : 6/15/2007
        Time       : 13:47:23
        Part number: DEVELP72(P72)
    BCPDMI information:
        Version    : 2.11
        Size       : 40
        OEM strings: 2
--- Log stopped: 01/02/09 14:48:08

--- Log started: 01/02/09 14:51:08
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                                                   Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 14:51:14

--- Log started: 01/02/09 14:51:49
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash        Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 019009A2
        UI or command line masks  : 00000000
        Effective flags           : 019009A2
        DMI update mode           : 3
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHNT.SYS
        Initializing driver...
        
        SFLS - Get Entry Point
        
         dwFuncNumErrorCode=00000000
         EntryPoint=b3ed286e
         
        SFLS - Get Capabilities (0201h)
        
        SFLS Get Capabilities Error.
    
    Get BIOS information from image file...
        BCPSYS information:
            Version    : 3.2
            Size       : 130
            Date       : 6/15/2007
            Time       : 13:47:23
            Part number: DEVELP72(P72)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 2
    
    Get BIOS information from system...
        BCPSYS information:
            Version    : 3.2
            Size       : 128
            Date       : 3/17/2006
            Time       : 9:52:10
            Part number: DEVEL3XV(3XV)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 3
        BIOS image is not Axx swapped
    Stage completed

Get BIOS information from image file...
    BCPSYS information:
        Version    : 3.2
        Size       : 130
        Date       : 6/15/2007
        Time       : 13:47:23
        Part number: DEVELP72(P72)
    BCPDMI information:
        Version    : 2.11
        Size       : 40
        OEM strings: 2
--- Log stopped: 01/02/09 14:52:24

--- Log started: 01/02/09 14:52:48
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash        Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 14:52:59

--- Log started: 01/02/09 14:53:34
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash        Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 019009A2
        UI or command line masks  : 00000000
        Effective flags           : 019009A2
        DMI update mode           : 3
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHNT.SYS
        Initializing driver...
        
        SFLS - Get Entry Point
        
         dwFuncNumErrorCode=00000000
         EntryPoint=b3c8186e
         
        SFLS - Get Capabilities (0201h)
        
        SFLS Get Capabilities Error.
    
    Get BIOS information from image file...
        BCPSYS information:
            Version    : 3.2
            Size       : 130
            Date       : 6/15/2007
            Time       : 13:47:23
            Part number: DEVELP72(P72)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 2
    
    Get BIOS information from system...
        BCPSYS information:
            Version    : 3.2
            Size       : 128
            Date       : 3/17/2006
            Time       : 9:52:10
            Part number: DEVEL3XV(3XV)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 3
        BIOS image is not Axx swapped
    Stage completed

Get BIOS information from image file...
    BCPSYS information:
        Version    : 3.2
        Size       : 130
        Date       : 6/15/2007
        Time       : 13:47:23
        Part number: DEVELP72(P72)
    BCPDMI information:
        Version    : 2.11
        Size       : 40
        OEM strings: 2
--- Log stopped: 01/02/09 14:53:57

--- Log started: 01/02/09 14:56:24
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash        Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 14:56:31

--- Log started: 01/02/09 14:58:29
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash        Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 14:58:38

--- Log started: 01/02/09 14:58:39
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 14:58:51

--- Log started: 01/02/09 15:00:00
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : D:\下载\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 009009A2
        UI or command line masks  : 00000000
        Effective flags           : 009009A2
        DMI update mode           : 3
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: D:\下载\winphlash2.0.3.4\PHLASHNT.SYS
        Initializing driver...
        
        SFLS - Get Entry Point
        
         dwFuncNumErrorCode=00000000
         EntryPoint=b3a3086e
         
        SFLS - Get Capabilities (0201h)
        
        SFLS Get Capabilities Error.
    
    Get BIOS information from image file...
        BCPSYS information:
            Version    : 3.2
            Size       : 130
            Date       : 6/15/2007
            Time       : 13:47:23
            Part number: DEVELP72(P72)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 2
    
    Get BIOS information from system...
        BCPSYS information:
            Version    : 3.2
            Size       : 128
            Date       : 3/17/2006
            Time       : 9:52:10
            Part number: DEVEL3XV(3XV)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 3
        BIOS image is not Axx swapped
    Stage completed

Get BIOS information from image file...
    BCPSYS information:
        Version    : 3.2
        Size       : 130
        Date       : 6/15/2007
        Time       : 13:47:23
        Part number: DEVELP72(P72)
    BCPDMI information:
        Version    : 2.11
        Size       : 40
        OEM strings: 2
--- Log stopped: 01/02/09 15:02:19

--- Log started: 01/02/09 15:28:10
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : D:\下载\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 009009A2
        UI or command line masks  : 00000000
        Effective flags           : 009009A2
        DMI update mode           : 3
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: D:\下载\winphlash2.0.3.4\PHLASHNT.SYS
        Initializing driver...
        
        SFLS - Get Entry Point
        
         dwFuncNumErrorCode=00000000
         EntryPoint=b37df86e
         
        SFLS - Get Capabilities (0201h)
        
        SFLS Get Capabilities Error.
    
    Get BIOS information from image file...
        BCPSYS information:
            Version    : 3.2
            Size       : 130
            Date       : 6/15/2007
            Time       : 13:47:23
            Part number: DEVELP72(P72)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 2
    
    Get BIOS information from system...
        BCPSYS information:
            Version    : 3.2
            Size       : 128
            Date       : 3/17/2006
            Time       : 9:52:10
            Part number: DEVEL3XV(3XV)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 3
        BIOS image is not Axx swapped
    Stage completed

Get BIOS information from image file...
    BCPSYS information:
        Version    : 3.2
        Size       : 130
        Date       : 6/15/2007
        Time       : 13:47:23
        Part number: DEVELP72(P72)
    BCPDMI information:
        Version    : 2.11
        Size       : 40
        OEM strings: 2
--- Log stopped: 01/02/09 15:28:37

--- Log started: 01/02/09 15:29:51
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : D:\下载\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 009009A2
        UI or command line masks  : 00000000
        Effective flags           : 009009A2
        DMI update mode           : 3
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: D:\下载\winphlash2.0.3.4\PHLASHNT.SYS
        Initializing driver...
        
        SFLS - Get Entry Point
        
         dwFuncNumErrorCode=00000000
         EntryPoint=b358e86e
         
        SFLS - Get Capabilities (0201h)
        
        SFLS Get Capabilities Error.
    
    Get BIOS information from image file...
        BCPSYS information:
            Version    : 3.2
            Size       : 130
            Date       : 6/15/2007
            Time       : 13:47:23
            Part number: DEVELP72(P72)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 2
    
    Get BIOS information from system...
        BCPSYS information:
            Version    : 3.2
            Size       : 128
            Date       : 3/17/2006
            Time       : 9:52:10
            Part number: DEVEL3XV(3XV)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 3
        BIOS image is not Axx swapped
    Stage completed

Get BIOS information from image file...
    BCPSYS information:
        Version    : 3.2
        Size       : 130
        Date       : 6/15/2007
        Time       : 13:47:23
        Part number: DEVELP72(P72)
    BCPDMI information:
        Version    : 2.11
        Size       : 40
        OEM strings: 2
--- Log stopped: 01/02/09 15:30:38

--- Log started: 01/02/09 15:38:01
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:39:02

--- Log started: 01/02/09 15:40:04
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log started: 01/02/09 15:41:18
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化

Error code : -200(0xFFFFFF38)
Description:
    错误代码： -200
--- Log stopped: 01/02/09 15:41:20

--- Log stopped: 01/02/09 15:41:22

--- Log started: 01/02/09 15:41:23
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : D:\下载\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 009001A2
        UI or command line masks  : 00000000
        Effective flags           : 009001A2
        DMI update mode           : 1
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: D:\下载\winphlash2.0.3.4\PHLASHNT.SYS
        Initializing driver...
        
        SFLS - Get Entry Point
        
         dwFuncNumErrorCode=00000000
         EntryPoint=b333d86e
         
        SFLS - Get Capabilities (0201h)
        
        SFLS Get Capabilities Error.
    
    Get BIOS information from image file...
        BCPSYS information:
            Version    : 3.2
            Size       : 130
            Date       : 6/15/2007
            Time       : 13:47:23
            Part number: DEVELP72(P72)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 2
    
    Get BIOS information from system...
        BCPSYS information:
            Version    : 3.2
            Size       : 128
            Date       : 3/17/2006
            Time       : 9:52:10
            Part number: DEVEL3XV(3XV)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 3
        BIOS image is not Axx swapped
    Stage completed

Get BIOS information from image file...
    BCPSYS information:
        Version    : 3.2
        Size       : 130
        Date       : 6/15/2007
        Time       : 13:47:23
        Part number: DEVELP72(P72)
    BCPDMI information:
        Version    : 2.11
        Size       : 40
        OEM strings: 2
--- Log stopped: 01/02/09 15:43:35

--- Log started: 01/02/09 15:44:18
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:44:27

--- Log started: 01/02/09 15:47:27
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:47:37

--- Log started: 01/02/09 15:50:33
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:50:36

--- Log started: 01/02/09 15:51:39
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:52:09

--- Log started: 01/02/09 15:53:07
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:53:15

--- Log started: 01/02/09 15:53:31
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:53:54

--- Log started: 01/02/09 15:55:13
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:56:06

--- Log started: 01/02/09 15:56:46
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 15:57:02

--- Log started: 01/02/09 16:02:45
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph
        Backup file    : D:\下载\winphlash2.0.3.4\BAK.wph
    
    Loading new BIOS image file...
        Opening file D:\下载\winphlash2.0.3.4\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 009001A2
        UI or command line masks  : 00000000
        Effective flags           : 009001A2
        DMI update mode           : 1
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: D:\下载\winphlash2.0.3.4\PHLASHNT.SYS
        Initializing driver...
        
        SFLS - Get Entry Point
        
         dwFuncNumErrorCode=00000000
         EntryPoint=b30ec86e
         
        SFLS - Get Capabilities (0201h)
        
        SFLS Get Capabilities Error.
    
    Get BIOS information from image file...
        BCPSYS information:
            Version    : 3.2
            Size       : 130
            Date       : 6/15/2007
            Time       : 13:47:23
            Part number: DEVELP72(P72)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 2
    
    Get BIOS information from system...
        BCPSYS information:
            Version    : 3.2
            Size       : 128
            Date       : 3/17/2006
            Time       : 9:52:10
            Part number: DEVEL3XV(3XV)
        BCPDMI information:
            Version    : 2.11
            Size       : 40
            OEM strings: 3
        BIOS image is not Axx swapped
    Stage completed

Get BIOS information from image file...
    BCPSYS information:
        Version    : 3.2
        Size       : 130
        Date       : 6/15/2007
        Time       : 13:47:23
        Part number: DEVELP72(P72)
    BCPDMI information:
        Version    : 2.11
        Size       : 40
        OEM strings: 2
--- Log stopped: 01/02/09 16:03:11

--- Log started: 01/02/09 16:04:32
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:04:38

--- Log started: 01/02/09 16:05:20
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:05:24

--- Log started: 01/02/09 16:05:35
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:05:45

--- Log started: 01/02/09 16:06:04
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:06:09

--- Log started: 01/02/09 16:06:32
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:06:50

--- Log started: 01/02/09 16:07:15
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:07:42

--- Log started: 01/02/09 16:07:46
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:07:52

--- Log started: 01/02/09 16:08:12
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:08:14

--- Log started: 01/02/09 16:09:39
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:09:44

--- Log started: 01/02/09 16:29:03
Initializing...
Log file       : D:\下载\winphlash2.0.3.4\PHLASH.LOG
Settings file  : D:\下载\winphlash2.0.3.4\PHLASH.INI (found)
Executable     : D:\下载\winphlash2.0.3.4\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/2/2009
Resource file  : D:\下载\winphlash2.0.3.4\PHLASHLC.DLL (loaded)
Help file      : D:\下载\winphlash2.0.3.4\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/02/09 16:29:08

--- Log started: 01/03/09 13:22:06
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/3/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\LE1I3A46+slic.wph
        Backup file    : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\BAK.wph
    
    Loading new BIOS image file...
        Opening file C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 009001A2
        UI or command line masks  : 00000000
        Effective flags           : 009001A2
        DMI update mode           : 1
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHNT.SYS
        Warning: Service "WinPhlash" already exists
        Error: Failed to start service "WinPhlash": 1058
        Installing and loading Windows NT driver: C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHNT.SYS
        Warning: Service "WinPhlash" already exists
        Error: Failed to start service "WinPhlash": 1058
        
        Error code : 1072(0x00000430)
        Description:
            指定的服务已标记为删除。
            错误代码： 1072
--- Log stopped: 01/03/09 13:22:29

--- Log started: 01/03/09 13:24:30
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/3/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/03/09 13:24:42

--- Log started: 01/03/09 13:29:10
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/3/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported

Preparation stage
    
    Processing parameters...
        Image file     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\LE1I3A46+slic.wph
        Backup file    : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\BAK.wph
    
    Loading new BIOS image file...
        Opening file C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\LE1I3A46+slic.wph...
        Allocating 1051235 bytes...
        Reading 32768 bytes from the file starting at      0...
        Reading 32768 bytes from the file starting at  32768...
        Reading 32768 bytes from the file starting at  65536...
        Reading 32768 bytes from the file starting at  98304...
        Reading 32768 bytes from the file starting at 131072...
        Reading 32768 bytes from the file starting at 163840...
        Reading 32768 bytes from the file starting at 196608...
        Reading 32768 bytes from the file starting at 229376...
        Reading 32768 bytes from the file starting at 262144...
        Reading 32768 bytes from the file starting at 294912...
        Reading 32768 bytes from the file starting at 327680...
        Reading 32768 bytes from the file starting at 360448...
        Reading 32768 bytes from the file starting at 393216...
        Reading 32768 bytes from the file starting at 425984...
        Reading 32768 bytes from the file starting at 458752...
        Reading 32768 bytes from the file starting at 491520...
        Reading 32768 bytes from the file starting at 524288...
        Reading 32768 bytes from the file starting at 557056...
        Reading 32768 bytes from the file starting at 589824...
        Reading 32768 bytes from the file starting at 622592...
        Reading 32768 bytes from the file starting at 655360...
        Reading 32768 bytes from the file starting at 688128...
        Reading 32768 bytes from the file starting at 720896...
        Reading 32768 bytes from the file starting at 753664...
        Reading 32768 bytes from the file starting at 786432...
        Reading 32768 bytes from the file starting at 819200...
        Reading 32768 bytes from the file starting at 851968...
        Reading 32768 bytes from the file starting at 884736...
        Reading 32768 bytes from the file starting at 917504...
        Reading 32768 bytes from the file starting at 950272...
        Reading 32768 bytes from the file starting at 983040...
        Reading 32768 bytes from the file starting at 1015808...
        Reading  2651 bytes from the file starting at 1048576...
    
    Looking for interface descriptors and code...
        cbSearch=    4096 (0x00001000)
        BIOS image size is          : 1048576 (0x00100000)
        Descriptors and code size is:   2651 (0x00000A5B)
    
    Verifying interface descriptors and code...
        Allocating 2792 bytes for interface data and code...
        Copying interface data and code...
        Looking for the part table structure...
        Part table contains 4 device(s)...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for part descriptor...
        Looking for the text descriptor table structure...
        Looking for Text descriptor...
            Device name  : EN29LV800AT (00DA007F)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : A29L800T (001A0037)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : S29AL008DT (00DA0001)
            Version label: ALPHA
            Block info   : 15X64K 32K 8K 8K 16K
        Looking for Text descriptor...
            Device name  : SST39VF088 (00D800BF)
            Version label: ALPHA
            Block info   : 256x4K
        Looking for the platform descriptor ...
        Looking for the keyboard table ...
        Looking for the IBM table...
        Verifying the block table ...
        	4GB flash area is 100000 bytes: FFF00000-FFFFFFFF
    
    Combine flags from the platform descriptor with flags from UI or command line
        Platform descriptor flags : 00000020
        UI or command line flags  : 019001A2
        UI or command line masks  : 01D121A6
        Effective flags           : 019001A2
        DMI update mode           : 1
    Stage completed

Analysis stage
    
    Loading and initializing driver...
        Installing and loading Windows NT driver: C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHNT.SYS
        Warning: Service "WinPhlash" already exists
        Error: Failed to start service "WinPhlash": 1058
        Installing and loading Windows NT driver: C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHNT.SYS
        Warning: Service "WinPhlash" already exists
        Error: Failed to start service "WinPhlash": 1058
        
        Error code : 1072(0x00000430)
        Description:
            指定的服务已标记为删除。
            错误代码： 1072
--- Log stopped: 01/03/09 13:29:33

--- Log started: 01/03/09 13:34:49
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/3/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/03/09 13:35:45

--- Log started: 01/03/09 13:37:40
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/3/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/03/09 13:38:35

--- Log started: 01/03/09 13:41:35
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/3/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/03/09 13:41:50

--- Log started: 01/03/09 13:50:46
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/3/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/03/09 13:50:47

--- Log started: 01/03/09 13:50:49
Initializing...
Log file       : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASH.LOG
Settings file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASH.INI (found)
Executable     : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\SWinFlash.exe
    Version    : 2.0.3.4    Build      : Phoenix cME Secure WinFlash
    Date       : 1/3/2009
Resource file  : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\PHLASHLC.DLL (loaded)
Help file      : C:\Documents and Settings\Administrator\桌面\winphlash2.0.3.4汉化\winphlash2.0.3.4汉化\WINPHLASH.HLP
App name       : Phoenix Secure WinFlash                              Skycn123汉化
OS Information : Windows NT 5.1.2600 Service Pack 3 - supported
--- Log stopped: 01/03/09 13:50:52

