README SUPPLEMENT FOR PS UNIVERSAL DRIVERS
Last Modified: 2011/09/21

[How to install/uninstall PS Universal printer driver]
1. Installing PS Universal printer driver

As the information contained in this document applies to multiple print devices, the word "Device" is used as a generic reference to whichever device you are using. 
1-1 For devices connected via USB
1-1-1 Windows 7, Server 2008 R2
Step 1 Log in to Windows as an Administrator.
Step 2 Close any open applications.
Step 3 Connect the "Device" to a PC using a USB cable and then power on the "Device".
Step 4 Automatic installation of the device driver will appear to start and then fail, displaying the message "Device driver software was not successfully installed". Close this message.
Step 5 Open "Device Manager".
Step 6 The "Device" should be listed under "Other devices". Right-click "Device" and select "Update Device Software...".
Step 7 When the "Update Device Software" screen is displayed, select "Browse my computer for driver software".
Step 8 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
Step 9 Follow the rest of the Wizard's instructions to complete the installation.
 
1-1-2 Windows XP, 2003, Vista, 2008
Step 1 Log in to Windows as an Administrator.
Step 2 Close any open applications.
Step 3 Connect the PC and the "Device" using a USB cable and then power on the "Device".
Step 4 If a "Found New Hardware" popup is displayed, click "Cancel" to close it.
Step 5 Open "Printers and Faxes" from the Start menu.
Step 6 Select "Add Printer".
Step 7 "Welcome to the Add Printer Wizard" is displayed. Click "Next >".
Step 8 The "Local or Network Printer" dialogue is displayed. Select "Local printer attached to this computer" and click "Next >". Note: Do not enable "Automatically detect and install my Plug and Play printer".
Step 9 The "Select a Printer Port" dialogue is displayed. Select "Virtual printer port for USB" as the port type.
Step 10 The "Install Printer Software" dialogue is displayed. Select "Have Disk".
Step 11 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
Step 12 Follow the rest of the Wizard's instructions to complete the installation.
 
1-2 For devices connected via network
 
1-2-1 Windows 7, Server 2008 R2
Step 1 Log in to Windows as an Administrator.
Step 2 Close any open applications.
Step 3 From the "Start" menu, select "Devices and Printers" > "Add a Printer".
Step 4 The "Add a Printer" dialogue will be displayed asking "What type of printer do you want to install?" Select "Add network, wireless, or Bluetooth printer".
Step 5 The "Searching for available printers" dialogue appears. Select the "Device" from the list of printers and click "Next". (If you do not see your "Device" in this list, please proceed to "What to do if your device is not found" at the end of this section.)
Step 6 The "Install the printer driver" dialogue appears. Click "Have Disk".
Step 7 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
Step 8 Follow the rest of the Wizard's instructions to complete the installation.
 
1-2-1-b What to do if your device is not found
Step 1 Log in to Windows as an Administrator.
Step 2 Close any open applications.
Step 3 From the "Start" menu, select "Devices and Printers" > "Add a Printer".
Step 4 The "Add a Printer" dialogue will be displayed asking "What type of printer do you want to install?" Select "Add a local printer".
Step 5 The "Choose a printer port" dialogue will be displayed. Create a new "Standard TCP/IP Port" and click "Next".
Step 6 Enter the "Device" IP address and uncheck "Query the printer and automatically select the driver to use". Click "Next".
Step 7 The "Install the printer driver" dialogue appears. Click "Have Disk".
Step 8 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
Step 9 Follow the rest of the Wizard's instructions to complete the installation.
 
1-2-2 Windows XP, 2003, Vista, 2008
Step 1 Log in to Windows as an Administrator.
Step 2 Close any open applications.
Step 3 Open "Printers and Faxes" from the Start menu.
Step 4 Select "Add Printer".
Step 5 "Welcome to the Add Printer Wizard" is displayed. Click "Next >".
Step 6 The "Local or Network Printer" dialogue is displayed. Select "Local printer attached to this computer" and click "Next >". Note: Do not enable "Automatically detect and install my Plug and Play printer".
Step 7 The "Select a Printer Port" dialogue is displayed. Select "Create a new port" > "Standard TCP/IP Port" as the port type and click "Next >".
Step 8 The "Add Standard TCP/IP Printer Port Wizard" is displayed. Click "Next >".
Step 9 Enter the device IP address or hostname and click "Next >".
Step 10 The "Install Printer Software" dialogue is displayed. Select "Have Disk".
Step 11 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
Step 12 Follow the rest of the Wizard's instructions to complete the installation.

2. Upgrading the PS Universal printer driver to a newer version

2-1 Upgrading the printer driver from an older version to a newer version:
Note: If upgrading from an earlier version of the driver (Ver.1.00.0 - Ver.3.10.00), the upgrade procedure might result in changes to the values configured for settings such as orientation and layout.
Step 1 Open the "Printers" folder (or "Printers and Faxes") from the "Start" menu or "Control Panel".
Step 2 Open the Properties of the printer to be upgraded.
Step 3 Advanced tab > New Driver button > Next button.
Step 4 Select "Have Disk..." then browse to the folder containing the extracted printer driver INF file. Click Open.
Step 5 Click OK and select the printer model. Click Next.
Step 6 Once the installation is complete, click Finish.
Step 7 Click OK to close the Printer Properties dialog box.
Step 8 Log the current user account off.
 
2-2 Upgrading an x86 driver installed as an "Additional Driver" on an x64 system (and vice versa)
To replace an x86 print driver on an x64 server (and vice versa), the following should be done: 
Step 1 Open the Devices and Printers folder.
Step 2 Select any print queue and open the Print Server Properties window.
Step 3 Select the "Drivers" tab.
Step 4 Remove the x86 PS Universal printer driver files.
Step 5 Select "Remove driver only" and click OK.
Step 6 Click "Add" to install the new version of the x86 PS Universal printer driver.

*We recommend performing a fresh install for any existing PS drivers 
installed for your device.

3. Uninstalling PS Universal printer driver

3-1 Windows 7, Server 2008 R2
Step 1 Log in to Windows as an Administrator.
Step 2 Close any open applications.
Step 3 Open the "Devices and Printers" folder from the "Start" menu.
Step 4 Delete the printer icon corresponding to the driver that is to be uninstalled.
Step 5 File > Server Properties > Driver tab.
Step 6 Click the "Change Driver Settings" button.
Step 7 Select the driver to be uninstalled.
Step 8 Press the Delete key.
Step 9 Log the current user account off.
 
3-2 Windows Vista/Windows Server 2008
Step 1 Log in to Windows as an Administrator.
Step 2 Close any open applications.
Step 3 Click the "Printer" icon in the "Control Panel".
Step 4 Right-click anything in the folder and select "Run as administrator".
Step 5 Delete the printer icon corresponding to the driver that is to be uninstalled.
Step 6 File > Server Properties > Driver tab.
Step 7 Select the driver to be uninstalled.
Step 8 Press the Delete key.
Step 9 Log the current user account off.
 
3-3 Windows XP/Windows Server 2003
Step 1 Log in to Windows as an Administrator.
Step 2 Close any open applications.
Step 3 Click the "Printer" icon in the "Control Panel".
Step 4 Delete the printer icon corresponding to the driver that is to be uninstalled.
Step 5 File > Server Properties > Driver tab.
Step 6 Select the driver to be uninstalled.
Step 7 Press the Delete key.
Step 8 Log the current user account off.


[Notes/Limitations]
1. Note for HP LJ8100 users:
The older Hewlett Packard LaserJet 8100 PCL 6 driver may interfere with 
the PostScript driver. To avoid this problem use LaserJet 8100 PCL6 driver 
V4.3.2.38 or later.

2. Collation:
Collation should only be performed by the driver. 
Do not use application collate functions. Doing so can result in unexpected side effects.

3. A hard disk is required for the following Job Types:
Sample Print, Locked Print, Hold Print, Stored Print, Store and Print, Document Server
Even if the driver is connected to a device that doesn't have a hard disk, the above listed Job Types can still be selected. If a job that uses one of these Job Types is submitted to a printer that doesnft have a hard disk, the job will be cancelled by the printer.

4. IE5 and Sample Printing:
Instead of just 1 sample copy being printed, all copies of Sample Print jobs will be printed. 
Furthermore all of the copies will be stored on the device as a single job.

5. Staple/Punch:
Stapling/punching can be selected even if the job is being output to a tray other than a finisher tray. 
However in this case, the stapling/punching will be cancelled by the printer.

6. Staple/Punch/Z-Folding with Landscape documents:
Staple/punch/z-folding might be out of position if printing Landscape documents. If this occurs, please try any of the following:
  a. Select "Landscape" for the "Orientation Override" setting.
  b. Select "Rotated Landscape" for the "Orientation" setting.
  c. Select "Off" for the "Orientation Override" setting, and enable the "Rotate by 180 degrees" setting.

7. Paper types that require the Bypass tray:
Some paper types such as Labels, Thick, and Transparency, can only be printed from the Bypass Tray. If one of these paper types is to be used, please make sure that the Bypass tray is the output tray. Do not use auto tray selection.

8. Custom Size Setup:
A warning message might be displayed on a PC when Custom paper sizes 
are configured even if the custom paper sizes are within the minimum/maximum 
size limits. Alternatively, a job will be cancelled with no warning message 
shown on the PC if custom paper sizes are NOT within the minimum/maximum size 
limits. In either case, please enlarge/reduce the values to be more/less than 
the entered values even if they are within the available range.

9. Separator Page:
(Windows XP/Server2003/Vista/Server2008/7)
If a Separator Page is selected, some document may not be printed 
as expected.

10. The effect of duplex jobs on the page counter:
Some applications add a blank page to the end of odd-paged duplex jobs. 
This added page might be counted by the page counter.

11. Form To Tray Assignment:
We do not recommend changing any of the settings under the heading "Form To Tray Assignment".

12. Booklet printing with Adobe Acrobat:
The use of the Booklet function with Adobe Acrobat documents might result in anomalies.

13. Preprinted, Prepunched and Letterhead paper types:
If use Preprinted, Prepunched or Letterhead paper types for the printing of 
Landscape document, it might be printed with the unexpected orientation.

14. Simplified Chinese fonts:
The use of multiple Simplified Chinese fonts in the same document might result in anomalies.

15. Chinese editions of PageMaker:
Printing from Chinese editions of PageMaker, require the use of the English PostScript Universal driver.

16. 1200 dpi printing from Visio2002 is not supported:
If anomalies occur, please lower the resolution to 600 dpi.

17. Print From Microsoft Word enabling Slip Sheet:
If print from Microsoft Word enabling Slip Sheet, Slip Sheet feeding may
not be conducted properly. In this case, perform printing after selecting
"Automatically Select" in "Detailed Settings" -> "Menu" -> "Paper" 
-> "Paper Source" -> "Automatically Select".

18. Output Protocol for redirected ports:
If a network port is forwarded to an LPT or USB port, please make sure that the driver's "Output Protocol" is "ASCII".

19. Displayed file names on the operation panel:
Filenames consisting of 2-byte or extended ASCII characters will not be correctly displayed on the operation panel.


20. CMYK used for Black and White Documents:
Black and White documents might be printed in full color (CMYK).
To ensure that the job prints using pure Black (K), please change the 
color mode to "Black and White".

21. Image Smoothing:
When "Image Smoothing" applied to image data with IndexColor mode, 
the printing quality of the image may not be the best.
Please turn "Image Smoothing" off before printing under the circumstances.

22. Do not use "ICM Handled by Printer" with "Output Protocol = TBCP":
If the setting "ICM Method > ICM Handled by Printer" is used with "Output Protocol = TBCP", jobs will be reset.

23. N-up with Full Bleed paper sizes:
The use of Page Layout (N-up) with Full Bleed paper sizes might result in slightly large page images than if a normal paper size were used.

24. Scale to Fit:
(Windows XP/Server2003/Vista/Server2008/7)
When printing from certain applications, the "Scale to Fit" function is 
ineffective if the print data contains images.

25. Enable advanced printing features:
(Windows XP/Server2003/Vista/Server2008/7)
The following features can not be used if "Enable advanced printing 
features" is disabled.
    - Booklet
    - Page Order
    - Draw Border
    - Pages per Sheet Layout
    - Booklet Binding Edge

26. Help pointer ("?" button):
(Windows XP/Server2003)
Nothing is displayed if the help pointer is used on an element in Printing 
Preferences. 
(Windows Vista/Server2008/7)
Nothing is displayed if the help pointer is used on an element in Printing 
Preferences or Printer Properties.

Instead of using the help pointer, please press the "Help" button to get 
information about objects in the driver dialogue.

27. Page Layout (N-up) function:
(Windows XP/Server2003/Vista/Server2008/7)
If "Pages per Sheet" is 2 or more, pages of mixed orientation documents 
might not be rotated in the way that is expected by the customer.
To make pages rotate differently, please do the following:
(1) Open "Printers and Faxes".
(2) Select a printer and open its Properties.
(3) Open the "Advanced" tab and click the "Print Processor..." button.
(4) Select "WinPrint" from the list of print processors.

28. Negative Output function:
The PostScript Universal driver does support the "Negative Output" function. This function is supported by some other PostScript drivers.

29. Default "Current Printer"
(Windows XP/Server2003/Vista/Server2008/7)
Default "Current Printer" is "Aficio MP C7500".

30. Slip Sheets
The PS driver does not support the use of Slip Sheets. 
Even if the device has an interposer, it cannot be configured
as an accessory in the PS driver.

31. Utilities
This driver supports the use of PrinterSwitcher v1.0.2.0 or later.
If the driver's "Automatically Update Printer Information" setting is disabled, device accessories will not be updated automatically. This could cause problems if using PrinterSwitcher.

32. Supported Models

Aficio MP 4000B, Aficio MP 4000, Aficio MP 5000B, Aficio MP 5000, 9040b, 9040, 9050b, 9050, MP 4000B, MP 4000, MP 5000B, MP 5000, MP 4000B/LD040B, MP 4000/LD040, MP 5000B/LD050B, MP 5000/LD050,
Aficio MP 2550B, Aficio MP 2550, Aficio MP 3350B, Aficio MP 3350, 9025b, 9025, 9033b, 9033, MP 2550B, MP 2550, MP 3350B, MP 3350,  MP 2550B/LD425B, MP 2550/LD425, MP 3350B/LD433B,  MP 3350/LD433,
Aficio SP C420DN, CLP131DN, SP C420DN, SP C420DN, LP331cn/SP C420, BPRO 3131CP, IP SP C420DN,
Aficio MP C2500, Aficio MP C3000, C2525, C3030, MPC2500/DSc525, MPC3000/DSc530, MP C2500, MP C3000, ISC 2525, ISC 3030, MP C2500/LD425c, MP C3000/LD430c, Aficio MP C2000, C2020, MPC2000/DSc520, MP C2000, ISC 2020, MP C2000/LD420c,
Aficio MP C3500, Aficio MP C4500, C3535, C4540, MPC3500/DSc535, MPC4500/DSc545, MP C3500, MP C4500, ISC 3535, ISC 4045, MP C3500/LD435c, MP C4500/LD445c,
Aficio SP 8200DN, MLP150DN, SP 8200DN, LP150dn/SP8200DN, SP 8200DN, IP SP 8200DN,
Aficio MP C6000, Aficio MP C7500, C6055, C7570, MP C6000, MP C7500, MP C6000/LD260c, MP C7500/LD275c, Pro C550EX, Pro C700EX,
Aficio MP C2800, Aficio MP C3300, C2828, C3333, MP C2800, MP C3300, MP C2800/LD528C, MP C3300/LD533C,
Aficio MP C4000, Aficio MP C5000, C4040, C5050, MP C4000, MP C5000, MP C4000/LD540C, MP C5000/LD550C,
Aficio MP 161, 816, MP 161/DSm416, MP 161, IS 2416, MP 161/LD016, 

Aficio SP C411DN, Aficio SP C410DN, CLP31DN, CLP27DN, C7531dn, C7526dn, SP C411DN, SP C410DN, IPC 3030DN, IPC 2525DN, LP231c/SP C411, LP226c/SP C410, BPRO 3131CP,
Aficio MP 3500, Aficio MP 4500, MP3500/DSm735e, MP4500/DSm745e, MP 3500, MP 4500, 8035e, 8045e, IS 2435, IS 2445, MP 3500/LD335, MP 4500/LD345,
Aficio MP 2510, Aficio MP 3010, 8025e, 8030e, MP 2510/DSm725e, MP 3010/DSm730e, MP 2510, MP 3010, IS 2425, IS 2430, MP 2510/LD325, MP 3010/LD330,
Aficio AP610N, MLP35n, P7535n, P7535n, LP135n,
Aficio CL7200, Aficio CL7300, CLP128, CLP135, C7528n, C7535n, C7528n, C7535hdn, IPC 2832, IPC 3535e, LP332c, LP335c,
Aficio MP C2050, Aficio MP C2550, C9020, C9025, MP C2050, MP C2550, MP C2050/LD520C, MP C2550/LD525C,
Aficio SP C820DN, Aficio SP C821DN, CLP340D, CLP350D, C8140ND, C8150ND, LP540C/SPC820DN, LP550C/SPC821DN, SP C820DN, SP C821DN,
Aficio SP 4210N, SP 4210N, MLP37N, SP 4210N, LP37N, SP 4210N,

Aficio SP C400DN, SP C400DN, SP C400DN,
Aficio CL3500N, CLP22, C7521n, C7521n, LP222cn/LP221c,
Aficio MP 2000, Aficio MP 1600, 9021d, 9016, MP2000/DSm721d, MP1600/DSm716, MP 2000, MP 1600, IS 2320, IS 2316, MP 2000/LD320d, MP 1600/LD316,
Aficio MP 171, 917, MP 171, MP 171/LD 117,

Aficio SP C811DN, CLP240D, C7640nD, SP C811DN, IPC 4040DN, LP440c/SP C811DN, BPRO 4040CP, IP SP C811DN,
Aficio SP 4100N, Aficio SP 4110N, SP 4100N, SP 4110N, MLP31n, MLP36n, P7031n, P7035n, LP131n, LP136n, BPRO 31MP, 
Aficio SP 4100NL, SP 4100NL, MLP31nL, P7031nL, LP131nL, IP SP 4100NL, IP SP 4100N, IP SP 4110N,
Aficio CL4000DN, Aficio CL4000HDN, CLP26DN, C7425dn, C7425dn, C7425hdn, IPC 2525, IPC 2525e, LP125cx/LP126cn,
Aficio 3035, Aficio 3045, DSm735/735G, DSm745/745G, DSm735, DSm745, 8035/8035g, 8045/8045g, IS 2235, IS 2245, LD235, LD245,
Aficio 3025, Aficio 3030, 8025, 8030, DSm725, DSm730, DSm725, DSm730, IS 2225, IS 2230, LD225, LD230,
Aficio MP 6000, Aficio MP 7000, Aficio MP 8000, 8060, 8070, 8080, MP 6000, MP 7000, MP 8000, MP 6000/LD260,, MP 7000/LD270, MP 8000/LD280,
Aficio MP 6001, Aficio MP 7001, Aficio MP 8001, Aficio MP 9001, 9060, 9070, 9080, 9090, MP 6001, MP 7001, MP 8001, MP 9001, MP 6001/LD360, MP 7001/LD370, MP 8001/LD380, MP 9001/LD390,
Pro 907EX, Pro 1107EX, Pro 1357EX,

Aficio SP 8100DN, MLP145, P7245, LP145n/SP 8100DN, SP 8100DN,
Aficio AP410N, MLP28n, P7527n, P7527n, LP127n/LP128n,
Aficio 3260C, Aficio Color5560, C6045, SDC555, DSc460, CS555, ISC 4560, ISC 5560, LD160c, LC155,
Aficio MP 5500, Aficio MP 6500, Aficio MP 7500, 8055, 8065, 8075, MP5500/DSm755, MP6500/DSm765, MP7500/DSm775, MP 5500/LD255, MP 6500/LD265, MP 7500/LD275, MP 5500, MP 6500, MP 7500, IS 2255, IS 2265, IS 2275,
Aficio 3235C, Aficio 3245C, Aficio 3228C, C3528, C4535, C2824, DSc435, DSc445, DSc428, ISC 2835, ISC 3545, ISC 2428, LD335c, LD345c, LD328c,

Aficio SP 6330N, SP 6330N, MLP235n, SP 6330N, LP235N,
Aficio MP 4001, Aficio MP 5001, 9240, 9250, MP 4001, MP 5001, MP 4001/LD140, MP 5001/LD150,
Aficio MP 2851, Aficio MP 3351, 9228, 9233, MP 2851, MP 3351, MP 2851/LD528, MP 3351/LD533,
Aficio MP C6501, Aficio MP C7501, C9065, C9075, MP C6501, MP C7501, MP C6501/LD365C, MP C7501/LD375C,
Aficio 3224C, Aficio 3232C, C2410, C3210e, DSc424, DSc432, ISC 1024c, ISC 1032c, LD124c, LD132c,
Aficio MP 2500, 7025, MP2500/DSm625, MP 2500, IS 2325, MP2500/LD125,
MP C1500/615C, SGC 1506, MPC1500/GS106, MP C1500sp, ISC 615G, MPC1500/LD215c,
Pro 906EX, Pro 1106EX, Pro 1356EX,
Aficio AP900, MLP75n, P7575, LP175/LP175hdn,

Aficio MP 9000, Aficio MP 1100, Aficio MP 1350, 8090, 8110, 8135, MP9000/Dsm790, MP1100/DSm7110, MP1350/DSm7135, MP 9000/LD1900, MP 1100/LD1100, MP 1350/LD1350, MP 9000, MP 1100, MP 1350, IS 3090, IS 3110, IS 3135,
Aficio 2051, Aficio 2060, Aficio 2075, 4051, 4060, 4075, DSm651, DSm660, DSm750, LD151, LD160, LD175, IS 2151, IS 2160, IS 2175,
Aficio SP 9100DN,
Aficio MP W2400, Aficio MP W3600, 2404WD, 2406WD, GWD2004, GWD2006, LW324, LW326, MP W2400, MP W3600,
Aficio SP W2470, 2404WDP, SP W2470, LP124w, SP W2470,
Aficio SP C430DN, Aficio SP C431DN, CLP37DN, CLP42DN, SP C430DN, SP C431DN, LP137CN, LP142CN, SP C430DN, SP C431DN,

Aficio MP C4501, Aficio MP C5501, Aficio MP C4501A, Aficio MP C5501A, C9145, C9155, C9145A, C9155A, MP C4501, MP C5501, MP C4501A, MP C5501A, MP C4501/LD645C, MP C5501/LD655C, MPC4501A/LD645CA, MPC5501A/LD655CA,
Aficio MP C3001, Aficio MP C3501, C9130, C9135, MP C3001, MP C3501, MP C3001/LD630C, MP C3501/LD635C, MP C3001, MP C3501,
Aficio MP C300, Aficio MP C300SR, Aficio MP C400, Aficio MP C400SR, C 230, C 230SR, C 240, C 240SR, MP C300, MP C300SR, MP C400, MP C400SR, LD 130C, LD 130CSR, LD 140C, LD 140CSR,
Aficio MP W2401, Aficio MP W3601, 3406WD, GWD3006, LW426, MP W2401, MP W3601,

Aficio MP C2051, Aficio MP C2551, C9120, C9125, MP C2051, MP C2551, LD 620C, LD 625C,
Aficio SP C320DN, SP C320DN,

Aficio MP 201, 920, MP 201/LD 220, MP 201,

Aficio SP 4310N, SP4310,

Aficio SP 5200S, Aficio SP 5210SF, Aficio SP 5210SR, SP5200S, SP5210SF, SP5210SR,
Aficio SP 5200DN, Aficio SP 5210DN, SP5200DN, SP5210DN,
Aficio MP 2352, Aficio MP 2852, Aficio MP 3352, MP 2352, MP 2852, MP 3352, MP2352/DSm923, MP2852/DSm928, MP3352/DSm933

33. Supported Models by Generic Model
The use of Generic Model is only supported with the following models:

 Aficio MP 4000B, Aficio MP 4000, Aficio MP 5000B, Aficio MP 5000, 9040b, 9040, 9050b, 9050, MP 4000B, MP 4000, MP 5000B, MP 5000, MP 4000B/LD040B, MP 4000/LD040, MP 5000B/LD050B, MP 5000/LD050,

 Aficio SP 8200DN, MLP150DN, SP 8200DN, LP150dn/SP8200DN, IP SP 8200DN,

 Aficio MP C4000, Aficio MP C5000, C4040, C5050, MP C4000, MP C5000, MP C4000/LD540C, MP C5000/LD550C,

 Aficio SP C820DN, Aficio SP C821DN, CLP340D, CLP350D, C8140ND, C8150ND, LP540C/SPC820DN, LP550C/SPC821DN, SP C820DN, SP C821DN,

 Aficio MP C2800, Aficio MP C3300, C2828, C3333, MP C2800, MP C3300, MP C2800/LD528C, MP C3300/LD533C,

 Aficio MP C2050, Aficio MP C2550, C9020, C9025, MP C2050, MP C2550, MP C2050/LD520C, MP C2550/LD525C,

 Aficio SP C420DN, CLP131DN, SP C420DN, LP331cn/SP C420, 

 Aficio MP 6001, Aficio MP 7001, Aficio MP 8001, Aficio MP 9001, 9060, 9070, 9080, 9090, MP 6001, MP 7001, MP 8001, MP 9001, MP 6001/LD360, MP 7001/LD370, MP 8001/LD380, MP 9001/LD390,

 Aficio MP 2550B, Aficio MP 2550, Aficio MP 3350B, Aficio MP 3350, 9025b, 9025, 9033b, 9033, MP 2550B, MP 2550, MP 3350B, MP 3350, MP 2550B/LD425B, MP 2550/LD425, MP 3350B/LD433B, MP 3350/LD433,

 Aficio MP 171, 917, MP 171, MP 171/LD 117,

 Aficio MP C6000, Aficio MP C7500, C6055, C7570, MP C6000, MP C7500, MP C6000/LD260c, MP C7500/LD275c,

 Pro 907EX, Pro 1107EX, Pro 1357EX,

 Aficio SP 6330N, SP 6330N, MLP235N, SP 6330N, LP235N, SP 6330N,

 Aficio MP 4001, Aficio MP 5001, 9240, 9250, MP4001, MP5001, MP4001/LD140, MP5001/LD150,

 Aficio MP 2851, Aficio MP 3351, 9228, 9233, MP 2851, MP 3351, MP 2851/LD528, MP 3351/LD533,

 Aficio MP C6501, Aficio MP C7501, C9065, C9075, MP C6501, MP C7501, MP C6501/LD365C, MP C7501/LD375C,

 Aficio SP C430DN, Aficio SP C431DN, CLP37DN, CLP42DN, SP C430DN, SP C431DN, LP137CN, LP142CN, SP C430DN, SP C431DN,

 Aficio MP C4501, Aficio MP C5501, Aficio MP C4501A, Aficio MP C5501A, C9145, C9155, C9145A, C9155A, MP C4501, MP C5501, MP C4501A, MP C5501A, MP C4501/LD645C, MP C5501/LD655C, MPC4501A/LD645CA, MPC5501A/LD655CA,

 Aficio MP C3001, Aficio MP C3501, C9130, C9135, MP C3001, MP C3501, MP C3001/LD630C, MP C3501/LD635C, MP C3001, MP C3501,

 Aficio MP C300, Aficio MP C300SR, Aficio MP C400, Aficio MP C400SR, C 230, C 230SR, C 240, C 240SR, MP C300, MP C300SR, MP C400, MP C400SR, LD 130C, LD 130CSR, LD 140C, LD 140CSR,

 Aficio MP W2401, Aficio MP W3601, 3406WD, GWD3006, LW426, MP W2401, MP W3601,

 Aficio MP C2051, Aficio MP C2551, C9120, C9125, MP C2051, MP C2551, LD 620C, LD 625C,

 Aficio SP C320DN, SP C320DN,

 Aficio MP 201, 920, MP 201/LD 220, MP 201,

 Aficio SP 4310N, SP4310,

 Aficio SP 5200S, Aficio SP 5210SF, Aficio SP 5210SR, SP5200S, SP5210SF, SP5210SR,

 Aficio SP 5200DN, Aficio SP 5210DN, SP5200DN, SP5210DN,

 Aficio MP 2352, Aficio MP 2852, Aficio MP 3352, MP 2352, MP 2852, MP 3352, MP2352/DSm923, MP2852/DSm928, MP3352/DSm933

-Using Generic Model the device will default to color/Black and White mode = color. 

34. Enhanced Locked Print NX FlexRelease Sever
In order to print using Enhanced Locked Print NX FlexRelease Sever, the selected model (Printer Selection tab) must be "Generic Model".
