! Sample coating.dat file supplied with ZEMAX
! See ZEMAX manual for complete syntax documentation

! Sample material definitions

MATE AIR
0.55 1.0 0

MATE N15
0.55 1.5 0

MATE AL2O3
.600 1.59 0
1.60 1.56 0

MATE ALUM
.550 0.7 -7.0

MATE ALUM2
.546 0.82 -5.99

MATE BK7
0.4  1.5308485 0
0.46 1.5244335 0
0.5  1.5414145 0
0.7  1.5130640 0
0.8  1.5107762 0
1.0  1.5075022 0
2.0  1.4945016 0

MATE CEF3
.550 1.63 0
2.00 1.59 0

MATE LA2O3
.550 1.95 0
2.00 1.86 0

MATE MGF2
0.4  1.38387 0
0.46 1.38110 0
0.5  1.37978 0
0.7  1.37608 0
0.8  1.37506 0
1.0  1.37358 0
2.0  1.36784 0
2.5  1.36426 0

MATE THF4
.400 1.52 0
.750 1.51 0

MATE ZNS
0.4  2.5571707 0
0.46 2.4579060 0
0.5  2.4190751 0
0.7  2.3317272 0
0.8  2.3131206 0
1.0  2.2922206 0
2.0  2.2859449 0

MATE ZRO2
.550 2.10 0
2.00 2.00 0

! Sample coating definitions

COAT NULL
MGF2 0.0

COAT AR
MGF2 .25

COAT WAR
MGF2 .25
LA2O3 .50

COAT HEAR1
MGF2 .25
ZRO2 .50
CEF3 .25

COAT HEAR2
MGF2  .25
ZNS   .50
AL2O3 .75

COAT GAP
AIR .1

COAT METAL
ALUM2 0.0075092

COAT METAL2
ALUM2 0.04

COAT AIR0010
AIR .01

COAT ETALON
ZNS  .25 0 4
MGF2 .25 0 4
BK7  5000 1 0
MGF2 .25 0 4
ZNS  .25 0 4

COAT FP
ALUM 0.004
AIR 150
ALUM 0.004

! Samples of defining simple ideal coatings using I. format; defines transmitted intensity, rest is assumed to be reflected
! Format: I.transmission

COAT I.05
COAT I.50
COAT I.95
COAT I.98
COAT I.99
COAT I.995
COAT I.99999999

! Sample of defining ideal coatings using IDEAL. Defines transmitted and reflected intensity, rest is assumed to be absorbed
! Format: IDEAL <name> <Transmitted intensity> <Reflected intensity>

IDEAL SPLIT 0.50 0.50

! Sample of defining ideal coatings using IDEAL2. Defines reflected and transmitted complex amplitude for S and P, rest is assumed to be absorbed
! Format: IDEAL <name> s_rr s_ri s_tr s_ti p_rr p_ri p_tr p_ti no_pi_flag

IDEAL2 PASS_P 1.0 0.0 0.0 0.0 0.0 0.0 1.0 0.0 0 

! Sample table coating
! See program manual for complete syntax and important comments

TABLE PASS45
ANGL 0.0
WAVE 0.55 1.0 1.0 0.0 0.0 0.0 0.0 0.0 0.0
ANGL 45.0
WAVE 0.55 0.0 0.0 1.0 1.0 0.0 0.0 0.0 0.0
ANGL 90.0
WAVE 0.55 1.0 1.0 0.0 0.0 0.0 0.0 0.0 0.0

! Sample taper function
TAPR QUAD
RT 2 -.1

! Sample coating using a defined taper
COAT AR_TAPR
MGF2 .25 0 0 QUAD


