Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network

### Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network

To connect your machine to your wireless network, we recommend using the Installer CD-ROM.

- Before Configuring Your Fuji Xerox Machine for a Wireless Network
- Configure Your Machine for a Wireless Network Using a USB Cable
  Connect your Fuji Xerox machine to your wireless network using a USB cable. Once connection is complete, remove the USB cable.
- Configure Your Machine's Wireless Network Using the Fuji Xerox Installer Application without USB Cable
  Wirelessly add your Fuji Xerox Machine to your wireless network.
- Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™
- Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)
  If your wireless LAN access point/router supports WPS, you can use the Personal Identification Number (PIN) Method to configure your wireless network settings.

Go to top of page