f=mxf_d10
top_field_first=1
vcodec=mpeg2video
pix_fmt=yuv422p
minrate=50M
maxrate=50M
vb=50M
g=1
bf=0
flags=+ildct+low_delay
dc=10
flags2=+ivlc+non_linear_q
ps=1
qmin=1
qmax=3
bufsize=2000k
rc_init_occupancy=2000k
rc_buf_aggressivity=0.25

acodec=pcm_s16le

meta.preset.extension=mxf
meta.preset.note=Intra-frame only, 50 Mb/s MPEG-2 also known as Sony IMX or SMPTE 365M
