:Base .\GPWH_ERR.hlp
:Title GX Developer帮助(错误代码一览表)
1 A系列CPU
2 AnN,AnS,A0J2H,A2C
3 [错误代码10-〉17]
4 [错误代码10]INSTRCT CODE ERR.=ERA_10
4 [错误代码11]PARAMETER ERROR=ERA_11
4 [错误代码12]MISSING END INS.=ERA_12
4 [错误代码13]CAN'T EXECUTE(P)=ERA_13
4 [错误代码14]CHK FORMAT ERR.=ERA_14
4 [错误代码15]CAN'T EXECUTE(I)=ERA_15
4 [错误代码16]CASSETTE ERROR=ERA_16
4 [错误代码17]ROM ERR.=ERA_17
3 [错误代码20-〉26]
4 [错误代码20]RAM ERROR=ERA_20
4 [错误代码21]OPE. CIRCUIT ERR.=ERA_21
4 [错误代码22]WDT ERROR=ERA_22
4 [错误代码23]SUB-CPU ERROR=ERA_23
4 [错误代码24]END NOT EXECUTE=ERA_24
4 [错误代码25]WDT ERROR=ERA_25
4 [错误代码26]MAIN CPU DOWN=ERA_26
3 [错误代码31-〉32]
4 [错误代码31]UNIT VERIFY ERR.=ERA_31
4 [错误代码32]FUSE BREAK OFF=ERA_32
3 [错误代码40-〉47]
4 [错误代码40]CONTROL-BUS ERR.=ERA_40
4 [错误代码41]SP. UNIT DOWN=ERA_41
4 [错误代码42]LINK UNIT ERROR=ERA_42
4 [错误代码43]I/O INT. ERROR=ERA_43
4 [错误代码44]SP. UNIT LAY. ERR.=ERA_44
4 [错误代码46]SP. UNIT ERROR=ERA_46
4 [错误代码47]LINK PARA. ERROR=ERA_47
3 [错误代码50-〉70]
4 [错误代码50]OPERATION ERROR=ERA_50
4 [错误代码60]MAIN CPU DOWN=ERA_60
4 [错误代码70]BATTERY ERROR=ERA_70
3 [错误代码80-〉84]
4 [错误代码80]SFC PARA. ERROR=ERA_80
4 [错误代码81]SFC CODE ERROR=ERA_81
4 [错误代码82]SFC STEP OVER=ERA_82
4 [错误代码83]SFC EXE. ERROR=ERA_83
4 [错误代码84]SFC OPE. ERROR=ERA_84
2 AnA
3 [错误代码10-〉16]
4 [错误代码10]INSTRCT CODE ERR.
5 [详细错误代码101]=ERA_101
5 [详细错误代码102]=ERA_102
5 [详细错误代码103]=ERA_103
5 [详细错误代码104]=ERA_104
5 [详细错误代码105]=ERA_105
5 [详细错误代码106]=ERA_106
5 [详细错误代码107]=ERA_107
5 [详细错误代码108]=ERA_108
4 [错误代码11]PARAMETER ERROR
5 [详细错误代码111]=ERA_111
5 [详细错误代码112]=ERA_112
5 [详细错误代码113]=ERA_113
5 [详细错误代码114]=ERA_114
5 [详细错误代码115]=ERA_115
5 [详细错误代码116]=ERA_116
5 [详细错误代码117]=ERA_117
5 [详细错误代码118]=ERA_118
4 [错误代码12]MISSING END INS.
5 [详细错误代码121]=ERA_121
5 [详细错误代码122]=ERA_122
4 [错误代码13]CAN'T EXECUTE(P)
5 [详细错误代码131]=ERA_131
5 [详细错误代码132]=ERA_132
5 [详细错误代码133]=ERA_133
5 [详细错误代码134]=ERA_134
5 [详细错误代码135]=ERA_135
4 [错误代码14]CHK FORMAT ERR.
5 [详细错误代码141]=ERA_141
5 [详细错误代码142]=ERA_142
5 [详细错误代码143]=ERA_143
5 [详细错误代码144]=ERA_144
5 [详细错误代码145]=ERA_145
5 [详细错误代码146]=ERA_146
5 [详细错误代码147]=ERA_147
5 [详细错误代码148]=ERA_148
4 [错误代码15]CAN'T EXECUTE(I)
5 [详细错误代码151]=ERA_151
5 [详细错误代码152]=ERA_152
5 [详细错误代码153]=ERA_153
4 [错误代码16]CASSETTE ERROR
5 [详细错误代码---]=ERA_16-
3 [错误代码20-〉26]
4 [错误代码20]RAM ERROR
5 [详细错误代码201]=ERA_201
5 [详细错误代码202]=ERA_202
5 [详细错误代码203]=ERA_203
5 [详细错误代码204]=ERA_204
4 [错误代码21]OPE. CIRCUIT ERR.
5 [详细错误代码211]=ERA_211
5 [详细错误代码212]=ERA_212
5 [详细错误代码213]=ERA_213
4 [错误代码22]WDT ERROR
5 [详细错误代码---]=ERA_22-
4 [错误代码24]END NOT EXECUTE
5 [详细错误代码241]=ERA_241
4 [错误代码26]MAIN CPU DOWN
5 [详细错误代码---]=ERA_26-
3 [错误代码31-〉32]
4 [错误代码31]UNIT VERIFY ERR.
5 [详细错误代码---]=ERA_31-
4 [错误代码32]FUSE BREAK OFF
5 [详细错误代码---]=ERA_32-
3 [错误代码40-〉47]
4 [错误代码40]CONTROL-BUS ERR.
5 [详细错误代码401]=ERA_401
5 [详细错误代码402]=ERA_402
4 [错误代码41]SP. UNIT DOWN
5 [详细错误代码411]=ERA_411
5 [详细错误代码412]=ERA_412
4 [错误代码42]LINK UNIT ERROR
5 [详细错误代码---]=ERA_42-
4 [错误代码43]I/O INT. ERROR
5 [详细错误代码---]=ERA_43-
4 [错误代码44]SP. UNIT LAY. ERR.
5 [详细错误代码441]=ERA_441
5 [详细错误代码442]=ERA_442
5 [详细错误代码443]=ERA_443
5 [详细错误代码444]=ERA_444
5 [详细错误代码445]=ERA_445
5 [详细错误代码446]=ERA_446
5 [详细错误代码447]=ERA_447
4 [错误代码46]SP. UNIT ERROR
5 [详细错误代码461]=ERA_461
5 [详细错误代码462]=ERA_462
4 [错误代码47]LINK PARA. ERROR
5 [详细错误代码---]=ERA_47-
3 [错误代码50-〉70]
4 [错误代码50]OPERATION ERROR
5 [详细错误代码501]=ERA_501
5 [详细错误代码502]=ERA_502
5 [详细错误代码503]=ERA_503
5 [详细错误代码504]=ERA_504
5 [详细错误代码505]=ERA_505
5 [详细错误代码506]=ERA_506
5 [详细错误代码507]=ERA_507
5 [详细错误代码509]=ERA_509
4 [错误代码60]MAIN CPU DOWN
5 [详细错误代码---]=ERA_60-
4 [错误代码62]MAIN CPU DOWN
5 [详细错误代号---]=ERA_62-
4 [错误代码70]BATTERY ERROR
5 [详细错误代码---]=ERA_70-
3 [错误代码80-〉84]
4 [错误代码80]SFC PARA. ERROR
5 [详细错误代码801]=ERA_801
5 [详细错误代码802]=ERA_802
5 [详细错误代码803]=ERA_803
5 [详细错误代码804]=ERA_804
5 [详细错误代码805]=ERA_805
4 [错误代码81]SFC CODE ERROR
5 [详细错误代码---]=ERA_81-
4 [错误代码82]SFC STEP OVER
5 [详细错误代码---]=ERA_82-
4 [错误代码83]SFC EXE. ERROR
5 [详细错误代码831]=ERA_831
4 [错误代码84]SFC OPE. ERROR
5 [详细错误代码84□]=ERA_840
2 AnU,A2US(H)
3 [错误代码10-〉16]
4 [错误代码10]INSTRCT CODE ERR.
5 [详细错误代码101]=ERA_101
5 [详细错误代码102]=ERA_102
5 [详细错误代码103]=ERA_103
5 [详细错误代码104]=ERA_104
5 [详细错误代码105]=ERA_105
5 [详细错误代码106]=ERA_106
5 [详细错误代码107]=ERA_107
5 [详细错误代码108]=ERA_108
4 [错误代码11]PARAMETER ERROR
5 [详细错误代码111]=ERA_111
5 [详细错误代码112]=ERA_112
5 [详细错误代码113]=ERA_113
5 [详细错误代码114]=ERA_114
5 [详细错误代码115]=ERA_115
5 [详细错误代码116]=ERA_116
5 [详细错误代码117]=ERA_117
5 [详细错误代码118]=ERA_118
4 [错误代码12]MISSING END INS.
5 [详细错误代码121]=ERA_121
5 [详细错误代码122]=ERA_122
5 [详细错误代码123]=ERA_123
5 [详细错误代码124]=ERA_124
4 [错误代码13]CAN'T EXECUTE(P)
5 [详细错误代码131]=ERA_131
5 [详细错误代码132]=ERA_132
5 [详细错误代码133]=ERA_133
5 [详细错误代码134]=ERA_134
5 [详细错误代码135]=ERA_135
4 [错误代码14]CHK FORMAT ERR.
5 [详细错误代码141]=ERA_141
5 [详细错误代码142]=ERA_142
5 [详细错误代码143]=ERA_143
5 [详细错误代码144]=ERA_144
5 [详细错误代码145]=ERA_145
5 [详细错误代码146]=ERA_146
5 [详细错误代码147]=ERA_147
5 [详细错误代码148]=ERA_148
4 [错误代码15]CAN'T EXECUTE(I)
5 [详细错误代码151]=ERA_151
5 [详细错误代码152]=ERA_152
5 [详细错误代码153]=ERA_153
4 [错误代码16]CASSETTE ERROR
5 [详细错误代码---]=ERA_16-
3 [错误代码20-〉26]
4 [错误代码20]RAM ERROR
5 [详细错误代码201]=ERA_201
5 [详细错误代码202]=ERA_202
5 [详细错误代码203]=ERA_203
5 [详细错误代码204]=ERA_204
4 [错误代码21]OPE. CIRCUIT ERR.
5 [详细错误代码211]=ERA_211
5 [详细错误代码212]=ERA_212
5 [详细错误代码213]=ERA_213
4 [错误代码22]WDT ERROR
5 [详细错误代码---]=ERA_22-
4 [错误代码24]END NOT EXECUTE
5 [详细错误代码241]=ERA_241
4 [错误代码26]MAIN CPU DOWN
5 [详细错误代码---]=ERA_26-
3 [错误代码31-〉32]
4 [错误代码31]UNIT VERIFY ERR.
5 [详细错误代码---]=ERA_31-
4 [错误代码32]FUSE BREAK OFF
5 [详细错误代码---]=ERA_32-
3 [错误代码40-〉47]
4 [错误代码40]CONTROL-BUS ERR.
5 [详细错误代码401]=ERA_401
5 [详细错误代码402]=ERA_402
4 [错误代码41]SP. UNIT DOWN
5 [详细错误代码411]=ERA_411
5 [详细错误代码412]=ERA_412
4 [错误代码42]LINK UNIT ERROR
5 [详细错误代码---]=ERA_42_-
4 [错误代码43]I/O INT. ERROR
5 [详细错误代码---]=ERA_43-
4 [错误代码44]SP. UNIT LAY. ERR.
5 [详细错误代码441]=ERA_441
5 [详细错误代码442]=ERA_442
5 [详细错误代码443]=ERA_443
5 [详细错误代码444]=ERA_444
5 [详细错误代码445]=ERA_445
5 [详细错误代码446]=ERA_446
5 [详细错误代码447]=ERA_447
5 [详细错误代码448]=ERA_448
4 [错误代码46]SP. UNIT ERROR
5 [详细错误代码461]=ERA_461
5 [详细错误代码462]=ERA_462
4 [错误代码47]LINK PARA. ERROR
5 [详细错误代码0]=ERA_47_0
5 [详细错误代码470]=ERA_470
5 [详细错误代码471]=ERA_471
5 [详细错误代码472]=ERA_472
5 [详细错误代码473]=ERA_473
5 [详细错误代码474]=ERA_474
5 [详细错误代码475]=ERA_475
5 [详细错误代码476]=ERA_476
3 [错误代码50-〉70]
4 [错误代码50]OPERATION ERROR
5 [详细错误代码501]=ERA_501
5 [详细错误代码502]=ERA_502
5 [详细错误代码503]=ERA_503
5 [详细错误代码504]=ERA_504
5 [详细错误代码505]=ERA_505
5 [详细错误代码506]=ERA_506
5 [详细错误代码507]=ERA_507
5 [详细错误代码509]=ERA_509_
4 [错误代码60]MAIN CPU DOWN
5 [详细错误代码---]=ERA_60-
4 [错误代码62]MAIN CPU DOWN
5 [详细错误代号---]=ERA_62-
4 [错误代码70]BATTERY ERROR
5 [详细错误代码---]=ERA_70-
3 [错误代码80-〉84]
4 [错误代码80]SFC PARA. ERROR
5 [详细错误代码801]=ERA_801
5 [详细错误代码802]=ERA_802
5 [详细错误代码803]=ERA_803
5 [详细错误代码804]=ERA_804
5 [详细错误代码805]=ERA_805
4 [错误代码81]SFC CODE ERROR
5 [详细错误代码---]=ERA_81-
4 [错误代码82]SFC STEP OVER
5 [详细错误代码---]=ERA_82-
4 [错误代码83]SFC EXE. ERROR
5 [详细错误代码831]=ERA_831
4 [错误代码84]SFC OPE. ERROR
5 [详细错误代码84□]=ERA_840
2 AnSH
3 [错误代码10-〉17]
4 [错误代码10]INSTRCT CODE ERR.
5 [详细错误代码---]=ERASH_10-
5 [详细错误代码101]=ERASH_101
5 [详细错误代码103]=ERASH_103
5 [详细错误代码104]=ERASH_104
5 [详细错误代码105]=ERASH_105
4 [错误代码11]PARAMETER ERROR
5 [详细错误代码---]=ERASH_11-
4 [错误代码12]MISSING END INS.
5 [详细错误代码---]=ERASH_12-
4 [错误代码13]CAN'T EXECUTE(P)
5 [详细错误代码---]=ERASH_13-
4 [错误代码14]CHK FORMAT ERR.
5 [详细错误代码---]=ERASH_14-
4 [错误代码15]CAN'T EXECUTE(I)
5 [详细错误代码---]=ERASH_15-
4 [错误代码17]ROM ERR.(仅A1SHCPU)
5 [详细错误代码---]=ERASH_17-
3 [错误代码20-〉25]
4 [错误代码20]RAM ERROR
5 [详细错误代码---]=ERASH_20-
4 [错误代码21]OPE. CIRCUIT ERR.
5 [详细错误代码---]=ERASH_21-
4 [错误代码22]WDT ERROR
5 [详细错误代码---]=ERASH_22-
4 [错误代码24]END NOT EXECUTE
5 [详细错误代码---]=ERASH_24-
4 [错误代码25]WDT ERROR
5 [详细错误代码---]=ERASH_25-
3 [错误代码31-〉32]
4 [错误代码31]UNIT VERIFY ERR.
5 [详细错误代码---]=ERASH_31-
4 [错误代码32]FUSE BREAK OFF
5 [详细错误代码---]=ERASH_32-
3 [错误代码40-〉47]
4 [错误代码40]CONTROL-BUS ERR.
5 [详细错误代码---]=ERASH_40-
4 [错误代码41]SP. UNIT DOWN
5 [详细错误代码---]=ERASH_41-
4 [错误代码43]I/O INT. ERROR
5 [详细错误代码---]=ERASH_43-
4 [错误代码44]SP. UNIT LAY. ERR.
5 [详细错误代码---]=ERASH_44-
4 [错误代码46]SP. UNIT ERROR
5 [详细错误代码---]=ERASH_46-
5 [详细错误代码462]=ERASH_462
4 [错误代码47]LINK PARA. ERROR
5 [详细错误代码---]=ERASH_47-
3 [错误代码50-〉70]
4 [错误代码50]OPERATION ERROR
5 [详细错误代码---]=ERASH_50-
5 [详细错误代码503]=ERASH_503
5 [详细错误代码504]=ERASH_504
5 [详细错误代码509]=ERASH_509
4 [错误代码70]BATTERY ERROR
5 [详细错误代码---]=ERASH_70-
3 [错误代码80-〉84]
4 [错误代码80]SFC PARA. ERROR=ERASH_80
4 [错误代码81]SFC CODE ERROR=ERASH_81
4 [错误代码82]SFC STEP OVER=ERASH_82
4 [错误代码83]SFC EXE. ERROR=ERASH_83
4 [错误代码84]SFC OPE. ERROR=ERASH_84
1 QnA系列CPU
2 [出错号码1000-〉1602]
3 [出错号码1000-〉1012]
4 [出错号码1000]MAIN CPU DOWN=ERQA_1000
4 [出错号码1001]MAIN CPU DOWN=ERQA_1001
4 [出错号码1009]MAIN CPU DOWN=ERQA_1009
4 [出错号码1010]END NOT EXECUTE=ERQA_1010
4 [出错号码1011]END NOT EXECUTE=ERQA_1011
4 [出错号码1012]END NOT EXECUTE=ERQA_1012
3 [出错号码1101-〉1105]
4 [出错号码1101]RAM ERROR=ERQA_1101
4 [出错号码1102]RAM ERROR=ERQA_1102
4 [出错号码1103]RAM ERROR=ERQA_1103
4 [出错号码1104]RAM ERROR=ERQA_1104
4 [出错号码1105]RAM ERROR=ERQA_1105
3 [出错号码1200-〉1206]
4 [出错号码1200]OPE. CIRCUIT ERR.=ERQA_1200
4 [出错号码1201]OPE. CIRCUIT ERR.=ERQA_1201
4 [出错号码1202]OPE. CIRCUIT ERR.=ERQA_1202
4 [出错号码1203]OPE. CIRCUIT ERR.=ERQA_1203
4 [出错号码1204]OPE. CIRCUIT ERR.=ERQA_1204
4 [出错号码1205]OPE. CIRCUIT ERR.=ERQA_1205
4 [出错号码1206]OPE. CIRCUIT ERR.=ERQA_1206
3 [出错号码1300-〉1310]
4 [出错号码1300]FUSE BREAK OFF=ERQA_1300
4 [出错号码1310]I/O INT.ERROR=ERQA_1310
3 [出错号码1401-〉1421]
4 [出错号码1401]SP. UNIT DOWN=ERQA_1401
4 [出错号码1402]SP. UNIT DOWN=ERQA_1402
4 [出错号码1411]CONTROL-BUS.ERR.=ERQA_1411
4 [出错号码1412]CONTROL-BUS.ERR.=ERQA_1412
4 [出错号码1421]SYS. UNIT DOWN=ERQA_1421
3 [出错号码1500-〉1530]
4 [出错号码1500]AC/DC DOWN=ERQA_1500
4 [出错号码1510]DUAL DC DOWN 5V=ERQA_1510
4 [出错号码1520]DC DOWN 5V=ERQA_1520
4 [出错号码1530]DC DOWN 24V=ERQA_1530
3 [出错号码1600-〉1602]
4 [出错号码1600]BATTERY ERROR=ERQA_1600
4 [出错号码1601]BATTERY ERROR=ERQA_1601
4 [出错号码1602]BATTERY ERROR=ERQA_1602
2 [出错号码2000-〉2504]
3 [出错号码2000]
4 [出错号码2000]UNIT VERIFY ERR.=ERQA_2000
3 [出错号码2100-〉2113]
4 [出错号码2100]SP.UNIT LAY ERR.=ERQA_2100
4 [出错号码2101]SP.UNIT LAY ERR.=ERQA_2101
4 [出错号码2102]SP.UNIT LAY ERR.=ERQA_2102
4 [出错号码2103]SP.UNIT LAY ERR.=ERQA_2103
4 [出错号码2104]SP.UNIT LAY ERR.=ERQA_2104
4 [出错号码2105]SP.UNIT LAY ERR.=ERQA_2105
4 [出错号码2106]SP.UNIT LAY ERR.=ERQA_2106
4 [出错号码2107]SP.UNIT LAY ERR.=ERQA_2107
4 [出错号码2108]SP.UNIT LAY ERR.=ERQA_2108
4 [出错号码2109]SP.UNIT LAY ERR.=ERQA_2109
4 [出错号码2110]SP.UNIT ERROR=ERQA_2110
4 [出错号码2111]SP.UNIT ERROR=ERQA_2111
4 [出错号码2112]SP.UNIT ERROR=ERQA_2112
4 [出错号码2113]SP.UNIT ERROR=ERQA_2113
3 [出错号码2200-〉2210]
4 [出错号码2200]MISSING PARA.=ERQA_2200
4 [出错号码2210]BOOT ERROR=ERQA_2210
3 [出错号码2300-〉2302]
4 [出错号码2300]ICM. OPE. ERROR=ERQA_2300
4 [出错号码2301]ICM. OPE. ERROR=ERQA_2301
4 [出错号码2302]ICM. OPE. ERROR=ERQA_2302
3 [出错号码2400-〉2413]
4 [出错号码2400]FILE SET ERROR=ERQA_2400
4 [出错号码2401]FILE SET ERROR=ERQA_2401
4 [出错号码2402]FILE SET ERROR=ERQA_2402
4 [出错号码2410]FILE OPE. ERROR=ERQA_2410
4 [出错号码2411]FILE OPE. ERROR=ERQA_2411
4 [出错号码2412]FILE OPE. ERROR=ERQA_2412
4 [出错号码2413]FILE OPE. ERROR=ERQA_2413
3 [出错号码2500-〉2504]
4 [出错号码2500]CAN'T EXE. PRG.=ERQA_2500
4 [出错号码2501]CAN'T EXE. PRG.=ERQA_2501
4 [出错号码2502]CAN'T EXE. PRG.=ERQA_2502
4 [出错号码2503]CAN'T EXE. PRG.=ERQA_2503
4 [出错号码2504]CAN'T EXE. PRG.=ERQA_2504
2 [出错号码3000-〉3203]
3 [出错号码3000-〉3004]
4 [出错号码3000]PARAMETER ERROR=ERQA_3000
4 [出错号码3001]PARAMETER ERROR=ERQA_3001
4 [出错号码3002]PARAMETER ERROR=ERQA_3002
4 [出错号码3003]PARAMETER ERROR=ERQA_3003
4 [出错号码3004]PARAMETER ERROR=ERQA_3004
3 [出错号码3100-〉3107]
4 [出错号码3100]LINK PARA.ERROR=ERQA_3100
4 [出错号码3101]LINK PARA.ERROR=ERQA_3101
4 [出错号码3102]LINK PARA.ERROR=ERQA_3102
4 [出错号码3103]LINK PARA.ERROR=ERQA_3103
4 [出错号码3104]LINK PARA.ERROR=ERQA_3104
4 [出错号码3105]LINK PARA.ERROR=ERQA_3105
4 [出错号码3107]LINK PARA.ERROR=ERQA_3107
3 [出错号码3200-〉3203]
4 [出错号码3200]SFC PARA. ERROR=ERQA_3200
4 [出错号码3201]SFC PARA. ERROR=ERQA_3201
4 [出错号码3202]SFC PARA. ERROR=ERQA_3202
4 [出错号码3203]SFC PARA. ERROR=ERQA_3203
2 [出错号码4000-〉4633]
3 [出错号码4000-〉4030]
4 [出错号码4000]INSTRCT.CODE ERR.=ERQA_4000
4 [出错号码4001]INSTRCT.CODE ERR.=ERQA_4001
4 [出错号码4002]INSTRCT.CODE ERR.=ERQA_4002
4 [出错号码4003]INSTRCT.CODE ERR.=ERQA_4003
4 [出错号码4004]INSTRCT.CODE ERR.=ERQA_4004
4 [出错号码4010]MISSING END INS.=ERQA_4010
4 [出错号码4020]CAN'T SET(P)=ERQA_4020
4 [出错号码4021]CAN'T SET(P)=ERQA_4021
4 [出错号码4030]CAN'T SET(I)=ERQA_4030
3 [出错号码4100-〉4108]
4 [出错号码4100]OPERATION ERROR=ERQA_4100
4 [出错号码4101]OPERATION ERROR=ERQA_4101
4 [出错号码4102]OPERATION ERROR=ERQA_4102
4 [出错号码4103]OPERATION ERROR=ERQA_4103
4 [出错号码4104]OPERATION ERROR=ERQA_4104
4 [出错号码4107]OPERATION ERROR=ERQA_4107
4 [出错号码4108]OPERATION ERROR=ERQA_4108
3 [出错号码4200-〉4235]
4 [出错号码4200]FOR NEXT ERROR=ERQA_4200
4 [出错号码4201]FOR NEXT ERROR=ERQA_4201
4 [出错号码4202]FOR NEXT ERROR=ERQA_4202
4 [出错号码4203]FOR NEXT ERROR=ERQA_4203
4 [出错号码4210]CAN'T EXECUTE(P)=ERQA_4210
4 [出错号码4211]CAN'T EXECUTE(P)=ERQA_4211
4 [出错号码4212]CAN'T EXECUTE(P)=ERQA_4212
4 [出错号码4213]CAN'T EXECUTE(P)=ERQA_4213
4 [出错号码4220]CAN'T EXECUTE(I)=ERQA_4220
4 [出错号码4221]CAN'T EXECUTE(I)=ERQA_4221
4 [出错号码4223]CAN'T EXECUTE(I)=ERQA_4223
4 [出错号码4230]INST. FORMAT ERR.=ERQA_4230
4 [出错号码4231]INST. FORMAT ERR.=ERQA_4231
4 [出错号码4235]INST. FORMAT ERR.=ERQA_4235
3 [出错号码4300-〉4301]
4 [出错号码4300]EXTENDINST. ERR.=ERQA_4300
4 [出错号码4301]EXTENDINST. ERR.=ERQA_4301
3 [出错号码4400-〉4422]
4 [出错号码4400]SFCP. CODE ERROR=ERQA_4400
4 [出错号码4410]CAN'T SET(BL)=ERQA_4410
4 [出错号码4411]CAN'T SET(BL)=ERQA_4411
4 [出错号码4420]CAN'T SET(S)=ERQA_4420
4 [出错号码4421]CAN'T SET(S)=ERQA_4421
4 [出错号码4422]CAN'T SET(S)=ERQA_4422
3 [出错号码4500-〉4504]
4 [出错号码4500]SFCP. FORMAT ERR.=ERQA_4500
4 [出错号码4501]SFCP. FORMAT ERR.=ERQA_4501
4 [出错号码4502]SFCP. FORMAT ERR.=ERQA_4502
4 [出错号码4503]SFCP. FORMAT ERR.=ERQA_4503
4 [出错号码4504]SFCP. FORMAT ERR.=ERQA_4504
3 [出错号码4600-〉4633]
4 [出错号码4600]SFCP. OPE. ERROR=ERQA_4600
4 [出错号码4601]SFCP. OPE. ERROR=ERQA_4601
4 [出错号码4602]SFCP. OPE. ERROR=ERQA_4602
4 [出错号码4610]SFCP. EXE. ERROR=ERQA_4610
4 [出错号码4611]SFCP. EXE. ERROR=ERQA_4611
4 [出错号码4620]BLOCK EXE. ERROR=ERQA_4620
4 [出错号码4621]BLOCK EXE. ERROR=ERQA_4621
4 [出错号码4630]STEP EXE. ERROR=ERQA_4630
4 [出错号码4631]STEP EXE. ERROR=ERQA_4631
4 [出错号码4632]STEP EXE. ERROR=ERQA_4632
4 [出错号码4633]STEP EXE. ERROR=ERQA_4633
3 [出错号码5000-〉5011]
4 [出错号码5000]WDT ERROR=ERQA_5000
4 [出错号码5001]WDT ERROR=ERQA_5001
4 [出错号码5010]PRG. TIME OVER=ERQA_5010
4 [出错号码5011]PRG. TIME OVER=ERQA_5011
3 [出错号码6000-〉6230]
4 [出错号码6000]PRG.VERIFY ERR.=ERQA_6000
4 [出错号码6010]MODE. VERIFY ERR.=ERQA_6010
4 [出错号码6100]TRUCKIN ERR.=ERQA_6100
4 [出错号码6101]TRUCKIN ERR.=ERQA_6101
4 [出错号码6200]CONTROL EXE.=ERQA_6200
4 [出错号码6210]CONTROL WAIT=ERQA_6210
4 [出错号码6220]CAN'T EXE CHANGE=ERQA_6220
4 [出错号码6221]CAN'T EXE CHANGE=ERQA_6221
4 [出错号码6222]CAN'T EXE CHANGE=ERQA_6222
4 [出错号码6230]DUAL SYS ERROR=ERQA_6230
3 [出错号码9000-〉9010]
4 [出错号码9000]F****=ERQA_9000
4 [出错号码9010]<CHK>ERR***_***=ERQA_9010
1 Q系列CPU(A模式)
2 [错误代码10-〉16]
3 [错误代码10]INSTRCT CODE ERR.
4 [详细错误代码101]=ERQ_A_101
4 [详细错误代码102]=ERQ_A_102
4 [详细错误代码103]=ERQ_A_103
4 [详细错误代码104]=ERQ_A_104
4 [详细错误代码105]=ERQ_A_105
4 [详细错误代码106]=ERQ_A_106
4 [详细错误代码107]=ERQ_A_107
4 [详细错误代码108]=ERQ_A_108
3 [错误代码11]PARAMETER ERROR
4 [详细错误代码111]=ERQ_A_111
4 [详细错误代码112]=ERQ_A_112
4 [详细错误代码113]=ERQ_A_113
4 [详细错误代码114]=ERQ_A_114
4 [详细错误代码115]=ERQ_A_115
4 [详细错误代码116]=ERQ_A_116
4 [详细错误代码117]=ERQ_A_117
4 [详细错误代码118]=ERQ_A_118
3 [错误代码12]MISSING END INS.
4 [详细错误代码121]=ERQ_A_121
4 [详细错误代码122]=ERQ_A_122
4 [详细错误代码123]=ERQ_A_123
4 [详细错误代码124]=ERQ_A_124
3 [错误代码13]CAN'T EXECUTE(P)
4 [详细错误代码131]=ERQ_A_131
4 [详细错误代码132]=ERQ_A_132
4 [详细错误代码133]=ERQ_A_133
4 [详细错误代码134]=ERQ_A_134
4 [详细错误代码135]=ERQ_A_135
3 [错误代码14]CHK FORMAT ERR.
4 [详细错误代码141]=ERQ_A_141
4 [详细错误代码142]=ERQ_A_142
4 [详细错误代码143]=ERQ_A_143
4 [详细错误代码144]=ERQ_A_144
4 [详细错误代码145]=ERQ_A_145
4 [详细错误代码146]=ERQ_A_146
4 [详细错误代码147]=ERQ_A_147
4 [详细错误代码148]=ERQ_A_148
3 [错误代码15]CAN'T EXECUTE(I)
4 [详细错误代码151]=ERQ_A_151
4 [详细错误代码152]=ERQ_A_152
4 [详细错误代码153]=ERQ_A_153
3 [错误代码16]MEMORYCARD ERROR
4 [详细错误代码---]=ERQ_A_16-
2 [错误代码20-〉26]
3 [错误代码20]RAM ERROR
4 [详细错误代码201]=ERQ_A_201
4 [详细错误代码202]=ERQ_A_202
4 [详细错误代码203]=ERQ_A_203
4 [详细错误代码204]=ERQ_A_204
3 [错误代码21]OPE. CIRCUIT ERR.
4 [详细错误代码211]=ERQ_A_211
4 [详细错误代码212]=ERQ_A_212
4 [详细错误代码213]=ERQ_A_213
3 [错误代码22]WDT ERROR
4 [详细错误代码---]=ERQ_A_22-
3 [错误代码24]END NOT EXECUTE
4 [详细错误代码241]=ERQ_A_241
3 [错误代码26]MAIN CPU DOWN
4 [详细错误代码---]=ERQ_A_26-
2 [错误代码31-〉32]
3 [错误代码31]UNIT VERIFY ERR.
4 [详细错误代码---]=ERQ_A_31-
3 [错误代码32]FUSE BREAK OFF
4 [详细错误代码---]=ERQ_A_32-
2 [错误代码40-〉47]
3 [错误代码40]CONTROL-BUS ERR.
4 [详细错误代码401]=ERQ_A_401
4 [详细错误代码402]=ERQ_A_402
4 [详细错误代码403]=ERQ_A_403
4 [详细错误代码405]=ERQ_A_405
3 [错误代码41]SP. UNIT DOWN
4 [详细错误代码411]=ERQ_A_411
4 [详细错误代码412]=ERQ_A_412
3 [错误代码42]LINK UNIT ERROR
4 [详细错误代码---]=ERQ_A_42-
3 [错误代码43]I/O INT. ERROR
4 [详细错误代码---]=ERQ_A_43-
3 [错误代码44]SP. UNIT LAY. ERR.
4 [详细错误代码441]=ERQ_A_441
4 [详细错误代码442]=ERQ_A_442
4 [详细错误代码443]=ERQ_A_443
4 [详细错误代码444]=ERQ_A_444
4 [详细错误代码445]=ERQ_A_445
4 [详细错误代码446]=ERQ_A_446
4 [详细错误代码447]=ERQ_A_447
4 [详细错误代码448]=ERQ_A_448
4 [详细错误代码449]=ERQ_A_449
3 [错误代码46]SP. UNIT ERROR
4 [详细错误代码461]=ERQ_A_461
4 [详细错误代码462]=ERQ_A_462
3 [错误代码47]LINK PARA. ERROR
4 [详细错误代码--]=ERQ_A_47-
4 [详细错误代码470]=ERQ_A_470
4 [详细错误代码471]=ERQ_A_471
4 [详细错误代码472]=ERQ_A_472
4 [详细错误代码473]=ERQ_A_473
4 [详细错误代码474]=ERQ_A_474
4 [详细错误代码475]=ERQ_A_475
4 [详细错误代码476]=ERQ_A_476
2 [错误代码50-〉70]
3 [错误代码50]OPERATION ERROR
4 [详细错误代码501]=ERQ_A_501
4 [详细错误代码502]=ERQ_A_502
4 [详细错误代码503]=ERQ_A_503
4 [详细错误代码504]=ERQ_A_504
4 [详细错误代码505]=ERQ_A_505
4 [详细错误代码506]=ERQ_A_506
4 [详细错误代码507]=ERQ_A_507
4 [详细错误代码509]=ERQ_A_509
3 [错误代码60]MAIN CPU DOWN
4 [详细错误代码---]=ERQ_A_60-
3 [错误代码61]MAIN CPU DOWN
4 [详细错误代码---]=ERQ_A_61-
3 [错误代码62]MAIN CPU DOWN
4 [详细错误代号---]=ERQ_A_62-
3 [错误代码70]BATTERY ERROR
4 [详细错误代码---]=ERQ_A_70-
1 Q系列CPU(Q模式)
2 [出错代码1000-〉1610]
3 [出错代码1000-〉1035]
4 [出错代码1000]MAIN CPU DOWN=ERQ-Q_1000
4 [出错代码1001]MAIN CPU DOWN=ERQ-Q_1001
4 [出错代码1002]MAIN CPU DOWN=ERQ-Q_1002
4 [出错代码1003]MAIN CPU DOWN=ERQ-Q_1003
4 [出错代码1004]MAIN CPU DOWN=ERQ-Q_1004
4 [出错代码1005]MAIN CPU DOWN=ERQ-Q_1005
4 [出错代码1006]MAIN CPU DOWN=ERQ-Q_1006
4 [出错代码1007]MAIN CPU DOWN=ERQ-Q_1007
4 [出错代码1008]MAIN CPU DOWN=ERQ-Q_1008
4 [出错代码1009]MAIN CPU DOWN=ERQ-Q_1009
4 [出错代码1010]END NOT EXECUTE=ERQ-Q_1010
4 [出错代码1020]SFCP. END ERROR=ERQ-Q_1020
4 [出错代码1035]MAIN CPU DOWN=ERQ-Q_1035
3 [出错代码1101-〉1164]
4 [出错代码1101]RAM ERROR=ERQ-Q_1101
4 [出错代码1102]RAM ERROR=ERQ-Q_1102
4 [出错代码1103]RAM ERROR=ERQ-Q_1103
4 [出错代码1104]RAM ERROR=ERQ-Q_1104
4 [出错代码1105]RAM ERROR=ERQ-Q_1105
4 [出错代码1106]RAM ERROR=ERQ-Q_1106
4 [出错代码1107]RAM ERROR=ERQ-Q_1107
4 [出错代码1108]RAM ERROR=ERQ-Q_1108
4 [出错代码1109]RAM ERROR=ERQ-Q_1109
4 [出错代码1110]TRK. CIR. ERROR=ERQ-Q_1110
4 [出错代码1111]TRK. CIR. ERROR=ERQ-Q_1111
4 [出错代码1112]TRK. CIR. ERROR=ERQ-Q_1112
4 [出错代码1113]TRK. CIR. ERROR=ERQ-Q_1113
4 [出错代码1115]TRK. CIR. ERROR=ERQ-Q_1115
4 [出错代码1116]TRK. CIR. ERROR=ERQ-Q_1116
4 [出错代码1150]RAM ERROR=ERQ-Q_1150
4 [出错代码1160]RAM ERROR=ERQ-Q_1160
4 [出错代码1161]RAM ERROR=ERQ-Q_1161
4 [出错代码1162]RAM ERROR=ERQ-Q_1162
4 [出错代码1164]RAM ERROR=ERQ-Q_1164
3 [出错代码1200-〉1205]
4 [出错代码1200]OPE. CIRCUIT ERR.=ERQ-Q_1200
4 [出错代码1201]OPE. CIRCUIT ERR.=ERQ-Q_1201
4 [出错代码1202]OPE. CIRCUIT ERR.=ERQ-Q_1202
4 [出错代码1203]OPE. CIRCUIT ERR.=ERQ-Q_1203
4 [出错代码1204]OPE. CIRCUIT ERR.=ERQ-Q_1204
4 [出错代码1205]OPE. CIRCUIT ERR.=ERQ-Q_1205
3 [出错代码1300-〉1321]
4 [出错代码1300]FUSE BREAK OFF=ERQ-Q_1300
4 [出错代码1310]I/O INT. ERROR=ERQ-Q_1310
4 [出错代码1311]I/O INT. ERROR=ERQ-Q_1311
4 [出错代码1320]LAN CTRL. DOWN=ERQ-Q_1320
4 [出错代码1321]LAN CTRL. DOWN=ERQ-Q_1321
3 [出错代码1401-〉1439]
4 [出错代码1401]SP. UNIT DOWN=ERQ-Q_1401
4 [出错代码1402]SP. UNIT DOWN=ERQ-Q_1402
4 [出错代码1403]SP. UNIT DOWN=ERQ-Q_1403
4 [出错代码1411]CONTROL-BUS. ERR.=ERQ-Q_1411
4 [出错代码1412]CONTROL-BUS. ERR.=ERQ-Q_1412
4 [出错代码1413]CONTROL-BUS. ERR.=ERQ-Q_1413
4 [出错代码1414]CONTROL-BUS. ERR.=ERQ-Q_1414
4 [出错代码1415]CONTROL-BUS. ERR.=ERQ-Q_1415
4 [出错代码1416]CONTROL-BUS. ERR.=ERQ-Q_1416
4 [出错代码1417]CONTROL-BUS. ERR.=ERQ-Q_1417
4 [出错代码1418]CONTROL-BUS. ERR.=ERQ-Q_1418
4 [出错代码1430]MULTI-C.BUS ERR.=ERQ-Q_1430
4 [出错代码1431]MULTI-C.BUS ERR.=ERQ-Q_1431
4 [出错代码1432]MULTI-C.BUS ERR.=ERQ-Q_1432
4 [出错代码1433]MULTI-C.BUS ERR.=ERQ-Q_1433
4 [出错代码1434]MULTI-C.BUS ERR.=ERQ-Q_1434
4 [出错代码1435]MULTI-C.BUS ERR.=ERQ-Q_1435
4 [出错代码1436]MULTI-C.BUS ERR.=ERQ-Q_1436
4 [出错代码1437]MULTI-C.BUS ERR.=ERQ-Q_1437
4 [出错代码1439]MULTI-C.BUS ERR.=ERQ-Q_1439
3 [出错代码1500-〉1520]
4 [出错代码1500]AC/DC DOWN=ERQ-Q_1500
4 [出错代码1510]SINGLE PS.DOWN=ERQ-Q_1510
4 [出错代码1520]SINGLE PS.ERROR=ERQ-Q_1520
3 [出错代码1600-〉1610]
4 [出错代码1600]BATTERY ERROR=ERQ-Q_1600
4 [出错代码1601]BATTERY ERROR=ERQ-Q_1601
4 [出错代码1610]FLASH ROM ERROR=ERQ-Q_1610
2 [出错代码2000-〉2710]
3 [出错代码2000-〉2020]
4 [出错代码2000]UNIT VERIFY ERR.=ERQ-Q_2000
4 [出错代码2001]UNIT VERIFY ERR.=ERQ-Q_2001
4 [出错代码2010]BASE LAY ERROR=ERQ-Q_2010
4 [出错代码2011]BASE LAY ERROR=ERQ-Q_2011
4 [出错代码2012]BASE LAY ERROR=ERQ-Q_2012
4 [出错代码2013]BASE LAY ERROR=ERQ-Q_2013
4 [出错代码2020]EXT.CABLE ERR.=ERQ-Q_2020
3 [出错代码2100-〉2151]
4 [出错代码2100]SP.UNIT LAY ERR.=ERQ-Q_2100
4 [出错代码2101]SP.UNIT LAY ERR.=ERQ-Q_2101
4 [出错代码2102]SP.UNIT LAY ERR.=ERQ-Q_2102
4 [出错代码2103]SP.UNIT LAY ERR.=ERQ-Q_2103
4 [出错代码2106]SP.UNIT LAY ERR.=ERQ-Q_2106
4 [出错代码2107]SP.UNIT LAY ERR.=ERQ-Q_2107
4 [出错代码2108]SP.UNIT LAY ERR.=ERQ-Q_2108
4 [出错代码2110]SP.UNIT ERROR=ERQ-Q_2110
4 [出错代码2111]SP.UNIT ERROR=ERQ-Q_2111
4 [出错代码2112]SP.UNIT ERROR=ERQ-Q_2112
4 [出错代码2113]SP.UNIT ERROR=ERQ-Q_2113
4 [出错代码2114]SP.UNIT ERROR=ERQ-Q_2114
4 [出错代码2115]SP.UNIT ERROR=ERQ-Q_2115
4 [出错代码2116]SP.UNIT ERROR=ERQ-Q_2116
4 [出错代码2117]SP.UNIT ERROR=ERQ-Q_2117
4 [出错代码2118]SP.UNIT ERROR=ERQ-Q_2118
4 [出错代码2120]SP.UNIT LAY ERR.=ERQ-Q_2120
4 [出错代码2121]SP.UNIT LAY ERR.=ERQ-Q_2121
4 [出错代码2122]SP.UNIT LAY ERR.=ERQ-Q_2122
4 [出错代码2124]SP.UNIT LAY ERR.=ERQ-Q_2124
4 [出错代码2125]SP.UNIT LAY ERR.=ERQ-Q_2125
4 [出错代码2126]SP.UNIT LAY ERR.=ERQ-Q_2126
4 [出错代码2128]SP.UNIT LAY ERR.=ERQ-Q_2128
4 [出错代码2150]SP.UNIT VER.ERR.=ERQ-Q_2150
4 [出错代码2151]SP.UNIT VER.ERR.=ERQ-Q_2151
3 [出错代码2200-〉2227]
4 [出错代码2200]MISSING PARA.=ERQ-Q_2200
4 [出错代码2210]BOOT ERROR=ERQ-Q_2210
4 [出错代码2211]BOOT ERROR=ERQ-Q_2211
4 [出错代码2220]RESTORE ERROR=ERQ-Q_2220
4 [出错代码2221]RESTORE ERROR=ERQ-Q_2221
4 [出错代码2225]RESTORE ERROR=ERQ-Q_2225
4 [出错代码2226]RESTORE ERROR=ERQ-Q_2226
4 [出错代码2227]RESTORE ERROR=ERQ-Q_2227
3 [出错代码2300-〉2302]
4 [出错代码2300]ICM. OPE. ERROR=ERQ-Q_2300
4 [出错代码2301]ICM. OPE. ERROR=ERQ-Q_2301
4 [出错代码2302]ICM. OPE. ERROR=ERQ-Q_2302
3 [出错代码2400-〉2413]
4 [出错代码2400]FILE SET ERROR=ERQ-Q_2400
4 [出错代码2401]FILE SET ERROR=ERQ-Q_2401
4 [出错代码2410]FILE OPE. ERROR=ERQ-Q_2410
4 [出错代码2411]FILE OPE. ERROR=ERQ-Q_2411
4 [出错代码2412]FILE OPE. ERROR=ERQ-Q_2412
4 [出错代码2413]FILE OPE. ERROR=ERQ-Q_2413
3 [出错代码2500-〉2710]
4 [出错代码2500]CAN'T EXE. PRG.=ERQ-Q_2500
4 [出错代码2501]CAN'T EXE. PRG.=ERQ-Q_2501
4 [出错代码2502]CAN'T EXE. PRG.=ERQ-Q_2502
4 [出错代码2503]CAN'T EXE. PRG.=ERQ-Q_2503
4 [出错代码2504]CAN'T EXE. PRG.=ERQ-Q_2504
4 [出错代码2700]REMOTE PASS. FAIL=ERQ-Q_2700
4 [出错代码2710]SNTP OPE. ERROR=ERQ-Q_2710
2 [出错代码3000-〉3401]
3 [出错代码3000-〉3042]
4 [出错代码3000]PARAMETER ERROR=ERQ-Q_3000
4 [出错代码3001]PARAMETER ERROR=ERQ-Q_3001
4 [出错代码3002]PARAMETER ERROR=ERQ-Q_3002
4 [出错代码3003]PARAMETER ERROR=ERQ-Q_3003
4 [出错代码3004]PARAMETER ERROR=ERQ-Q_3004
4 [出错代码3005]PARAMETER ERROR=ERQ-Q_3005
4 [出错代码3006]PARAMETER ERROR=ERQ-Q_3006
4 [出错代码3007]PARAMETER ERROR=ERQ-Q_3007
4 [出错代码3009]PARAMETER ERROR=ERQ-Q_3009
4 [出错代码3010]PARAMETER ERROR=ERQ-Q_3010
4 [出错代码3012]PARAMETER ERROR=ERQ-Q_3012
4 [出错代码3013]PARAMETER ERROR=ERQ-Q_3013
4 [出错代码3014]PARAMETER ERROR=ERQ-Q_3014
4 [出错代码3015]PARAMETER ERROR=ERQ-Q_3015
4 [出错代码3016]PARAMETER ERROR=ERQ-Q_3016
4 [出错代码3040]PARAMETER ERROR=ERQ-Q_3040
4 [出错代码3041]PARAMETER ERROR=ERQ-Q_3041
4 [出错代码3042]PARAMETER ERROR=ERQ-Q_3042
3 [出错代码3100-〉3107]
4 [出错代码3100]LINK PARA. ERROR=ERQ-Q_3100
4 [出错代码3101]LINK PARA. ERROR=ERQ-Q_3101
4 [出错代码3102]LINK PARA. ERROR=ERQ-Q_3102
4 [出错代码3103]LINK PARA. ERROR=ERQ-Q_3103
4 [出错代码3104]LINK PARA. ERROR=ERQ-Q_3104
4 [出错代码3105]LINK PARA. ERROR=ERQ-Q_3105
4 [出错代码3106]LINK PARA. ERROR=ERQ-Q_3106
4 [出错代码3107]LINK PARA. ERROR=ERQ-Q_3107
3 [出错代码3200-〉3203]
4 [出错代码3200]SFC PARA. ERROR=ERQ-Q_3200
4 [出错代码3201]SFC PARA. ERROR=ERQ-Q_3201
4 [出错代码3202]SFC PARA. ERROR=ERQ-Q_3202
4 [出错代码3203]SFC PARA. ERROR=ERQ-Q_3203
3 [出错代码3300-〉3303]
4 [出错代码3300]SP.PARA ERROR=ERQ-Q_3300
4 [出错代码3301]SP.PARA ERROR=ERQ-Q_3301
4 [出错代码3302]SP.PARA ERROR=ERQ-Q_3302
4 [出错代码3303]SP.PARA ERROR=ERQ-Q_3303
3 [出错代码3400-〉3401]
4 [出错代码3400]REMOTE PASS.ERR.=ERQ-Q_3400
4 [出错代码3401]REMOTE PASS.ERR.=ERQ-Q_3401
2 [出错代码4000-〉10000]
3 [出错代码4000-〉4030]
4 [出错代码4000]INSTRCT. CODE ERR=ERQ-Q_4000
4 [出错代码4001]INSTRCT. CODE ERR=ERQ-Q_4001
4 [出错代码4002]INSTRCT. CODE ERR=ERQ-Q_4002
4 [出错代码4003]INSTRCT. CODE ERR=ERQ-Q_4003
4 [出错代码4004]INSTRCT. CODE ERR=ERQ-Q_4004
4 [出错代码4010]MISSING END INS.=ERQ-Q_4010
4 [出错代码4020]CAN'T SET(P)=ERQ-Q_4020
4 [出错代码4021]CAN'T SET(P)=ERQ-Q_4021
4 [出错代码4030]CAN'T SET(I)=ERQ-Q_4030
3 [出错代码4100-〉4141]
4 [出错代码4100]OPERATION ERROR=ERQ-Q_4100
4 [出错代码4101]OPERATION ERROR=ERQ-Q_4101
4 [出错代码4102]OPERATION ERROR=ERQ-Q_4102
4 [出错代码4103]OPERATION ERROR=ERQ-Q_4103
4 [出错代码4105]OPERATION ERROR=ERQ-Q_4105
4 [出错代码4107]OPERATION ERROR=ERQ-Q_4107
4 [出错代码4109]OPERATION ERROR=ERQ-Q_4109
4 [出错代码4111]OPERATION ERROR=ERQ-Q_4111
4 [出错代码4112]OPERATION ERROR=ERQ-Q_4112
4 [出错代码4113]OPERATION ERROR=ERQ-Q_4113
4 [出错代码4120]OPERATION ERROR=ERQ-Q_4120
4 [出错代码4121]OPERATION ERROR=ERQ-Q_4121
4 [出错代码4122]OPERATION ERROR=ERQ-Q_4122
4 [出错代码4130]OPERATION ERROR=ERQ-Q_4130
4 [出错代码4131]OPERATION ERROR=ERQ-Q_4131
4 [出错代码4140]OPERATION ERROR=ERQ-Q_4140
4 [出错代码4141]OPERATION ERROR=ERQ-Q_4141
3 [出错代码4200-〉4355]
4 [出错代码4200]FOR-NEXT ERROR=ERQ-Q_4200
4 [出错代码4201]FOR-NEXT ERROR=ERQ-Q_4201
4 [出错代码4202]FOR-NEXT ERROR=ERQ-Q_4202
4 [出错代码4203]FOR-NEXT ERROR=ERQ-Q_4203
4 [出错代码4210]CAN'T EXECUTE(P)=ERQ-Q_4210
4 [出错代码4211]CAN'T EXECUTE(P)=ERQ-Q_4211
4 [出错代码4212]CAN'T EXECUTE(P)=ERQ-Q_4212
4 [出错代码4213]CAN'T EXECUTE(P)=ERQ-Q_4213
4 [出错代码4220]CAN'T EXECUTE(I)=ERQ-Q_4220
4 [出错代码4221]CAN'T EXECUTE(I)=ERQ-Q_4221
4 [出错代码4223]CAN'T EXECUTE(I)=ERQ-Q_4223
4 [出错代码4225]CAN'T EXECUTE(I)=ERQ-Q_4225
4 [出错代码4230]INST. FORMAT ERR.=ERQ-Q_4230
4 [出错代码4231]INST. FORMAT ERR.=ERQ-Q_4231
4 [出错代码4235]INST. FORMAT ERR.=ERQ-Q_4235
4 [出错代码4350]MULTI-COM. ERROR=ERQ-Q_4350
4 [出错代码4351]MULTI-COM. ERROR=ERQ-Q_4351
4 [出错代码4352]MULTI-COM. ERROR=ERQ-Q_4352
4 [出错代码4353]MULTI-COM. ERROR=ERQ-Q_4353
4 [出错代码4354]MULTI-COM. ERROR=ERQ-Q_4354
4 [出错代码4355]MULTI-COM. ERROR=ERQ-Q_4355
3 [出错代码4400-〉4432]
4 [出错代码4400]SFCP. CODE ERROR=ERQ-Q_4400
4 [出错代码4410]CAN'T SET(BL)=ERQ-Q_4410
4 [出错代码4411]CAN'T SET(BL)=ERQ-Q_4411
4 [出错代码4420]CAN'T SET(S)=ERQ-Q_4420
4 [出错代码4421]CAN'T SET(S)=ERQ-Q_4421
4 [出错代码4422]CAN'T SET(S)=ERQ-Q_4422
4 [出错代码4423]CAN'T SET(S)=ERQ-Q_4423
4 [出错代码4430]SFC EXE. ERROR=ERQ-Q_4430
4 [出错代码4431]SFC EXE. ERROR=ERQ-Q_4431
4 [出错代码4432]SFC EXE. ERROR=ERQ-Q_4432
3 [出错代码4500-〉4506]
4 [出错代码4500]SFCP. FORMAT ERR.=ERQ-Q_4500
4 [出错代码4501]SFCP. FORMAT ERR.=ERQ-Q_4501
4 [出错代码4502]SFCP. FORMAT ERR.=ERQ-Q_4502
4 [出错代码4503]SFCP. FORMAT ERR.=ERQ-Q_4503
4 [出错代码4504]SFCP. FORMAT ERR.=ERQ-Q_4504
4 [出错代码4505]SFCP. FORMAT ERR.=ERQ-Q_4505
4 [出错代码4506]SFCP. FORMAT ERR.=ERQ-Q_4506
3 [出错代码4600-〉4633]
4 [出错代码4600]SFCP. OPE. ERROR=ERQ-Q_4600
4 [出错代码4601]SFCP. OPE. ERROR=ERQ-Q_4601
4 [出错代码4602]SFCP. OPE. ERROR=ERQ-Q_4602
4 [出错代码4610]SFCP. EXE. ERROR=ERQ-Q_4610
4 [出错代码4611]SFCP. EXE. ERROR=ERQ-Q_4611
4 [出错代码4620]BLOCK EXE. ERROR=ERQ-Q_4620
4 [出错代码4621]BLOCK EXE. ERROR=ERQ-Q_4621
4 [出错代码4630]STEP EXE. ERROR=ERQ-Q_4630
4 [出错代码4631]STEP EXE. ERROR=ERQ-Q_4631
4 [出错代码4632]STEP EXE. ERROR=ERQ-Q_4632
4 [出错代码4633]STEP EXE. ERROR=ERQ-Q_4633
3 [出错代码5000-〉5011]
4 [出错代码5000]WDT ERROR=ERQ-Q_5000
4 [出错代码5001]WDT ERROR=ERQ-Q_5001
4 [出错代码5010]PRG. TIME OVER=ERQ-Q_5010
4 [出错代码5011]PRG. TIME OVER=ERQ-Q_5011
3 [出错代码6000-〉6501]
4 [出错代码6000]FILE DIFF.=ERQ-Q_6000
4 [出错代码6001]FILE DIFF.=ERQ-Q_6001
4 [出错代码6010]OPE. MODE DIFF.=ERQ-Q_6010
4 [出错代码6020]OPE. MODE DIFF.=ERQ-Q_6020
4 [出错代码6030]UNIT LAY. DIFF.=ERQ-Q_6030
4 [出错代码6035]UNIT LAY. DIFF.=ERQ-Q_6035
4 [出错代码6036]UNIT LAY. DIFF.=ERQ-Q_6036
4 [出错代码6040]CARD TYPE DIFF.=ERQ-Q_6040
4 [出错代码6041]CARD TYPE DIFF.=ERQ-Q_6041
4 [出错代码6050]CAN'T EXE. MODE=ERQ-Q_6050
4 [出错代码6060]CPU MODE DIFF.=ERQ-Q_6060
4 [出错代码6061]CPU MODE DIFF.=ERQ-Q_6061
4 [出错代码6062]CPU MODE DIFF.=ERQ-Q_6062
4 [出错代码6100]TRK. TRANS. ERR.=ERQ-Q_6100
4 [出错代码6101]TRK. TRANS. ERR.=ERQ-Q_6101
4 [出错代码6102]TRK. TRANS. ERR.=ERQ-Q_6102
4 [出错代码6103]TRK. TRANS. ERR.=ERQ-Q_6103
4 [出错代码6105]TRK. TRANS. ERR.=ERQ-Q_6105
4 [出错代码6106]TRK. TRANS. ERR.=ERQ-Q_6106
4 [出错代码6107]TRK. TRANS. ERR.=ERQ-Q_6107
4 [出错代码6108]TRK. TRANS. ERR.=ERQ-Q_6108
4 [出错代码6110]TRK. SIZE ERROR=ERQ-Q_6110
4 [出错代码6111]TRK. SIZE ERROR=ERQ-Q_6111
4 [出错代码6112]TRK. SIZE ERROR=ERQ-Q_6112
4 [出错代码6120]TRK. CABLE ERR.=ERQ-Q_6120
4 [出错代码6130]TRK. DISCONNECT=ERQ-Q_6130
4 [出错代码6140]TRK. INIT. ERROR=ERQ-Q_6140
4 [出错代码6200]CONTROL EXE.=ERQ-Q_6200
4 [出错代码6210]STANDBY=ERQ-Q_6210
4 [出错代码6220]CAN'T SWITCH=ERQ-Q_6220
4 [出错代码6300]STANDBY SYS. DOWN=ERQ-Q_6300
4 [出错代码6310]CONTROL SYS. DOWN=ERQ-Q_6310
4 [出错代码6311]CONTROL SYS. DOWN=ERQ-Q_6311
4 [出错代码6312]CONTROL SYS. DOWN=ERQ-Q_6312
4 [出错代码6313]CONTROL SYS. DOWN=ERQ-Q_6313
4 [出错代码6400]PRG. MEM.CLEAR=ERQ-Q_6400
4 [出错代码6410]MEM. COPY EXE.=ERQ-Q_6410
4 [出错代码6500]TRK. PARA. ERROR=ERQ-Q_6500
4 [出错代码6501]TRK. PARA. ERROR=ERQ-Q_6501
3 [出错代码7000-〉8031]
4 [出错代码7000]MULTI CPU DOWN=ERQ-Q_7000
4 [出错代码7002]MULTI CPU DOWN=ERQ-Q_7002
4 [出错代码7003]MULTI CPU DOWN=ERQ-Q_7003
4 [出错代码7004]MULTI CPU DOWN=ERQ-Q_7004
4 [出错代码7010]MULTI EXE.ERROR=ERQ-Q_7010
4 [出错代码7011]MULTI EXE.ERROR=ERQ-Q_7011
4 [出错代码7013]MULTI EXE.ERROR=ERQ-Q_7013
4 [出错代码7020]MULTI CPU ERROR=ERQ-Q_7020
4 [出错代码7030]CPU LAY ERROR=ERQ-Q_7030
4 [出错代码7031]CPU LAY ERROR=ERQ-Q_7031
4 [出错代码7032]CPU LAY ERROR=ERQ-Q_7032
4 [出错代码7035]CPU LAY ERROR=ERQ-Q_7035
4 [出错代码7036]CPU RAY ERROR=ERQ-Q_7036
4 [出错代码8031]INCORRECT FILE=ERQ-Q_8031
3 [出错代码9000-〉9020]
4 [出错代码9000]F****=ERQ-Q_9000
4 [出错代码9010]<CHK>ERR***_***=ERQ-Q_9010
4 [出错代码9020]BOOT OK=ERQ-Q_9020
3 [出错代码10000]
4 [出错代码10000]CONT.UNIT ERROR=ERQ-Q_10000
1 FX系列CPU
2 [错误代码0000]
3 [错误代码0000]无错误=ERFX_0000
2 [错误代码1***]
3 [错误代码1***]I/O配置错误=ERFX_1000
2 [错误代码3801-〉3820]
3 [错误代码3801]串行口通讯错误2=ERFX_3801
3 [错误代码3802]串行口通讯错误2=ERFX_3802
3 [错误代码3803]串行口通讯错误2=ERFX_3803
3 [错误代码3804]串行口通讯错误2=ERFX_3804
3 [错误代码3805]串行口通讯错误2=ERFX_3805
3 [错误代码3806]串行口通讯错误2=ERFX_3806
3 [错误代码3807]串行口通讯错误2=ERFX_3807
3 [错误代码3808]串行口通讯错误2=ERFX_3808
3 [错误代码3812]串行口通讯错误2=ERFX_3812
3 [错误代码3813]串行口通讯错误2=ERFX_3813
3 [错误代码3814]串行口通讯错误2=ERFX_3814
3 [错误代码3820]串行口通讯错误2=ERFX_3820
2 [错误代码6101-〉6107]
3 [错误代码6101]PLC硬件错误=ERFX_6101
3 [错误代码6102]PLC硬件错误=ERFX_6102
3 [错误代码6103]PLC硬件错误=ERFX_6103
3 [错误代码6104]PLC硬件错误=ERFX_6104
3 [错误代码6105]PLC硬件错误=ERFX_6105
3 [错误代码6106]PLC硬件错误=ERFX_6106
3 [错误代码6107]PLC硬件错误=ERFX_6107
2 [错误代码6201-〉6205]
3 [错误代码6201]PLC/PP通讯错误=ERFX_6201
3 [错误代码6202]PLC/PP通讯错误=ERFX_6202
3 [错误代码6203]PLC/PP通讯错误=ERFX_6203
3 [错误代码6204]PLC/PP通讯错误=ERFX_6204
3 [错误代码6205]PLC/PP通讯错误=ERFX_6205
2 [错误代码6301-〉6320]
3 [错误代码6301]串行口通讯错误1=ERFX_6301
3 [错误代码6302]串行口通讯错误1=ERFX_6302
3 [错误代码6303]串行口通讯错误1=ERFX_6303
3 [错误代码6304]串行口通讯错误1=ERFX_6304
3 [错误代码6305]串行口通讯错误1=ERFX_6305
3 [错误代码6306]串行口通讯错误1=ERFX_6306
3 [错误代码6307]串行口通讯错误1=ERFX_6307
3 [错误代码6308]串行口通讯错误1=ERFX_6308
3 [错误代码6312]串行口通讯错误1=ERFX_6312
3 [错误代码6313]串行口通讯错误1=ERFX_6313
3 [错误代码6314]串行口通讯错误1=ERFX_6314
3 [错误代码6320]串行口通讯错误1=ERFX_6320
2 [错误代码6401-〉6409]
3 [错误代码6401]参数错误=ERFX_6401
3 [错误代码6402]参数错误=ERFX_6402
3 [错误代码6403]参数错误=ERFX_6403
3 [错误代码6404]参数错误=ERFX_6404
3 [错误代码6405]参数错误=ERFX_6405
3 [错误代码6409]参数错误=ERFX_6409
2 [错误代码6501-〉6512]
3 [错误代码6501]语法错误=ERFX_6501
3 [错误代码6502]语法错误=ERFX_6502
3 [错误代码6503]语法错误=ERFX_6503
3 [错误代码6504]语法错误=ERFX_6504
3 [错误代码6505]语法错误=ERFX_6505
3 [错误代码6506]语法错误=ERFX_6506
3 [错误代码6507]语法错误=ERFX_6507
3 [错误代码6508]语法错误=ERFX_6508
3 [错误代码6509]语法错误=ERFX_6509
3 [错误代码6510]语法错误=ERFX_6510
3 [错误代码6511]语法错误=ERFX_6511
3 [错误代码6512]语法错误=ERFX_6512
2 [错误代码6601-〉6632]
3 [错误代码6601]回路错误=ERFX_6601
3 [错误代码6602]回路错误=ERFX_6602
3 [错误代码6603]回路错误=ERFX_6603
3 [错误代码6604]回路错误=ERFX_6604
3 [错误代码6605]回路错误=ERFX_6605
3 [错误代码6606]回路错误=ERFX_6606
3 [错误代码6607]回路错误=ERFX_6607
3 [错误代码6608]回路错误=ERFX_6608
3 [错误代码6609]回路错误=ERFX_6609
3 [错误代码6610]回路错误=ERFX_6610
3 [错误代码6611]回路错误=ERFX_6611
3 [错误代码6612]回路错误=ERFX_6612
3 [错误代码6613]回路错误=ERFX_6613
3 [错误代码6614]回路错误=ERFX_6614
3 [错误代码6615]回路错误=ERFX_6615
3 [错误代码6616]回路错误=ERFX_6616
3 [错误代码6617]回路错误=ERFX_6617
3 [错误代码6618]回路错误=ERFX_6618
3 [错误代码6619]回路错误=ERFX_6619
3 [错误代码6620]回路错误=ERFX_6620
3 [错误代码6621]回路错误=ERFX_6621
3 [错误代码6622]回路错误=ERFX_6622
3 [错误代码6623]回路错误=ERFX_6623
3 [错误代码6624]回路错误=ERFX_6624
3 [错误代码6625]回路错误=ERFX_6625
3 [错误代码6626]回路错误=ERFX_6626
3 [错误代码6627]回路错误=ERFX_6627
3 [错误代码6628]回路错误=ERFX_6628
3 [错误代码6629]回路错误=ERFX_6629
3 [错误代码6630]回路错误=ERFX_6630
3 [错误代码6631]回路错误=ERFX_6631
3 [错误代码6632]回路错误=ERFX_6632
2 [错误代码6701-〉6773]
3 [错误代码6701]操作错误=ERFX_6701
3 [错误代码6702]操作错误=ERFX_6702
3 [错误代码6703]操作错误=ERFX_6703
3 [错误代码6704]操作错误=ERFX_6704
3 [错误代码6705]操作错误=ERFX_6705
3 [错误代码6706]操作错误=ERFX_6706
3 [错误代码6707]操作错误=ERFX_6707
3 [错误代码6708]操作错误=ERFX_6708
3 [错误代码6709]操作错误=ERFX_6709
3 [错误代码6710]操作错误=ERFX_6710
3 [错误代码6712]操作错误=ERFX_6712
3 [错误代码6730]操作错误=ERFX_6730
3 [错误代码6732]操作错误=ERFX_6732
3 [错误代码6733]操作错误=ERFX_6733
3 [错误代码6734]操作错误=ERFX_6734
3 [错误代码6735]操作错误=ERFX_6735
3 [错误代码6736]操作错误=ERFX_6736
3 [错误代码6740]操作错误=ERFX_6740
3 [错误代码6742]操作错误=ERFX_6742
3 [错误代码6743]操作错误=ERFX_6743
3 [错误代码6744]操作错误=ERFX_6744
3 [错误代码6745]操作错误=ERFX_6745
3 [错误代码6746]操作错误=ERFX_6746
3 [错误代码6747]操作错误=ERFX_6747
3 [错误代码6748]操作错误=ERFX_6748
3 [错误代码6749]操作错误=ERFX_6749
3 [错误代码6750]操作错误=ERFX_6750
3 [错误代码6751]操作错误=ERFX_6751
3 [错误代码6752]操作错误=ERFX_6752
3 [错误代码6753]操作错误=ERFX_6753
3 [错误代码6754]操作错误=ERFX_6754
3 [错误代码6755]操作错误=ERFX_6755
3 [错误代码6756]操作错误=ERFX_6756
3 [错误代码6757]操作错误=ERFX_6757
3 [错误代码6758]操作错误=ERFX_6758
3 [错误代码6759]操作错误=ERFX_6759
3 [错误代码6760]操作错误=ERFX_6760
3 [错误代码6762]操作错误=ERFX_6762
3 [错误代码6763]操作错误=ERFX_6763
3 [错误代码6764]操作错误=ERFX_6764
3 [错误代码6765]操作错误=ERFX_6765
3 [错误代码6770]操作错误=ERFX_6770
3 [错误代码6771]操作错误=ERFX_6771
3 [错误代码6772]操作错误=ERFX_6772
3 [错误代码6773]操作错误=ERFX_6773
1 QS系列CPU
2 [出错代码1000-〉1010]
3 [出错代码1000]MAIN CPU DOWN=ERQS_1000
3 [出错代码1001]MAIN CPU DOWN=ERQS_1001
3 [出错代码1002]MAIN CPU DOWN=ERQS_1002
3 [出错代码1003]MAIN CPU DOWN=ERQS_1003
3 [出错代码1004]MAIN CPU DOWN=ERQS_1004
3 [出错代码1006]MAIN CPU DOWN=ERQS_1006
3 [出错代码1009]MAIN CPU DOWN=ERQS_1009
3 [出错代码1010]MAIN CPU DOWN=ERQS_1010
2 [出错代码1030-〉1031]
3 [出错代码1030]MAIN CPU DOWN=ERQS_1030
3 [出错代码1031]MAIN CPU DOWN=ERQS_1031
2 [出错代码1131-〉1146]
3 [出错代码1131]RAM ERROR=ERQS_1131
3 [出错代码1132]RAM ERROR=ERQS_1132
3 [出错代码1133]RAM ERROR=ERQS_1133
3 [出错代码1136]RAM ERROR=ERQS_1136
3 [出错代码1137]RAM ERROR=ERQS_1137
3 [出错代码1141]RAM ERROR=ERQS_1141
3 [出错代码1142]RAM ERROR=ERQS_1142
3 [出错代码1143]RAM ERROR=ERQS_1143
3 [出错代码1146]RAM ERROR=ERQS_1146
2 [出错代码1210-〉1404]
3 [出错代码1210]OPERATION CIRCUIT ERROR=ERQS_1210
3 [出错代码1311]I/O INTERRUPT ERROR=ERQS_1311
3 [出错代码1401]INTELLIGENT FUNCTION MODULE DOWN=ERQS_1401
3 [出错代码1403]INTELLIGENT FUNCTION MODULE DOWN=ERQS_1403
3 [出错代码1404]INTELLIGENT FUNCTION MODULE DOWN=ERQS_1404
2 [出错代码1411-〉1415]
3 [出错代码1411]CONTROL-BUS ERROR=ERQS_1411
3 [出错代码1413]CONTROL-BUS ERROR=ERQS_1413
3 [出错代码1414]CONTROL-BUS ERROR=ERQS_1414
3 [出错代码1415]CONTROL-BUS ERROR=ERQS_1415
2 [出错代码1500]
3 [出错代码1500]AC/DC DOWN=ERQS_1500
2 [出错代码1600-〉1610]
3 [出错代码1600]BATTERY ERROR=ERQS_1600
3 [出错代码1610]EXCEED MAX FLASH ROM REWRIT.ERR.=ERQS_1610
2 [出错代码2000-〉2210]
3 [出错代码2000]MODULE VERIFY ERROR=ERQS_2000
3 [出错代码2100]MODULE LAYOUT ERROR=ERQS_2100
3 [出错代码2106]MODULE LAYOUT ERROR=ERQS_2106
3 [出错代码2107]MODULE LAYOUT ERROR=ERQS_2107
3 [出错代码2112]INTELLIGENT FUNCTION MODULE ERR.=ERQS_2112
3 [出错代码2124]MODULE LAYOUT ERROR=ERQS_2124
3 [出错代码2125]MODULE LAYOUT ERROR=ERQS_2125
3 [出错代码2200]MISSING PARAMETER=ERQS_2200
3 [出错代码2210]BOOT ERROR=ERQS_2210
2 [出错代码2500-〉2503]
3 [出错代码2500]CAN'T EXECUTE PROGRAM=ERQS_2500
3 [出错代码2501]CAN'T EXECUTE PROGRAM=ERQS_2501
3 [出错代码2502]CAN'T EXECUTE PROGRAM=ERQS_2502
3 [出错代码2503]CAN'T EXECUTE PROGRAM=ERQS_2503
2 [出错代码3000-〉3008]
3 [出错代码3000]PARAMETER ERROR=ERQS_3000
3 [出错代码3001]PARAMETER ERROR=ERQS_3001
3 [出错代码3003]PARAMETER ERROR=ERQS_3003
3 [出错代码3004]PARAMETER ERROR=ERQS_3004
3 [出错代码3008]PARAMETER ERROR=ERQS_3008
2 [出错代码3100-〉3401]
3 [出错代码3100]NETWORK PARAMETER ERROR=ERQS_3100
3 [出错代码3101]NETWORK PARAMETER ERROR=ERQS_3101
3 [出错代码3102]NETWORK PARAMETER ERROR=ERQS_3102
3 [出错代码3103]NETWORK PARAMETER ERROR=ERQS_3103
3 [出错代码3104]NETWORK PARAMETER ERROR=ERQS_3104
3 [出错代码3105]CC-LINK PARAMETER ERROR=ERQS_3105
3 [出错代码3106]CC-LINK PARAMETER ERROR=ERQS_3106
3 [出错代码3107]CC-LINK PARAMETER ERROR=ERQS_3107
3 [出错代码3400]REMOTE PASSWORD ERROR=ERQS_3400
3 [出错代码3401]REMOTE PASSWORD ERROR=ERQS_3401
2 [出错代码4000-〉5010]
3 [出错代码4000]INSTRUCTION CODE ERROR=ERQS_4000
3 [出错代码4002]INSTRUCTION CODE ERROR=ERQS_4002
3 [出错代码4003]INSTRUCTION CODE ERROR=ERQS_4003
3 [出错代码4004]INSTRUCTION CODE ERROR=ERQS_4004
3 [出错代码4010]MISSING END INSTRUCTION=ERQS_4010
3 [出错代码4100]OPERATION ERROR=ERQS_4100
3 [出错代码4101]OPERATION ERROR=ERQS_4101
3 [出错代码4102]OPERATION ERROR=ERQS_4102
3 [出错代码4700]PROGRAM ABORT EXECUTED=ERQS_4700
3 [出错代码5001]WDT ERROR=ERQS_5001
3 [出错代码5010]PROGRAM SCAN TIME OVER=ERQS_5010
2 [出错代码8000-〉8120]
3 [出错代码8000]INTERNAL REGISTER ERROR=ERQS_8000
3 [出错代码8010]INTERNAL BUS ERROR=ERQS_8010
3 [出错代码8020]CPU A & B CAN'T BE SYNCHRONIZED=ERQS_8020
3 [出错代码8021]CPU A & B CAN'T BE SYNCHRONIZED=ERQS_8021
3 [出错代码8031]INCORRECT FILE=ERQS_8031
3 [出错代码8032]INCORRECT FILE=ERQS_8032
3 [出错代码8050]SAFETY OUTPUT VERIFY ERROR=ERQS_8050
3 [出错代码8060]INCORRECT FIRMWARE=ERQS_8060
3 [出错代码8070]INTERNALCPU COMMUNICATION ERROR=ERQS_8070
3 [出错代码8071]INTERNALCPU COMMUNICATION ERROR=ERQS_8071
3 [出错代码8072]INTERNALCPU COMMUNICATION ERROR=ERQS_8072
3 [出错代码8073]INTERNALCPU COMMUNICATION ERROR=ERQS_8073
3 [出错代码8074]INTERNALCPU COMMUNICATION ERROR=ERQS_8074
3 [出错代码8080]POWER SUPPLY ERROR=ERQS_8080
3 [出错代码8090]VOLTAGE DIAGNOSIS ERROR=ERQS_8090
3 [出错代码8100]TEST MODE TIME EXCEEDED=ERQS_8100
3 [出错代码8120]WDT CLOCK CHECK ERROR=ERQS_8120
2 [出错代码8300-〉8334]
3 [出错代码8300]CC-LINK REMOTE DETECTION ERROR=ERQS_8300
3 [出错代码8310]CC-LINK PRODUCT INFO. MISMATCH=ERQS_8310
3 [出错代码8320]CC-LINK DATA RECEPTION TIMEOUT=ERQS_8320
3 [出错代码8321]CC-LINK DATA RECEPTION TIMEOUT=ERQS_8321
3 [出错代码8322]CC-LINK DATA RECEPTION TIMEOUT=ERQS_8322
3 [出错代码8330]CC-LINK RECEIVED DATA ERROR=ERQS_8330
3 [出错代码8331]CC-LINK RECEIVED DATA ERROR=ERQS_8331
3 [出错代码8332]CC-LINK RECEIVED DATA ERROR=ERQS_8332
3 [出错代码8333]CC-LINK RECEIVED DATA ERROR=ERQS_8333
3 [出错代码8334]CC-LINK RECEIVED DATA ERROR=ERQS_8334
2 [出错代码9000]
3 [出错代码9000]F****=ERQS_9000
