Only in /usr/local/share/snmp/rfc: .index
diff -ru /usr/local/share/snmp/rfc.orig/ADSL-LINE-MIB.txt /usr/local/share/snmp/rfc/ADSL-LINE-MIB.txt
--- /usr/local/share/snmp/rfc.orig/ADSL-LINE-MIB.txt	Sat Mar  3 17:27:00 2001
+++ /usr/local/share/snmp/rfc/ADSL-LINE-MIB.txt	Tue Jan 23 00:42:41 2001
@@ -3379,7 +3379,6 @@
                static profiles are implemented."
 
           OBJECT      adslAtucConfMinSnrMgn
-          MIN-ACCESS  read-wr
           MIN-ACCESS  read-write
           DESCRIPTION
               "Read-write access is applicable when
diff -ru /usr/local/share/snmp/rfc.orig/DLSW-MIB.txt /usr/local/share/snmp/rfc/DLSW-MIB.txt
--- /usr/local/share/snmp/rfc.orig/DLSW-MIB.txt	Sat Mar  3 17:18:28 2001
+++ /usr/local/share/snmp/rfc/DLSW-MIB.txt	Tue Jan 23 00:13:40 2001
@@ -7,7 +7,7 @@
 
         Counter32, Gauge32, TimeTicks,
         OBJECT-TYPE, MODULE-IDENTITY,
-        NOTIFICATION-TYPE                 FROM SNMPv2-SMI
+        NOTIFICATION-TYPE, mib-2          FROM SNMPv2-SMI
         MODULE-COMPLIANCE, OBJECT-GROUP,
         NOTIFICATION-GROUP                FROM SNMPv2-CONF
         ifIndex                           FROM IF-MIB
@@ -150,12 +150,12 @@
 
 -- The DLSw MIB module contains an object part and a conformance part.
 -- Object part is organized in the following groups:
--- (1) dlswNode      -- information about this DLSw
--- (2) dlswTConn     -- about adjacent DLSw partners
--- (3) dlswInterface -- about which interfaces DLSw is active on
--- (4) dlswDirectory -- about any directory of local/remote resources
--- (5) dlswCircuit   -- about established circuits.
--- (6) dlswSdlc      -- about SDLC data link switched devices
+-- (1) dlswNode      - information about this DLSw
+-- (2) dlswTConn     - about adjacent DLSw partners
+-- (3) dlswInterface - about which interfaces DLSw is active on
+-- (4) dlswDirectory - about any directory of local/remote resources
+-- (5) dlswCircuit   - about established circuits.
+-- (6) dlswSdlc      - about SDLC data link switched devices
 
 dlswNode        OBJECT IDENTIFIER ::= { dlswMIB 1 }
 dlswTConn       OBJECT IDENTIFIER ::= { dlswMIB 2 }
@@ -168,9 +168,9 @@
 -- THE NODE GROUP
 -- *******************************************************************
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- DLSw Node Identity
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswNodeVersion  OBJECT-TYPE
     SYNTAX     OCTET STRING (SIZE (2))
     MAX-ACCESS read-only
@@ -211,9 +211,9 @@
        "DLSW: Switch-to-Switch Protocol RFC 1795"
     ::= { dlswNode 3 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- DLSw Code Capability
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswNodeStdPacingSupport  OBJECT-TYPE
     SYNTAX     INTEGER  {
        none              (1),  -- does not support DLSw
@@ -238,9 +238,9 @@
         scheme but never varies its receive window size."
     ::= { dlswNode 4 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- DLSw Node Operational Objects
--- -------------------------------------------------------------------
+--====================================================================
 dlswNodeStatus  OBJECT-TYPE
     SYNTAX     INTEGER  {
         active        (1),
@@ -339,10 +339,10 @@
 -- TRANSPORT CONNECTION (aka: PARTNER DLSW)
 -- *******************************************************************
 
--- -------------------------------------------------------------------
+-- ===================================================================
 
 -- Transport Connection Statistics Objects
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswTConnStat    OBJECT IDENTIFIER ::= { dlswTConn 1 }
 
 dlswTConnStatActiveConnections  OBJECT-TYPE
@@ -375,9 +375,9 @@
         this means the transport connection failed unexpectedly."
     ::= { dlswTConnStat 3 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- Transport Connection Configuration Table
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswTConnConfigTable  OBJECT-TYPE
     SYNTAX     SEQUENCE OF DlswTConnConfigEntry
     MAX-ACCESS not-accessible
@@ -651,15 +651,15 @@
         row definition out of use."
     ::= { dlswTConnConfigEntry 13 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- Transport Connection Operation Table
--- -------------------------------------------------------------------
+-- ===================================================================
 -- (1) At most one transport connection can be connected between
 --     this DLSw and one of its DLSw partners at a given time.
 -- (2) Multiple transport types are supported.
 -- (3) Since the entries may be reused, dlswTConnOperEntryTime
 --     needs to be consulted for the possibility of counter reset.
--- -------------------------------------------------------------------
+-- ===================================================================
 
 dlswTConnOperTable  OBJECT-TYPE
     SYNTAX     SEQUENCE OF DlswTConnOperEntry
@@ -1254,14 +1254,14 @@
         connection, where `active' means not in `disconnected' state."
     ::= { dlswTConnOperEntry 36 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- Transport Connection Specific
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswTConnSpecific OBJECT IDENTIFIER ::= { dlswTConn 4 }
 dlswTConnTcp      OBJECT IDENTIFIER ::= { dlswTConnSpecific 1 }
 
 -- ...................................................................
--- TCP Transport Connection Specific -- Configuration
+-- TCP Transport Connection Specific - Configuration
 -- ...................................................................
 dlswTConnTcpConfigTable  OBJECT-TYPE
     SYNTAX     SEQUENCE OF DlswTConnTcpConfigEntry
@@ -1328,7 +1328,7 @@
     ::= { dlswTConnTcpConfigEntry 3 }
 
 -- ...................................................................
--- TCP Transport Connection Specific -- Operation
+-- TCP Transport Connection Specific - Operation
 -- ...................................................................
 dlswTConnTcpOperTable  OBJECT-TYPE
     SYNTAX     SEQUENCE OF DlswTConnTcpOperEntry
@@ -1472,9 +1472,9 @@
 -- transport address of the DLSw partner is cached.
 -- *******************************************************************
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- Directory Related Statistical Objects
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswDirStat     OBJECT IDENTIFIER ::= { dlswDirectory 1 }
 
 dlswDirMacEntries  OBJECT-TYPE
@@ -1556,9 +1556,9 @@
         create new rows."
     ::= { dlswDirStat 8 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- Directory Cache
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswDirCache     OBJECT IDENTIFIER ::= { dlswDirectory 2 }
 
 -- ...................................................................
@@ -1566,7 +1566,7 @@
 -- All Possible combinations of values of these objects.
 --
 --     EntryType   LocationType       Location        Status
---  -------------- ------------ ------------------ --------------
+--  ============== ============ ================== ==============
 --  userConfigured    local     ifEntry or 0.0     reachable, or
 --                                                 notReachable, or
 --                                                 unknown
@@ -1743,7 +1743,7 @@
 -- All Possible combinations of values of these objects.
 --
 --     EntryType   LocationType       Location        Status
---  -------------- ------------ ------------------ --------------
+--  ============== ============ ================== ==============
 --  userConfigured    local     ifEntry or 0.0     reachable, or
 --                                                 notReachable, or
 --                                                 unknown
@@ -1918,9 +1918,9 @@
         following the RowStatus textual convention."
     ::= { dlswDirNBEntry 9 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- Resource Locations
--- -------------------------------------------------------------------
+-- ===================================================================
 
 dlswDirLocate       OBJECT IDENTIFIER ::= { dlswDirectory 3 }
 
@@ -2056,9 +2056,9 @@
 -- station that receives the initiation.
 -- *******************************************************************
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- Statistics Related to Circuits
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswCircuitStat      OBJECT IDENTIFIER ::= { dlswCircuit 1 }
 
 dlswCircuitStatActives  OBJECT-TYPE
@@ -2079,7 +2079,7 @@
         or reactivated upon exiting `disconnected' state."
     ::= { dlswCircuitStat 2 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- Circuit Table
 --
 -- This table is the DLSw entity's view of circuits.  There will be
@@ -2090,9 +2090,9 @@
 -- this Circuit Table:
 --
 --           number of       |    Origin End Station Location
---         entries in the    |--------------------------------------
+--         entries in the    |======================================
 --         Circuit Table     |  internal     local       remote
---    -----------------------|--------------------------------------
+--    =======================|======================================
 --     Target    |  internal |     NA          2           1
 --     End       |  local    |     2           2           1
 --     Station   |  remote   |     1           1           NA
@@ -2106,7 +2106,7 @@
 --
 -- Most of statistics related to circuits can be collected
 -- from LLC-2 Link Station Table.
--- -------------------------------------------------------------------
+-- ===================================================================
 dlswCircuitTable  OBJECT-TYPE
     SYNTAX     SEQUENCE OF DlswCircuitEntry
     MAX-ACCESS not-accessible
@@ -2814,7 +2814,7 @@
 -- *******************************************************************
 dlswTraps              OBJECT IDENTIFIER ::= { dlswMIB 0 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- This section defines the well-known notifications sent by
 -- DLSW agents.
 -- Care must be taken to insure that no particular notification
@@ -2827,7 +2827,7 @@
 -- (3) Transport connection up/down
 
 -- (4) Circuit up/down
--- -------------------------------------------------------------------
+-- ===================================================================
 --
 
 dlswTrapTConnPartnerReject NOTIFICATION-TYPE
@@ -2902,9 +2902,9 @@
 dlswCompliances        OBJECT IDENTIFIER ::= { dlswConformance 1 }
 dlswGroups             OBJECT IDENTIFIER ::= { dlswConformance 2 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- COMPLIANCE STATEMENTS
--- -------------------------------------------------------------------
+-- ===================================================================
 
 -- ...................................................................
 -- Core compliance for all DLSw entities
@@ -3245,9 +3245,9 @@
                "Write access is not required."
     ::= { dlswCompliances 5 }
 
--- -------------------------------------------------------------------
+-- ===================================================================
 -- CONFORMANCE GROUPS
--- -------------------------------------------------------------------
+-- ===================================================================
 
 -- ...................................................................
 -- Node Conformance Group
diff -ru /usr/local/share/snmp/rfc.orig/DSA-MIB.txt /usr/local/share/snmp/rfc/DSA-MIB.txt
--- /usr/local/share/snmp/rfc.orig/DSA-MIB.txt	Sat Mar  3 17:15:36 2001
+++ /usr/local/share/snmp/rfc/DSA-MIB.txt	Thu Feb 22 00:33:45 2001
@@ -10,7 +10,7 @@
           mib-2
                      FROM RFC1213-MIB
           applIndex, DistinguishedName
-                     FROM APPLICATION-MIB;
+                     FROM NETWORK-SERVICES-MIB;
 
         dsaMIB MODULE-IDENTITY
            LAST-UPDATED "9311250000Z"
diff -ru /usr/local/share/snmp/rfc.orig/FDDI-SMT73-MIB.txt /usr/local/share/snmp/rfc/FDDI-SMT73-MIB.txt
--- /usr/local/share/snmp/rfc.orig/FDDI-SMT73-MIB.txt	Sat Mar  3 17:15:09 2001
+++ /usr/local/share/snmp/rfc/FDDI-SMT73-MIB.txt	Tue Jan 23 00:11:46 2001
@@ -3,6 +3,8 @@
 IMPORTS
         Counter
             FROM RFC1155-SMI
+	transmission
+	    FROM RFC1213-MIB
         OBJECT-TYPE
             FROM RFC-1212;
 
diff -ru /usr/local/share/snmp/rfc.orig/HPR-MIB.txt /usr/local/share/snmp/rfc/HPR-MIB.txt
--- /usr/local/share/snmp/rfc.orig/HPR-MIB.txt	Sat Mar  3 17:19:54 2001
+++ /usr/local/share/snmp/rfc/HPR-MIB.txt	Tue Jan 23 00:25:54 2001
@@ -18,7 +18,7 @@
                 FROM APPN-MIB;
 
 hprMIB MODULE-IDENTITY
-        LAST-UPDATED  "970514000000Z"
+        LAST-UPDATED  "9705140000Z"
         ORGANIZATION  "AIW APPN / HPR MIB SIG"
         CONTACT-INFO
                 "
diff -ru /usr/local/share/snmp/rfc.orig/MIP-MIB.txt /usr/local/share/snmp/rfc/MIP-MIB.txt
--- /usr/local/share/snmp/rfc.orig/MIP-MIB.txt	Sat Mar  3 17:17:42 2001
+++ /usr/local/share/snmp/rfc/MIP-MIB.txt	Tue Jan 23 00:25:27 2001
@@ -1,7 +1,7 @@
     MIP-MIB DEFINITIONS ::= BEGIN
 
     IMPORTS
-        Counter32, Gauge32, Integer32, IpAddress, experimental,
+        Counter32, Gauge32, Integer32, IpAddress, mib-2,
         MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE
                                         FROM SNMPv2-SMI
         RowStatus, TruthValue, TimeStamp,
@@ -2117,7 +2117,7 @@
                 function within a home agent."
         ::= { mipGroups 12 }
 
-    mipSecNotifcationsGroup NOTIFICATION-GROUP
+    mipSecNotificationsGroup NOTIFICATION-GROUP
         NOTIFICATIONS { mipAuthFailure }
         STATUS      current
         DESCRIPTION
diff -ru /usr/local/share/snmp/rfc.orig/Modem-MIB.txt /usr/local/share/snmp/rfc/Modem-MIB.txt
--- /usr/local/share/snmp/rfc.orig/Modem-MIB.txt	Sat Mar  3 17:16:35 2001
+++ /usr/local/share/snmp/rfc/Modem-MIB.txt	Mon Jan 22 23:53:08 2001
@@ -23,7 +23,7 @@
              E-mail: waldbusser@cmu.edu"
     DESCRIPTION
             "The MIB module for management of dial-up modems."
-    ::= { mdmMIB 1 }
+    ::= { mdmMib 1 }
 
 mdmMib OBJECT IDENTIFIER ::= { mib-2 38 }
 
diff -ru /usr/local/share/snmp/rfc.orig/PPP-LCP-MIB.txt /usr/local/share/snmp/rfc/PPP-LCP-MIB.txt
--- /usr/local/share/snmp/rfc.orig/PPP-LCP-MIB.txt	Sat Mar  3 17:14:46 2001
+++ /usr/local/share/snmp/rfc/PPP-LCP-MIB.txt	Sat Mar  3 23:13:27 2001
@@ -182,7 +182,7 @@
      ::= { pppLinkStatusEntry 5 }
 
 pppLinkStatusLocalMRU   OBJECT-TYPE
-     SYNTAX    INTEGER(1..2147483648)
+     SYNTAX    INTEGER(1..2147483647)
      ACCESS    read-only
      STATUS    mandatory
      DESCRIPTION
@@ -195,7 +195,7 @@
      ::= { pppLinkStatusEntry 6 }
 
 pppLinkStatusRemoteMRU   OBJECT-TYPE
-     SYNTAX    INTEGER(1..2147483648)
+     SYNTAX    INTEGER(1..2147483647)
      ACCESS    read-only
      STATUS    mandatory
      DESCRIPTION
@@ -535,7 +535,7 @@
      ::= { pppLqrEntry 2 }
 
 pppLqrLocalPeriod   OBJECT-TYPE
-     SYNTAX    INTEGER(1..2147483648)
+     SYNTAX    INTEGER(1..2147483647)
      ACCESS    read-only
      STATUS    mandatory
      DESCRIPTION
@@ -548,7 +548,7 @@
      ::= { pppLqrEntry 3 }
 
 pppLqrRemotePeriod   OBJECT-TYPE
-     SYNTAX    INTEGER(1..2147483648)
+     SYNTAX    INTEGER(1..2147483647)
      ACCESS    read-only
      STATUS    mandatory
      DESCRIPTION
diff -ru /usr/local/share/snmp/rfc.orig/RDBMS-MIB.txt /usr/local/share/snmp/rfc/RDBMS-MIB.txt
--- /usr/local/share/snmp/rfc.orig/RDBMS-MIB.txt	Sat Mar  3 17:16:41 2001
+++ /usr/local/share/snmp/rfc/RDBMS-MIB.txt	Tue Jan 23 00:24:04 2001
@@ -6,8 +6,8 @@
         FROM SNMPv2-SMI
     DisplayString, DateAndTime, AutonomousType
         FROM SNMPv2-TC
-    applIndex, applGroup
-        FROM APPLICATION-MIB
+    applIndex, applGroups
+        FROM NETWORK-SERVICES-MIB
     mib-2
         FROM RFC1213-MIB;
 
@@ -1263,8 +1263,8 @@
          implement the RDBMS MIB"
     MODULE HOST-RESOURCES-MIB
         MANDATORY-GROUPS    { hrSystem }
-    MODULE APPLICATION-MIB
-        MANDATORY-GROUPS { applGroup }
+    MODULE NETWORK-SERVICES-MIB
+        MANDATORY-GROUPS { applGroups }
     MODULE RDBMS-MIB
         MANDATORY-GROUPS { rdbmsGroup }
 
Only in /usr/local/share/snmp/rfc: RFC-1215.txt
diff -ru /usr/local/share/snmp/rfc.orig/RFC1414-MIB.txt /usr/local/share/snmp/rfc/RFC1414-MIB.txt
--- /usr/local/share/snmp/rfc.orig/RFC1414-MIB.txt	Sat Mar  3 17:14:37 2001
+++ /usr/local/share/snmp/rfc/RFC1414-MIB.txt	Tue Feb 20 00:25:21 2001
@@ -3,6 +3,7 @@
 IMPORTS
     OBJECT-TYPE
         FROM RFC-1212
+    mib-2,
     tcpConnLocalAddress, tcpConnLocalPort,
     tcpConnRemAddress, tcpConnRemPort
             FROM RFC1213-MIB;
diff -ru /usr/local/share/snmp/rfc.orig/SNA-NAU-MIB.txt /usr/local/share/snmp/rfc/SNA-NAU-MIB.txt
--- /usr/local/share/snmp/rfc.orig/SNA-NAU-MIB.txt	Sat Mar  3 17:16:24 2001
+++ /usr/local/share/snmp/rfc/SNA-NAU-MIB.txt	Mon Jan 22 23:57:44 2001
@@ -17,7 +17,7 @@
         DisplayString, RowStatus, TimeStamp, InstancePointer
                 FROM SNMPv2-TC
 
-        Counter32, Gauge32, Integer32,
+        Counter32, Gauge32, Integer32, mib-2,
         OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE
                 FROM SNMPv2-SMI
 
diff -ru /usr/local/share/snmp/rfc.orig/TCPIPX-MIB.txt /usr/local/share/snmp/rfc/TCPIPX-MIB.txt
--- /usr/local/share/snmp/rfc.orig/TCPIPX-MIB.txt	Sat Mar  3 17:17:17 2001
+++ /usr/local/share/snmp/rfc/TCPIPX-MIB.txt	Sat Mar  3 16:51:11 2001
@@ -1,6 +1,8 @@
    TCPIPX-MIB DEFINITIONS ::= BEGIN
 
    IMPORTS
+	   enterprises
+		   FROM RFC1155-SMI
            OBJECT-TYPE
                    FROM RFC-1212;
 
@@ -10,7 +12,7 @@
 
 -- as hex digits, as in:  nnnnnnnn:mmmmmmmmmmmm
 
-IpxAddress ::= OCTET STRING (size (10))
+IpxAddress ::= OCTET STRING (SIZE (10))
 
    -- TCP/IPX MIB object idenfifiers
 
diff -ru /usr/local/share/snmp/rfc.orig/UPS-MIB.txt /usr/local/share/snmp/rfc/UPS-MIB.txt
--- /usr/local/share/snmp/rfc.orig/UPS-MIB.txt	Sat Mar  3 17:16:01 2001
+++ /usr/local/share/snmp/rfc/UPS-MIB.txt	Mon Jan 22 23:55:45 2001
@@ -2,7 +2,7 @@
 
 IMPORTS
     MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
-    OBJECT-IDENTITY, Counter32, Gauge32, Integer32
+    OBJECT-IDENTITY, Counter32, Gauge32, Integer32, mib-2
         FROM SNMPv2-SMI
     DisplayString, TimeStamp, TimeInterval, TestAndIncr,
       AutonomousType
diff -ru /usr/local/share/snmp/rfc.orig/SMUX-MIB.txt /usr/local/share/snmp/rfc/SMUX-MIB.txt
--- /usr/local/share/snmp/rfc.orig/SMUX-MIB.txt	2002-06-15 15:31:22.000000000 +0200
+++ /usr/local/share/snmp/rfc/SMUX-MIB.txt	2002-06-15 15:31:22.000000000 +0200
@@ -3,6 +3,8 @@
 IMPORTS
         enterprises
                 FROM RFC1155-SMI
+        DisplayString
+                FROM RFC1213-MIB
         OBJECT-TYPE
                 FROM RFC1212;
 
@@ -120,7 +122,7 @@
         ::= { smuxTreeEntry 1 }
 
 smuxTpriority OBJECT-TYPE
-        SYNTAX  INTEGER (0..'07fffffff'h)
+        SYNTAX  INTEGER (0..'7fffffff'h)
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
