Scalable Multicasting

广播分发

In scalable multicasting, there is no control channel between the player and server. For this reason, the number of clients that could potentially receive a scalable multicast event is unlimited. Use this type of multicasting when multicasting to a very large audience and your network is multicast enabled.

| 可扩展多播 |  | 帮助

加载点* |

频道 |

Set up authentication for a live channel.

编辑频道描述
启用频道
启用SAP
路径
端口范围
to
IP
to
可扩展多播的IP地址范围不能和后台多播的地址范围重叠,同时,必须在以下范围以内 224.0.0.0 到 239.255.255.255.
生存时间
(用于路由转发)
超时
(in seconds)
重新使用地址
转换为单播
交替的单播地址
将客户端状态发布到WEB服务器
WEB服务器名或者IP地址
WEB服务器端口
WEB服务器CGI 路径

*以上字段的更改将在服务器重新启动以后生效.