// $Xorg: xfree98,v 1.4 2001/02/09 02:05:52 xorgcvs Exp $
//
//Copyright 1996, 1998  The Open Group
//
//Permission to use, copy, modify, distribute, and sell this software and its
//documentation for any purpose is hereby granted without fee, provided that
//the above copyright notice appear in all copies and that both that
//copyright notice and this permission notice appear in supporting
//documentation.
//
//The above copyright notice and this permission notice shall be
//included in all copies or substantial portions of the Software.
//
//THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
//EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
//MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
//IN NO EVENT SHALL THE OPEN GROUP BE LIABLE FOR ANY CLAIM, DAMAGES OR
//OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,
//ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
//OTHER DEALINGS IN THE SOFTWARE.
//
//Except as contained in this notice, the name of The Open Group shall
//not be used in advertising or otherwise to promote the sale, use or
//other dealings in this Software without prior written authorization
//from The Open Group.
//
// $XFree86: xc/programs/xkbcomp/keycodes/xfree98,v 3.6 2001/01/17 23:45:51 dawes Exp $
//
default xkb_keycodes "pc98" {

    minimum= 8;
    maximum= 255;

    <ESC>  =   8;
    <AE01> =   9;
    <AE02> =  10;
    <AE03> =  11;
    <AE04> =  12;
    <AE05> =  13;
    <AE06> =  14;
    <AE07> =  15;
    <AE08> =  16;
    <AE09> =  17;
    <AE10> =  18;
    <AE11> =  19;
    <AE12> =  20;
    <BKSL> =  21;
    <BKSP> =  22;

    <TAB>  =  23;
    <AD01> =  24;
    <AD02> =  25;
    <AD03> =  26;
    <AD04> =  27;
    <AD05> =  28;
    <AD06> =  29;
    <AD07> =  30;
    <AD08> =  31;
    <AD09> =  32;
    <AD10> =  33;
    <AD11> =  34;
    <AD12> =  35;
    <RTRN> =  36;

    <LCTL> =  124;
    <CAPS> =  121;
    <AC01> =  37;
    <AC02> =  38;
    <AC03> =  39;
    <AC04> =  40;
    <AC05> =  41;
    <AC06> =  42;
    <AC07> =  43;
    <AC08> =  44;
    <AC09> =  45;
    <AC10> =  46;
    <AC11> =  47;
    <AC12> =  48;

    <LFSH> = 120;
    <AB01> =  49;
    <AB02> =  50;
    <AB03> =  51;
    <AB04> =  52;
    <AB05> =  53;
    <AB06> =  54;
    <AB07> =  55;
    <AB08> =  56;
    <AB09> =  57;
    <AB10> =  58;
    <AB11> =  59;

    <ALGR> = 122;
    <LALT> = 123;
    <NFER> =  89;
    <SPCE> =  60;
    <XFER> =  61;

    <BRK>  = 104;
    <PRSC> = 105;
    <FK01> = 106;
    <FK02> = 107;
    <FK03> = 108;
    <FK04> = 109;
    <FK05> = 110;
    <FK06> = 111;
    <FK07> = 112;
    <FK08> = 113;
    <FK09> = 114;
    <FK10> = 115;
    <FK11> =  90;
    <FK12> =  91;
    <FK13> =  92;
    <FK14> =  93;
    <FK15> =  94;


    <INS>  =  64;
    <DELE> =  65;
    <PGUP> =  63;
    <PGDN> =  62;
    <UP>   =  66;
    <LEFT> =  67;
    <RGHT> =  68;
    <DOWN> =  69;

    <HOME> =  70;
    <HELP> =  71;

    <KPSU> =  72;
    <KPDV> =  73;

    <KP7>  =  74;
    <KP8>  =  75;
    <KP9>  =  76;
    <KPMU> =  77;

    <KP4>  =  78;
    <KP5>  =  79;
    <KP6>  =  80;
    <KPAD> =  81;

    <KP1>  =  82;
    <KP2>  =  83;
    <KP3>  =  84;
    <KPEQ> =  85;

    <KP0>  =  86;
    <KPSP> =  87;
    <KPDC> =  88;

    indicator 1 = "Caps Lock";
    indicator 2 = "Kana";
};

